# Menu 12 Single Line Descriptions − User Functions 2 and Brake Control

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
12.001 | Threshold Detector 1 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
12.002 | Threshold Detector 2 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
12.003 | Threshold Detector 1 Source | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.004 | Threshold Detector 1 Level | 0.00 to 100.00 % | 0.00 % | RW | Num |  |  |  | US
12.005 | Threshold Detector 1 Hysteresis | 0.00 to 25.00 % | 0.00 % | RW | Num |  |  |  | US
12.006 | Threshold Detector 1 Output Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
12.007 | Threshold Detector 1 Destination | 0.000 to 30.999 | 0.000 | RW | Num | DE |  | PT | US
12.008 | Variable Selector 1 Source 1 | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.009 | Variable Selector 1 Source 2 | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.010 | Variable Selector 1 Mode | 0 (0), 1 (1), 2 (2), 3 (3), 4 (4), 5 (5), 6 (6), 7 (7), 8 (8), 9 (9) | 0 (0) | RW | Txt |  |  |  | US
12.011 | Variable Selector 1 Destination | 0.000 to 30.999 | 0.000 | RW | Num | DE |  | PT | US
12.012 | Variable Selector 1 Output | ±100.00 % |  | RO | Num | ND | NC | PT |
12.013 | Variable Selector 1 Source 1 Scaling | ±4.000 | 1.000 | RW | Num |  |  |  | US
12.014 | Variable Selector 1 Source 2 Scaling | ±4.000 | 1.000 | RW | Num |  |  |  | US
12.015 | Variable Selector 1 Control | 0.00 to 100.00 | 0.00 | RW | Num |  |  |  | US
12.016 | Variable Selector 1 Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
12.023 | Threshold Detector 2 Source | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.024 | Threshold Detector 2 Level | 0.00 to 100.00 % | 0.00 % | RW | Num |  |  |  | US
12.025 | Threshold Detector 2 Hysteresis | 0.00 to 25.00 % | 0.00 % | RW | Num |  |  |  | US
12.026 | Threshold Detector 2 Output Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
12.027 | Threshold Detector 2 Destination | 0.000 to 30.999 | 0.000 | RW | Num | DE |  | PT | US
12.028 | Variable Selector 2 Source 1 | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.029 | Variable Selector 2 Source 2 | 0.000 to 30.999 | 0.000 | RW | Num |  |  | PT | US
12.030 | Variable Selector 2 Mode | 0 (0), 1 (1), 2 (2), 3 (3), 4 (4), 5 (5), 6 (6), 7 (7), 8 (8), 9 (9) | 0 (0) | RW | Txt |  |  |  | US
12.031 | Variable Selector 2 Destination | 0.000 to 30.999 | 0.000 | RW | Num | DE |  | PT | US
12.032 | Variable Selector 2 Output | ±100.00 % |  | RO | Num | ND | NC | PT |
12.033 | Variable Selector 2 Source 1 Scaling | ±4.000 | 1.000 | RW | Num |  |  |  | US
12.034 | Variable Selector 2 Source 2 Scaling | ±4.000 | 1.000 | RW | Num |  |  |  | US
12.035 | Variable Selector 2 Control | 0.00 to 100.00 | 0.00 | RW | Num |  |  |  | US
12.036 | Variable Selector 2 Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
12.040 | BC Brake Release | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
12.041 | BC Enable | Dis (0), Relay (1), dig IO (2), USEr (3) | Dis (0) | RW | Txt |  |  |  | US
12.042 | BC Upper Current Threshold | 0 to 200 % | 50 % | RW | Num |  |  |  | US
12.043 | BC Lower Current Threshold | 0 to 200 % | 10 % | RW | Num |  |  |  | US
12.044 | BC Brake Release Frequency | 0.00 to 20.00 Hz | 1.00 Hz | RW | Num |  |  |  | US
12.045 | BC Brake Apply Frequency | 0.00 to 20.00 Hz | 2.00 Hz | RW | Num |  |  |  | US
12.046 | BC Brake Delay | 0.0 to 25.0 s | 1.0 s | RW | Num |  |  |  | US
12.047 | BC Post‑brake Release Delay | 0.0 to 25.0 s | 1.0 s | RW | Num |  |  |  | US
12.050 | BC Initial Direction | reF (0), For (1), Rev (2) | reF (0) | RW | Txt |  |  |  | US
12.051 | BC Brake Apply Through Zero Threshold | 0.00 to 20.00 Hz | 1.00 Hz | RW | Num |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |