# Menu 7 − Analog I/O

Mode: Open‑Loop

Thermistor Input

Drive thermal monitoring

Parameter | 07.001 Analogue Input 1
--- | ---
Short description | Displays the value of analog input 1
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms
Display Format | Standard | Decimal Places | 2
Coding | RO, FI, ND, NC, PT

The Analog input 1 can operate in different modes as defined by Analogue Input 1 Mode (07.007) including current modes. See Analog I/O.

Voltage mode: Resolution of 11 bits. It is a single ended unipolar voltage input 0V-10V

Current mode: Resolution of 11 bits. It is a single ended unipolar 0-20mA

The "Input Level" is defined for the different modes in the table below.

Mode | Input Level
Voltage | (Input Voltage/ 10V) x 100.00%
0-20mA | (Input Current / 20mA) x 100.00%
20-0mA | (20mA - Input Current) / 20mA x 100.00%
4-20mA | (Input Current - 4mA) / 16mA x 100.00%
20-4mA | (20mA - Input Current) / 16mA x 100.00%

Parameter | 07.002 Analogue Input 2
--- | ---
Short description | Displays the value of analog input 2
Mode | Open‑Loop
Minimum | 0.00 | Maximum | 100.00
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms
Display Format | Standard | Decimal Places | 2
Coding | RO, FI, ND, NC, PT

See Analog I/O.

Voltage mode: This input is a unipolar voltage 0-10V.

Digital mode: This input can also be configured as a digital input in which case this parameter will indicate 0.00% or 100.00% depending on the state of the input.

The "Input Level" is defined for the different modes in the table below.

Mode | Input Level
Voltage | (Input Voltage/ 10V) x 100.00%
Digital | 0.00% (corresponds to logical 0 if less than 9V) or 100.0% (corresponds to logical 1 if more than 11V)

Parameter | 07.004 Stack Temperature
--- | ---
Short description | Displays the temperature currently being measured on the heat sink
Mode | Open‑Loop
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

This parameter displays the temperature currently being measured on the heat sink. This is used as part of the drive thermal model, see Drive Over-temperature Alarm (10.018) for further details.

Parameter | 07.005 Auxiliary Temperature
--- | ---
Short description | Displays the temperature currently being measured on the power system
Mode | Open‑Loop
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

This parameter displays the temperature currently being measured on the power system on large frame. This is used as part of the drive thermal model.

Parameter | 07.007 Analogue Input 1 Mode
--- | ---
Short description | Defines the mode of analog input 1
Mode | Open‑Loop
Minimum | -6 | Maximum | 6
Default | 6 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
‑6 | 4-20.S
‑5 | 20-4.S
‑4 | 4-20.L
‑3 | 20-4.L
‑2 | 4-20.H
‑1 | 20-4.H
0 | 0-20
1 | 20-0
2 | 4-20.tr
3 | 20-4.tr
4 | 4-20
5 | 20-4
6 | Volt

See Analogue Input 1 (07.001).

The table below gives all the possible analogue input modes.

Value | Mode | Function
-6 | 4-20mA Stop | Stop on loss
-5 | 20-4mA Stop | Stop on loss
-4 | 4-20mA Low | 4-20mA switching to equivalent of 4mA input current on loss(1). See Analog Input 1 Preset on Current Loss (07.026).
-3 | 20-4mA Low | 20-4mA switching to equivalent of 4mA input current on loss(1). See Analog Input 1 Preset on Current Loss (07.026)
-2 | 4-20mA Hold | 4-20mA hold at level before loss on current loss (2)
-1 | 20-4mA Hold | 20-4mA hold at level before loss on current loss (2)
0 | 0-20mA | 0-20mA
1 | 20-0mA | 20-0mA
2 | 4-20mA Trip | 4-20mA trip on current loss (1), (3)
3 | 20-4mA Trip | 20-4mA trip on current loss (1), (3)
4 | 4-20mA | 4-20mA no action on loss (1)
5 | 20-4mA | 20-4mA no action on loss (1)
6 | Voltage | Voltage

(1) Analogue input level is 0.00% if the current is below 3mA.

(2) Analogue input level remains at the value it had in the previous sample before the current fell below 3mA.

(3) A An Input 1 Loss is initiated if the current falls below 3mA.

Parameter | 07.008 Analogue Input 1 Scaling
--- | ---
Short description | Defines the scaling factor of analog input 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See Analog I/O.

Analogue Input 1 (07.001) is modified by Analogue Input 1 Scaling (07.008), Analogue Input 1 Offset (07.030) and Analogue Input 1 Invert (07.009) before it is routed to its destination as follows:

A1O = Analogue Input 1 (07.001) + Analogue Input 1 Offset (07.030)
A1O is the value after the offset has been applied and is limited between -100.00% and 100.00%

A1S = A1O x Analogue Input 1 Scaling (07.008)
A1S is the value after the scaling and the offset have been applied and is limited between -100.00% and 100.00%

If Analogue Input 1 Invert (07.009) = 0 then A1I = A1S otherwise A1I = -A1S

A1I is the value after the invert, scaling and offset have been applied and is the final value that is routed to the destination defined by

- Analogue Input 1 Destination A (07.010) if Analogue Input 1 Control (07.051) = 0
- Analogue Input 1 Destination B (07.090) if Analogue Input 1 Control (07.051) > 0

Parameter | 07.009 Analogue Input 1 Invert
--- | ---
Short description | Inverts the signal for analog input 1
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Analogue Input 1 Scaling (07.008).

Parameter | 07.010 Analogue Input 1 Destination A
--- | ---
Short description | Defines the output parameter for analog input 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 1.036 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

See Analogue Input 1 Scaling (07.008).

Parameter | 07.011 Analogue Input 2 Mode
--- | ---
Short description | Defines the mode for analog input 2
Mode | Open‑Loop
Minimum | 6 | Maximum | 7
Default | 6 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
6 | Volt
7 | dig

See Analogue Input 2 (07.002).

The table below gives all the possible analogue input modes.

Value | Mode | Function
6 | Voltage | Voltage
7 | Digital | Digital

Parameter | 07.012 Analogue Input 2 Scaling
--- | ---
Short description | Defines the scaling factor for analog input 2
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See Analog I/O.

Analogue Input 2 (07.002) is modified by Analogue Input 2 Scaling (07.012), Analogue Input 2 Offset (07.031) and Analogue Input 2 Invert (07.013) before it is routed to its destination as follows:

A2O = Analogue Input 2 (07.002)+ Analogue Input 2 Offset (07.031)
A2O is the value after the offset has been applied and is limited between 0.00% and 100.00%

A2S = A2O x Analogue Input 2 Scaling (07.012)
A2S is the value after the scaling and the offset have been applied and is limited between 0.00% and 100.00%

If Analogue Input 2 Invert (07.013) = 0 then A2I = A2S otherwise A2I = -A2S

A2I is the value after the invert, scaling and offset have been applied and is the final value that is routed to the destination defined by

- Analogue Input 2 Destination A (07.014) if Analogue Input 2 Control (07.052) = 0
- Analogue Input 2 Destination B (07.094) if Analogue Input 2 Control (07.052) > 0

Parameter | 07.013 Analogue Input 2 Invert
--- | ---
Short description | Inverts the signal for analog input 2
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Analogue Input 2 Scaling (07.012).

Parameter | 07.014 Analogue Input 2 Destination A
--- | ---
Short description | Defines the output parameter for analog input 2
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 1.037 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

See Analogue Input 2 Scaling (07.012).

Parameter | 07.019 Analogue Output 1 Source A
--- | ---
Short description | Defines the input parameter for analog output 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 2.001 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT

Analogue Output 1 Source A (07.019) defines the source parameter for Analogue Output 1. The value is then scaled with Analogue Output 1 Scaling (07.020) and if the scaling is greater than 1.000 the value is clamped between -100.0% and +100.0% which corresponds to:

M200, M201, M300:

- In voltage mode: 0V to +10V

M400:

- In voltage mode: 0V to +10V
- In current mode: 4-20mA or 0-20mA depending on the mode selected
- In digital mode: 0V to +24V. Scaling parameter has no effect.

- If source is a bit parameter then "Off" gives 0V and "On" gives +24V
- If source is not a bit parameter then source parameter must be more than half its positive range to be +24V.

Parameter | 07.020 Analogue Output 1 Scaling
--- | ---
Short description | Defines the scaling factor for analog output 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 40.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW, BU

See Analogue Output 1 Source A (07.019).

Parameter | 07.026 Analog Input 1 Preset on Current Loss
--- | ---
Short description | Defines the current level held on analogue input 1 current loss
Mode | Open‑Loop
Minimum | 4.00 | Maximum | 20.00
Default | 4.00 | Units | mA
Type | 16 Bit User Save | Update Rate | 4ms read
Display Format | Standard | Decimal Places | 2
Coding | RW

If Analogue Input 1 Mode (07.007) is set to any of the 4-20mA Low or 20-4mA Low modes and the current falls below 3mA (Analogue Input 1 Current Loop Loss (07.028) = 1) then the analogue input 1 is held to Analog Input 1 Preset on Current Loss (07.026).

If the current rise above 4mA (Analogue Input 1 Current Loop Loss (07.028) = 0) then the analogue input 1 current is used as normal.

Parameter | 07.028 Analogue Input 1 Current Loop Loss
--- | ---
Short description | Displays when analog input 1 falls below 3mA
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Analog Input 1 Preset on Current Loss (07.026).

Parameter | 07.030 Analogue Input 1 Offset
--- | ---
Short description | Defines the offset of analog input 1
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 1 Scaling (07.008).

Parameter | 07.031 Analogue Input 2 Offset
--- | ---
Short description | Defines the offset of analog input 2
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 2 Scaling (07.012).

Parameter | 07.034 Inverter Temperature
--- | ---
Short description | Displays the estimated junction temperature of the hottest power device within the drive inverter
Mode | Open‑Loop
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Inverter Temperature (07.034) shows the estimated junction temperature of the hottest power device within the drive inverter. If this temperature exceeds the switch down threshold defined for the power stage the switching frequency is reduced provided this feature has not been disabled (i.e. Auto-switching Frequency Change Disable (05.035) = 0) or the minimum switching frequency has not been reached. The switching frequency can be reduced from 12kHz to 6kHz to 3kHz, or from 16kHz to 8kHz to 4kHz to 2kHz. If the switching frequency has been reduced the drive will attempt to restore it to the required level when the Inverter Temperature (07.034) reduces.

Parameter | 07.035 Percentage Of d.c. Link Thermal Trip Level
--- | ---
Short description | Displays the percentage of the maximum allowed temperature as estimated by the thermal model of the d.c. link components
Mode | Open‑Loop
Minimum | 0 | Maximum | 100
Default |  | Units | %
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Percentage Of d.c. Link Thermal Trip Level (07.035) gives the percentage of the maximum allowed temperature as estimated by the thermal model of the d.c. link components.

Parameter | 07.036 Percentage Of Drive Thermal Trip Level
--- | ---
Short description | Displays the percentage of the thermal trip level of the temperature monitoring point or thermal model in the drive that is highest
Mode | Open‑Loop
Minimum | 0 | Maximum | 100
Default |  | Units | %
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Percentage Of Drive Thermal Trip Level (07.036) gives the percentage of the thermal trip level of the temperature monitoring point or thermal model in the drive that is highest. This includes all thermal monitoring points Stack Temperature (07.004), Auxiliary Temperature (07.005), Inverter Temperature (07.034) and Percentage Of d.c. Link Thermal Trip Level (07.035).

Percentage Of d.c. Link Thermal Trip Level (07.035) is used directly to give Percentage Of Drive Thermal Trip Level (07.036), but for all other monitored values which are temperatures this is given by

Percentage of thermal trip level = (Temperature - 40°C) / (Trip temperature - 40°C) x 100%

The location of the measurement or the thermal model that is related to this temperature is given in Temperature Nearest To Trip Level (07.037). If Percentage Of Drive Thermal Trip Level (07.036) exceeds 90% Drive Over-temperature Alarm (10.018) is set to one. If Percentage Of Drive Thermal Trip Level (07.036) reaches 100% one of the trips given in the table below is initiated. The trip can be reset when the percentage of thermal trip level fall below 95%.

Temperature | Trip
Inverter Temperature (07.034) | OHt Inverter
Auxiliary Temperature (07.005) | OHt Power
Percentage Of d.c. Link Thermal Trip Level (07.035) | OHt dc bus

Parameter | 07.037 Temperature Nearest To Trip Level
--- | ---
Short description | Displays the location or the model that corresponds to the value shown in Percentage Of Drive Thermal Trip Level
Mode | Open‑Loop
Minimum | 0 | Maximum | 29999
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Temperature Nearest To Trip Level (07.037) shows the location or the model that corresponds to the value shown in Percentage Of Drive Thermal Trip Level (07.036) in the form xxyzz as shown in the table below.

Source | xx | y | zz
Control system | 00 | 1 | 00: Inverter thermal model
Control system | 00 | 2 | 00: D.c. link thermal model
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power system
Power system (Large frame only) | 01 | 1 | zz: Thermistor location defined by zz in the rectifier

Parameter | 07.046 Thermistor Type
--- | ---
Short description | Defines the thermistor type when used
Mode | Open‑Loop
Minimum | 0 | Maximum | 4
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | D44081
1 | 84
2 | PT1000
3 | PT2000
4 | other

Thermistor Type (07.046) defines the operation of the temperature feedback interface for DI/O 05 when Digital input 5 mode (08.035) is 1, 2 or 3.

If Thermistor Type (07.046) = 0, the thermistor DIN44081 is designed to react like a temperature switch and therefore Thermistor Temperature (07.050) always reads 0.0°C.

If Thermistor Type (07.046) = 1 to 3 is selected, the digital input operation of the terminal is disabled.

If Thermistor Type (07.046) = 4, any thermistor can be used but Thermistor Temperature (07.050) always reads 0.0°C.

Parameter | 07.047 Thermistor Feedback
--- | ---
Short description | Displays the measured resistance of the thermistor when used
Mode | Open‑Loop
Minimum | 0 | Maximum | 4000
Default |  | Units | Ω
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, FI, ND, NC, PT

Thermistor Feedback (07.047) shows the measured resistance. If Digital input 5 mode (08.035) is 2 then {Th} trip is initiated if the feedback value is higher than Thermistor Trip Threshold (07.048). The trip cannot be reset unless the feedback is below Thermistor Reset Threshold (07.049). The default values for Thermistor Trip Threshold (07.048) and Thermistor Reset Threshold (07.049) are the levels specified in the DIN 44082 standard.

Parameter | 07.048 Thermistor Trip Threshold
--- | ---
Short description | Defines the thermistor trip threshold when used
Mode | Open‑Loop
Minimum | 0 | Maximum | 4000
Default | 3300 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Thermistor Feedback (07.047).

Parameter | 07.049 Thermistor Reset Threshold
--- | ---
Short description | Defines the thermistor reset threshold when used
Mode | Open‑Loop
Minimum | 0 | Maximum | 4000
Default | 1800 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Thermistor Feedback (07.047).

Parameter | 07.050 Thermistor Temperature
--- | ---
Short description | Displays the temperature of the device based on the resistance to temperature characteristic for the specified device
Mode | Open‑Loop
Minimum | -50 | Maximum | 300
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, FI, ND, NC, PT

If a KTY84, PT1000 or PT2000 type device is selected for temperature feedback (i.e. Thermistor Type (07.046) = 1 to 3) then Thermistor Temperature (07.050) shows the temperature of the device based on the resistance to temperature characteristic specified for this device. Otherwise Thermistor Temperature (07.050) = 0.0.

Parameter | 07.051 Analogue Input 1 Control
--- | ---
Short description | Defines the functionality of analog input 1
Mode | Open‑Loop
Minimum | 0 | Maximum | 5
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Actioned on exit of edit mode and on drive reset
Display Format | Standard | Decimal Places | 0
Coding | RW

Value | Description | Analogue Input 1 Destination B (07.090)
0 | User defined by Analogue Input 1 Destination A (07.010) | 00.000
1 | Frequency reference 1 | 01.036
2 | Frequency reference 2 | 01.037
3 | Maximum reference clamp | 01.006
4 | Current limit | 04.007
5 | Torque reference | 04.008

This offers a simple control of parameter to change the analogue input 1 functionality.

If Analogue Input 1 Control (07.051) is more than 0 then the destination is defined by Analogue Input 1 Destination B (07.090). The destination Analogue Input 1 Destination B (07.090) is written by Analogue Input 1 Control (07.051) selection. (i.e. If Analogue Input 1 Control (07.051) = 3 then Analogue Input 1 Destination B (07.090) = 01.006)

If Analogue Input 1 Control (07.051) is 0 then then the destination is defined by Analogue Input 1 Destination A (07.010).

Parameter | 07.052 Analogue Input 2 Control
--- | ---
Short description | Defines the functionality of analog input 2
Mode | Open‑Loop
Minimum | 0 | Maximum | 5
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Actioned on exit of edit mode and on drive reset
Display Format | Standard | Decimal Places | 0
Coding | RW

Value | Description | Analogue Input 2 Destination B (07.094)
0 | User defined by Analogue Input 2 Destination A (07.014) | 00.000
1 | Frequency reference 1 | 01.036
2 | Frequency reference 2 | 01.037
3 | Maximum reference clamp | 01.006
4 | Current limit | 04.007
5 | Torque reference | 04.008

This offers a simple control of parameter to change the analogue input 2 functionality.

If Analogue Input 2 Control (07.052) is more than 0 then the destination is defined by Analogue Input 2 Destination B (07.094). The destination Analogue Input 2 Destination B (07.094) is written by Analogue Input 2 Control (07.052) selection. (i.e. If Analogue Input 2 Control (07.052)= 3 then Analogue Input 2 Destination B (07.094) = 01.006)

If Analogue Input 2 Control (07.052) is 0 then then the destination is defined by Analogue Input 2 Destination A (07.014).

Parameter | 07.055 Analogue Output 1 Control
--- | ---
Short description | Defines the functionality of analog output 1
Mode | Open‑Loop
Minimum | 0 | Maximum | 15
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Actioned on exit of edit mode and on drive reset
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

Value | Description | Analogue Output 1 Source B (07.099)
0 | User defined by Analogue Output 1 Source A (07.019) | 00.000
1 | Frequency output | 02.001
2 | Frequency reference | 01.003
3 | Motor speed | 05.004
4 | Current output vs drive | 04.001
5 | Current output vs motor | TBD: 0 ~ double motor rated current
6 | Torque output | 04.020
7 | Torque current output | 04.002
8 | Voltage output | 05.002
9 | DC bus voltage (0~800V) | 05.005
10 | Analogue Input 1 | 07.001
11 | Analogue Input 2 | 07.002
12 | Power output (0~2*Pe) | 05.003
13 | Torque limitation | 04.018
14 | Torque reference (0~300%Tem) | 04.008
15 | External function of host (0~4095) | TBD (from comms)

This offers a simple control of parameter Analogue Output 1 Source B (07.099) to change the analogue output 1 source.

If Analogue Output 1 Control (07.055) is more than 0 then the source is defined by Analogue Output 1 Source B (07.099). The source Analogue Output 1 Source B (07.099) is written by Analogue Output 1 Control (07.055) selection. (i.e. If Analogue Output 1 Control (07.055) = 13 then Analogue Output 1 Source B (07.099) = 04.018)

If 07.055 is 0 then then the source is defined by 07.019.

Parameter | 07.061 Analogue Input 1 Minimum Reference
--- | ---
Short description | Defines the minimum reference for analog input 1
Mode | Open‑Loop
Minimum | 0.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

Analogue Input 1 (07.001) can be scaled and limited using the following parameters:

- Analogue Input 1 Minimum Reference (07.061)
- Analogue Input 1 At Minimum Reference (07.062)
- Analogue Input 1 Maximum Reference (07.063)
- Analogue Input 1 At Maximum Reference (07.064)

Parameters above can be selected to limit the range of Analogue Input 1 (07.001) and also scale it between the minimum and maximum reference.

If Analogue Input 1 Minimum Reference (07.061) ≥ Analogue Input 1 Maximum Reference (07.063) then Ai1 = 0.00%whatever the input level.

Input Level is limited between Analogue Input 1 At Minimum Reference (07.062) and Analogue Input 1 At Maximum Reference (07.064)

Analogue Input 1 (07.001) = [(Analogue Input 1 At Maximum Reference (07.064) - Analogue Input 1 At Minimum Reference (07.062)) / (Analogue Input 1 Maximum Reference (07.063) - Analogue Input 1 Minimum Reference (07.061))] x (Input level - Analogue Input 1 Minimum Reference (07.061)) + Analogue Input 1 At Minimum Reference (07.062).

Parameter | 07.062 Analogue Input 1 At Minimum Reference
--- | ---
Short description | Defines the value of analog input 1 at minimum reference
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 1 Minimum Reference (07.061).

Parameter | 07.063 Analogue Input 1 Maximum Reference
--- | ---
Short description | Defines the maximum reference for analog input 1
Mode | Open‑Loop
Minimum | 0.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 1 Minimum Reference (07.061).

Parameter | 07.064 Analogue Input 1 At Maximum Reference
--- | ---
Short description | Defines the value of analog input 1 at maximum reference
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 1 Minimum Reference (07.061).

Parameter | 07.065 Analogue Input 2 Minimum Reference
--- | ---
Short description | Defines the minimum reference for analog input 2
Mode | Open‑Loop
Minimum | 0.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See graph in Analogue Input 1 Minimum Reference (07.061).

Analogue Input 2 (07.002) can be scaled and limited using the following parameters:

- Analogue Input 2 Minimum Reference (07.065)
- Analogue Input 2 At Minimum Reference (07.066)
- Analogue Input 2 Maximum Reference (07.067)
- Analogue Input 2 At Maximum Reference (07.068)

Parameters above can be selected to limit the range of Analogue Input 2 (07.002) and also scale it between the minimum and maximum reference.

If Analogue Input 2 Minimum Reference (07.065) ≥ Analogue Input 2 Maximum Reference (07.067) then Ai2 = 0.00% whatever the input level.

Input Level is limited between Analogue Input 2 At Minimum Reference (07.066) and Analogue Input 2 At Maximum Reference (07.068)

Analogue Input 2 (07.002) = [(Analogue Input 2 At Maximum Reference (07.068) - Analogue Input 2 At Minimum Reference (07.066))/(Analogue Input 2 Maximum Reference (07.067) - Analogue Input 2 Minimum Reference (07.065))] x (Input level - Analogue Input 2 Minimum Reference (07.065))+ Analogue Input 2 At Minimum Reference (07.066).

Parameter | 07.066 Analogue Input 2 At Minimum Reference
--- | ---
Short description | Defines the value of analog input 2 at minimum reference
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 2 Minimum Reference (07.065).

Parameter | 07.067 Analogue Input 2 Maximum Reference
--- | ---
Short description | Defines the maximum reference for analog input 2
Mode | Open‑Loop
Minimum | 0.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 2 Minimum Reference (07.065).

Parameter | 07.068 Analogue Input 2 At Maximum Reference
--- | ---
Short description | Defines the value of analog input 2 at maximum reference
Mode | Open‑Loop
Minimum | -100.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analogue Input 2 Minimum Reference (07.065).

Parameter | 07.090 Analogue Input 1 Destination B
--- | ---
Short description | Defines the secondary destination for analog input 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See Analogue Input 1 Destination A (07.010).

Parameter | 07.094 Analogue Input 2 Destination B
--- | ---
Short description | Defines the secondary destination for analog input 2
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See Analogue Input 2 Destination A (07.014).

Parameter | 07.099 Analogue Output 1 Source B
--- | ---
Short description | Defines the secondary source for analog output 1
Mode | Open‑Loop
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RO, PT

See Analogue Output 1 Source A (07.019).