# Trips

Mode: Open‑Loop

Trip 0 (10.020) to Trip 9 (10.029) store the most recent 10 trips that have occurred where Trip Trip 0 (10.020) is the most recent and Trip 9 (10.029) is the oldest. When a new trip occurs it is written to Trip 0 (10.020) and all the other trips move down the log, with oldest being lost.

The date and time when each trip occurs are also stored in the date and time log, i.e. Trip 0 Date (10.041) to Trip 9 Time (10.060). The date and time are taken from Date (06.016) and Time (06.017) (See Date/Time Selector (06.019)). Some trips have sub-trip numbers which give more detail about the reason for the trip. If a trip has a sub-trip number its value is stored in the sub-trip log, i.e. Trip 0 Sub-trip Number (10.070) to Trip 9 Sub-trip Number (10.079). If the trip does not have a sub-trip number then zero is stored in the sub-trip log.

Trip categories and priorities
Trips are grouped into the categories given in the table below. A trip can only occur when the drive is not tripped, or if it is already tripped and the new trip has a higher priority than the active trip (i.e. lower priority number). Unless otherwise stated a trip cannot be reset until 1.0s after it has been initiated.

Priority | Category | Trips | Comments
1 | Internal faults | HF01 - HF19 | These are fatal problems that cannot be reset. All drive features are inactive after any of these trips occur. If a basic keypad is fitted it will show the trip, but the keypad will not function. These trips are not stored in the trip log.
1 | Stored HF trip | Stored HF | This trip cannot be cleared unless 1299 is entered into Parameter mm.000 (mm.000) and a reset is initiated.
2 | Non-resettable trips | Trip numbers 218 - 247 and Slot1 HF | These trips cannot be reset.
3 | Volatile memory failure | EEPROM Fail | This can only be reset if Parameter mm.000 (mm.000) is set to 1233 or 1244, or if Load Defaults (11.043) is set to a non-zero value
4 | Non-volatile media trips | Trip numbers 174, 175 and 177 - 188 | These trips are priority 5 during power-up
5 | Trips with extended reset times | OI ac, OI Brake and Reserved | These trips cannot be reset until 10s after the trip was initiated.
5 | Phase loss and d.c. link power circuit protection | Phase Loss and OHt dc bus | The drive will attempt to stop the motor before tripping if a Phase Loss.000 trip occurs unless this feature has been disabled (see Action On Trip Detection (10.037)). The drive will always attempt to stop the motor before tripping if an OHt dc bus occurs.
5 | Standard trips | All other trips |

Trips {HF01} to {HF19} are internal faults that do not have trip numbers. If one of these trips occurs, the main drive processor has detected an irrecoverable error. All drive functions are stopped and the trip message will be displayed on the drive keypad. The error can only be reset by powering the drive down and up again. The table below gives the reasons for internal faults and their corresponding trip

Trip | Reason
{HF01} | CPU hardware fault during exception processing
{HF02} | CPU memory management fault is an exception that occurs because of a memory protection related fault
{HF03} | CPU has detected a Bus Fault. A Bus Fault is an exception that occurs because of a memory related fault for an instruction or data memory transaction. This might be from an error detected on a bus in the memory system.
{HF04} | CPU has detected a usage fault: A Usage Fault is an exception that occurs because of a fault related to instruction execution. This includes: an undefined instruction an illegal unaligned access invalid state on instruction execution an error on exception return. The following can cause a Usage Fault when the core is configured to report them: an unaligned address on word and half word memory access division by zero.
{HF05} | Reserved
{HF06} | Reserved
{HF07} | Watchdog failure
{HF08} | CPU Interrupt crash. Interrupt crash level indicated by subtrip number.
{HF09} | Free store overflow
{HF10} | Reserved
{HF11} | The HF11 trip indicates that a non-volatile memory comms error has occurred.
Sub-trip | Reason | Recommended action
1 | Non-volatile memory comms error. | Hardware fault – contact the supplier of the drive.
2 | EEPROM size is incompatible with the user firmware. | After 1min the drive will go to its bootloader. Re-program drive with compatible user firmware using UniMConnect
{HF12} | Stack overflow
Sub-trip | Reason
1 | User program or derivative background stack overflow
2 | User program or derivative timed stack overflow
3 | Main system interrupt stack overflow
4 | Main system background stack overflow
{HF13} | Reserved
{HF14} | Reserved
{HF15} | Reserved
{HF16} | RTOS error (the background task has returned)
{HF17} | Reserved
{HF18} | The HF18 trip indicates that the internal flash memory has failed when writing option module parameter data. The reason for the trip can be identified by the sub-trip number.
Sub-trip | Reason
1 | Option module initialization timed out
2 | Programming error while writing menu in flash
3 | Erase flash block containing setup menus failed
4 | Erase flash block containing application menus failed
5 | Incorrect setup menu CRC contained in flash
6 | Incorrect application menu CRC contained in flash
{HF19} | The HF19 trip indicates that the drive firmware is partially or completed deleted. The drive is now in its bootloader and is waiting for a new image to be downloaded using UniMConnect. Once a new image is downloaded, the drive can run normally.

When the drive is subsequently powered up a Stored HF trip is initiated where the sub-trip number is the number of the HF trip that last occurred. This trip will occur at every power-up until it is reset. The trip can only be reset by first entering 1299 into Parameter mm.000 (mm.000).

Trip descriptions
Trips shown in the table below can be generated either from the drive control system or from the power system. The sub-trip number which is in the form xxyzz is used to identify the source of the trip. The digits xx are 00 for a trip generated by the control system or the number of a power module if generated by the power system. If the drive is not a multi-power module drive then xx will always have a value of 1 the trip is related to the power system. The y digit is used to identify the location of a trip which is generated by a rectifier module connected to a power module. Where the y digit is relevant it will have a value of 1 or more, otherwise it will be 0. The zz digits give the reason for the trip and are defined in each trip description.

Over Volts | OHt dc bus
OI ac | Phase Loss
OI Brake | LF Power Comms
PSU | OI Snubber
OHt Inverter | Reserved
OHt Power | Temp Feedback
| Power Data

Trips Summary (numerical order)

Value | Trip
--- | ---
0 | None
1 | Res
2 | OV
3 | OI.aC
4 | OI.br
5 | PSU
6 | Et
7 | O.Spd
8 | U.OI
9 | Res
10 | Th.br
11 | Tun.1
12 | Res
14 | Res
15 | Res
16 | Res
17 | Res
18 | Tun.S
19 | It.br
20 | It.ac
21 | Oht.I
22 | Oht.P
23 | Res
24 | th
25 | thS
26 | O.Ld1
27 | Oh.dc
28 | cL.A1
29 | cL.A2
30 | SCL
31 | EEF
32 | PH.Lo
33 | rS
34 | Pad
35 | CL.bt
36 | U.S
37 | Pd.S
38 | Res
39 | Res
40 | t040
41 | t041
42 | t042
43 | t043
44 | t044
45 | t045
46 | t046
47 | t047
48 | t048
49 | t049
50 | t050
51 | t051
52 | t052
53 | t053
54 | t054
55 | t055
56 | t056
57 | t057
58 | t058
59 | t059
60 | t060
61 | t061
62 | t062
63 | t063
64 | t064
65 | t065
66 | t066
67 | t067
68 | t068
69 | t069
70 | t070
71 | t071
72 | t072
73 | t073
74 | t074
75 | t075
76 | t076
77 | t077
78 | t078
79 | t079
80 | t080
81 | t081
82 | t082
83 | t083
84 | t084
85 | t085
86 | t086
87 | t087
88 | t088
89 | t089
90 | LF.Er
91 | Res
92 | OI.Sn
93 | Pb.Er
94 | Res
95 | Res
96 | UP.us
97 | D.Ch
98 | Out.P
99 | Res
100 | Reset
101 | Res
102 | Res
103 | Res
104 | Res
105 | Res
106 | Res
107 | Res
108 | Res
109 | Res
110 | dcct
111 | Res
112 | t112
113 | t113
114 | t114
115 | t115
116 | t116
117 | t117
118 | t118
119 | t119
120 | t120
121 | t121
122 | t122
123 | t123
124 | t124
125 | t125
126 | t126
127 | t127
128 | t128
129 | t129
130 | t130
131 | t131
132 | t132
133 | t133
134 | t134
135 | t135
136 | t136
137 | t137
138 | t138
139 | t139
140 | t140
141 | t141
142 | t142
143 | t143
144 | t144
145 | t145
146 | t146
147 | t147
148 | t148
149 | t149
150 | t150
151 | t151
152 | t152
153 | t153
154 | t154
155 | t155
156 | t156
157 | t157
158 | t158
159 | t159
160 | t160
161 | t161
162 | t162
163 | t163
164 | t164
165 | t165
166 | t166
167 | t167
168 | Res
169 | Res
170 | Res
171 | Res
172 | Res
173 | FaN.f
174 | C.Sl
175 | C.Pr
176 | Res
177 | Res
178 | C.by
179 | C.d.e
180 | C.OPt
181 | C.rdo
182 | C.Err
183 | C.dAt
184 | C.Ful
185 | C.Acc
186 | C.rtg
187 | C.Typ
188 | C.cPr
189 | OI.A1
190 | OI.A2
191 | Res
192 | Res
193 | Res
194 | Res
195 | Res
196 | Res
197 | Res
198 | Res
199 | dESt
200 | SL.HF
201 | SL.tO
202 | SL.Er
203 | SL.nF
204 | SL.dF
205 | Res
206 | Res
207 | Res
208 | Res
209 | Res
210 | Res
211 | Res
212 | Res
213 | Res
214 | Res
215 | Res
216 | Res
217 | Res
218 | TH.fb
219 | Oht.C
220 | P.Dat
221 | St.HF
222 | Res
223 | Res
224 | Res
225 | Cur.O
226 | So.St
227 | r.All
228 | OI.SC
229 | Res
230 | Res
231 | Cur.c
232 | Dr.Cf
233 | Res
234 | STO
235 | Pb.HF
236 | no.PS
237 | FI.In
238 | Res
239 | Res
240 | Res
241 | Res
242 | Res
243 | Res
244 | Res
245 | Pb.bt
246 | Der.E
247 | Fi.Ch
248 | Der.I
249 | UPrG
250 | R.b.ht
251 | Res
252 | Res
253 | Res
254 | Res
255 | Rst.L

Trips (alphabetical order)

Trip | C.Acc
--- | ---
Value | 185
Short description |

A communications failure has occurred with a NV media card. If this occurs during a data transfer to the card then the file being written may be corrupted. If this occurs when data is being transferred from the card then the data transfer may be incomplete. If a parameter file is transferred to the drive and this trip occurs during the transfer the parameters are not saved to non-volatile memory, and so the original parameters can be restored by powering the drive down and up again.

Recommended actions:

- Check the NV media card is installed / located correctly.
- Replace the NV media card.

Trip | C.by
--- | ---
Value | 178
Short description |

An attempt has been made to access a file on a NV media card, but the file is already being accessed be an Option Module, such as one of the Applications modules. No data is transferred.

Recommended actions:

- Wait for the Option Module to finish accessing the NV media card and re-attempt the required function.

Trip | C.cPr
--- | ---
Value | 188
Short description |

A compare has been carried out between a file on a NV media card and the drive and these are different and no other NV media card related trips have occurred.

Recommended actions:

- Set Pr mm.000 to 0 to reset the trip.
- Check to ensure the correct data block on the NV media card has been used for the compare.

Trip | C.d.e
--- | ---
Value | 179
Short description |

An attempt has been made to store data on a NV media card, but the file already exists. No data is transferred. The file should be erased first to prevent this trip.

Recommended actions:

- Erase the data in data location.
- Write data to an alternative data location.

Trip | C.dAt
--- | ---
Value | 183
Short description |

An attempt has been made to access a non-existent file on a NV media card. No data is transferred.

Recommended actions:

- Ensure data block number is correct.

Trip | C.Err
--- | ---
Value | 182
Short description |

An attempt has been made to access a NV media card, but an error has been detected in the data structure on the card. Resetting this trip will cause the drive to erase the <MCDF> folder from the NV media card (if it exists) and create the correct folder structure. On an SD card, whilst this trip is still present, missing directories will be created, and if the header file is missing it will be created. The following sub-trip numbers are used with this trip.

Sub-trip | Reason
1 | The required folder and file structure is not present.
2 | The <000> file is corrupted.
3 | Two or more files in the <MCDF\> folder have the same file identification number.

Recommended actions:

- Erase all the data block and re-attempt the process.
- Ensure the card is located correctly.
- Replace the NV media card.

Trip | C.Ful
--- | ---
Value | 184
Short description |

An attempt has been made to write to a NV media card, but there is insufficient space available. No data is transferred.

Recommended actions:

- Delete a data block or the entire NV media card to create space.
- Replace the NV media card.

Trip | C.OPt
--- | ---
Value | 180
Short description |

A parameter file has been transferred from a NV media card to the drive, but at least one of the option modules are difference between source and target drives. This trip does not stop the data transfer, but is a warning that the data for the option modules that are different will be set to the default values and not the values from the card. This trip also applies if a compare is performed between a parameter file on a card and the drive and the option modules fitted are different between the source and target.

Recommended actions:

- Ensure the correct option modules are installed.
- Ensure the option modules are in the same option module slot as the parameter set stored.
- Press the red reset button to acknowledge that the parameters for one or more of the option modules installed will be at their default vaules.
- This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.

Trip | C.Pr
--- | ---
Value | 175
Short description |

Product or derivative are incompatible between the source and target drives.

Sub-trip | Reason
1 | If Drive Derivative (11.028) is different between the source and target drives. This trip is initiated either at power-up or when the SDcard is accessed. This trip can be reset and data can be transferred in either direction between the drive and the card.
2 | If Product Type (11.063) is different between the source and target drives or the file is corrupted or incompatible. This trip is initiated either at power-up or when the SDcard is accessed. This trip can be reset but no data are transferred in either direction between the drive and the card.
3 | Reserved

Recommended actions:

Sub-trip | Actions
1 | Use a different NV media card or choose a file compatible between the source and target drives. This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.
2 | Use a different NV media card or choose a file compatible between the source and target drives.

Trip | C.rdo
--- | ---
Value | 181
Short description |

An attempt has been made to modify data on a read-only NV media card or to modify a read-only file (i.e. erase the card, erase a file or create a file). No data is transferred.

Recommended actions:

- Clear the read only flag by setting Pr mm.000 to 9777 and reset the drive. This will clear the read only flag for all data blocks in the NV media card.

Trip | C.rtg
--- | ---
Value | 186
Short description |

A parameter file has been transferred from a NV media card to the drive, but the current and/or voltage rating are different between source and target drive. This trip does not stop the data transfer, but is a warning that the data for rating dependent parameters may not be the same on the target as the source drive. This trip also applies if a compare (using Pr mm.000 set to 8yyy) is performed between a parameter file on the card on the drive.

Recommended actions:

- Reset the drive to clear the trip.
- This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.

Trip | C.Sl
--- | ---
Value | 174
Short description |

The transfer of an option module application program to or from an application module can fail because the option module does not respond correctly. If this happens this trip is produced with the sub-trip indicating the option module slot number.

Sub-trip number | Reason
1 | Error in option slot 1

Recommended actions:

- Ensure the source / destination option module is installed on the correct slot.

Trip | C.Typ
--- | ---
Value | 187
Short description |

This trip is produced during a compare if the drive mode in the file on the NV media card is different from the current drive mode and the file is a parameter file. This trip is also produced if an attempt is made to transfer a parameter file where the source and target drive modes are different and the drive mode is outside the range allowed for the target drive.

Recommended actions:

- Ensure the destination drive supports the drive operating mode in the parameter file.
- Clear the value in Pr mm.000 and reset the drive.
- Ensure destination derive operating mode is the same as the source parameter file.

Trip | cL.A1
--- | ---
Value | 28
Short description |

Indicates that a current loss was detected in current mode on Analog Input 1. In 4-20mA and 20-4mA modes. loss of input is detected if the current falls below 3mA. See Analogue Input 1 Mode (07.007) for further details.

Recommended actions:

- Check control wiring is correct.
- Check control wiring is undamaged.
- Check Analogue Input 1 Mode (07.007).
- Check that the current signal is present and greater than 3mA

Trip | cL.A2
--- | ---
Value | 29
Short description |

Indicates that a current loss was detected in current mode on Analog Input 2. In 4-20mA and 20-4mA modes. loss of input is detected if the current falls below 3mA. See Analogue Input 2 Mode (07.011) for further details.

Recommended actions:

- Check control wiring is correct.
- Check control wiring is undamaged.
- Check Analogue Input 2 Mode (07.011).
- Check that the current signal is present and greater than 3mA

Trip | CL.bt
--- | ---
Value | 35
Short description |

This trip is initiated by setting bit 12 on the control word in Control Word (06.042) when the control word is enabled (Control Word Enable (06.043) = On).

Recommended actions:

- Check the value of Control Word (06.042).
- Disable the control word in Control Word Enable (06.043).

Trip | Cur.c
--- | ---
Value | 231
Short description |

Current calibration range error.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Cur.O
--- | ---
Value | 225
Short description |

The current feedback offset is too large to be trimmed correctly.

Recommended actions:

- Ensure that there is no possibility of current flowing in the output phase of the drive when the drive is not enabled.
- Hardware fault - contact the supplier of the drive.

Trip | D.Ch
--- | ---
Value | 97
Short description |

A user action or a file system write is active that is changing the drive parameters and the drive has become active, i.e. Drive Active (10.002) = 1. The user actions that change drive parameters are loading defaults, changing drive mode, or transferring data from an NV memory card or a position feedback device to the drive. The file system actions that will cause this trip to be initiated if the drive is enabled during the transfer are writing a parameter or macro file to the drive, or transferring a derivative or user program to the drive. It should be noted that none of these actions can be started if the drive is active, and so the trip only occurs if the action is started and then the drive is enabled.

Recommended actions:

- Ensure the drive is not enabled when one of the following is being carried out:

- Loading defaults
- Transferring user programs

Trip | dcct
--- | ---
Value | 110
Short description |

DCCT reference out of range for large frames only.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Der.E
--- | ---
Value | 246
Short description |

An error has been detected in the derivative product image. The sub-trip indicated the reason for the trip.

Sub-trip | Reason | Comments
1 | The derivative image is missing or is invalid | Occurs when the drive powers-up. Load valid derivative image matching the control board hardware.
2 | The derivative image does not match the control board hardware | Occurs when the drive powers-up. Load valid derivative image matching the control board hardware.
3 | The derivative image has been changed for an image with a different derivative number. | Occurs when the drive powers-up or the image is programmed. The image tasks will not run.

Trip | Der.I
--- | ---
Value | 248
Short description |

An error has been detected in the derivative product image. The sub-trip indicated the reason for the trip.

Sub-trip | Reason | Comments
1 | Divide by zero |
2 | Undefined trip |
3 | Attempted fast parameter access set-up with non-existent parameter |
4 | Attempted access to non-existent parameter |
5 | Attempted write to read-only parameter |
6 | Attempted and over-range write |
7 | Attempted read from write-only parameter |
30 | The image has failed because either its CRC is incorrect, or there are less than 6 bytes in the image or the image header version is less than 5. | Occurs when the drive powers-up or the image is programmed. The image tasks will not run.
31 | The image requires more RAM for heap and stack than can be provided by the drive. | As 30.
32 | The image requires an OS function call that is higher than the maximum allowed. | As 30.
33 | The ID code within the image is not valid | As 30.
34 | The derivative image has been changed for an image with a different derivative number. | As 30.
40 | The timed task has not completed in time and has been suspended. |
41 | Undefined function called, i.e. a function in the host system vector table that has not been assigned. |
51 | Core menu customisation table CRC check failed | As 30.
52 | Customisable menu table CRC check failed | As 30.
53 | Customisable menu table changed | Occurs when the drive powers-up or the image is programmed and the table has changed. Defaults are loaded for the derivative menu and the trip will keep occurring until drive parameters are saved.
61 | The option module fitted in slot 1 is not allowed with the derivative image. | As 30.
62 | The option module fitted in slot 2 is not allowed with the derivative image. | As 30.
63 | The option module fitted in slot 3 is not allowed with the derivative image. | As 30.
64 | The option module fitted in slot 4 is not allowed with the derivative image. | As 30.
70 | An option module that is required by the derivative image is not fitted in any slot. | As 30.
71 | An option module specifically required to be fitted in slot 1 not present. | As 30.
72 | An option module specifically required to be fitted in slot 2 not present. | As 30.
73 | An option module specifically required to be fitted in slot 3 not present. | As 30.
74 | An option module specifically required to be fitted in slot 4 not present. | As 30.
80 | *Image is not compatible with the control board | Initiated from within the image code.
81 | *Image is not compatible with the control board serial number | As 80.

Recommended actions:

- Contact the supplier of the drive.

Trip | dESt
--- | ---
Value | 199
Short description |

This trip indicated that destination output parameters of two or more logic functions within the drive are writing to the same parameter.

Recommended actions:

- Set Pr mm.000 to "Destinations" or 12001 and check all visible parameters in all menus for parameter write conflicts

Trip | Dr.Cf
--- | ---
Value | 232
Short description |

The power stage ID does not match the rating table ID

Sub-trip | Reason
1 | The power stage ID does not match the rating table ID (Large frame only).
2 | Invalid power stage ID.
3 | The power stage ID does not match the rating table ID (Size A-D)

Recommended actions:

- Check the personnality file matches the hardware

Trip | EEF
--- | ---
Value | 31
Short description |

This trip indicates that default parameters have been loaded because of the reasons given below.

Sub-trip | Reason
1 | The most significant digit of the internal parameter database version number has changed.
2 | The CRC’s applied to the parameter data stored in internal non-volatile memory indicate that a valid set of parameters cannot be loaded.
3 | The drive mode restored from internal non-volatile memory is outside the allowed range for the product or the derivative image does not allow the previous drive mode.
4 | The drive derivative image has been changed and it has changed the customisation of the drive core menus.
5 | The power stage hardware has been change and changed the customisation of the drive core menus.
6 | Reserved
7 | Reserved
8 | The control board hardware has been change and changed the customisation of the drive core menus.
9 | The checksum on the non-parameter area of the EEPROM has failed.

The drive holds two banks of user save parameters and two banks of power down save parameters in non-volatile memory. If the last bank of either set of parameters that was saved is corrupted a User Save or Power Down Save trip is produced. If one of these trips occurs the parameters values that were last saved successfully are used. It can take some time to save parameters when requested by the user and if the power is removed from the drive during this process it is possible to corrupt the data in the non-volatile memory.

If both banks of user save parameters or both banks of power down save parameters are corrupted or one of the other conditions given in the table above occurs EEPROM Fail.xxx trip is produced. If this trip occurs it is not possible to use the data that has been saved previously, and so the drive will be loaded with default parameters. The trip can only be reset if Parameter mm.000 (mm.000) is set to 10, 11, 1233 or 1244 or if Load Defaults (11.043) is set to a non-zero value

Trip | Et
--- | ---
Value | 6
Short description |

External trip is initiated as shown in the table below.

Sub-trip | Reason
3 | External Trip (10.032) = 1

Recommended actions:

- Check the value of External Trip (10.032).
- Select "Destinations" (or enter 12001) in Pr mm.000 and check for a parameter controlling External Trip (10.032).
- Ensure External Trip (10.032) or User Trip (10.038) (=6) is not being used by serial comms.

Trip | FaN.f
--- | ---
Value | 173
Short description |

Fan failure

Recommended actions:

- Check that the fan is fitted and connected correctly.
- Contact the supplier of the drive to replace the fan.

Trip | Fi.Ch
--- | ---
Value | 247
Short description |

Rating table changed

Recommended actions:

- Power cycle drive

Trip | FI.In
--- | ---
Value | 237
Short description |

Firmware version between user board and power board does not match.

Trip | It.ac
--- | ---
Value | 20
Short description |

This trip indicates a motor thermal overload based on the Motor Rated Current (05.007) and Motor Thermal Time Constant 1 (04.015). Motor Protection Accumulator (04.019) displays the motor temperature as a percentage of the maximum value. The drive will trip on Motor Too Hot when Motor Protection Accumulator (04.019) gets to 100%.

Recommended actions:

- Ensure the load is not jammed / sticking.
- Check the load on the motor has not changed.
- Tune the Motor Rated Speed (05.008) (RFC-A mode only).
- Ensure the motor rated current is not zero.

Trip | It.br
--- | ---
Value | 19
Short description |

This trip indicates that braking resistor overload has timed out. The value in Braking Resistor Thermal Accumulator (10.039) is calculated using Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061). This trip is initiated when Braking Resistor Thermal Accumulator (10.039) reaches 100%.

Recommended actions:

- Ensure the values entered in Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061) are correct.
- If an external thermal protection device is being used and the braking resistor software overload protection is not required, set Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061) to 0 to disable the trip.

Trip | LF.Er
--- | ---
Value | 90
Short description |

This trip is initiated if there is no communications between power, control or the rectifier module or if excessive communication errors have been detected. The reason for the trip can be identified by the sub-trip number.

Source | xx | y | zz
Control system | 00 | 0 | 01: No communications between the control system and the power system.
Control system | 00 | 0 | 02: Excessive communication errors between the control system and power system.
Control system | 01 | 1 | 00: Excessive communications errors detected by the rectifier module.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | no.PS
--- | ---
Value | 236
Short description |

Reserved trip number.

Trip | None
--- | ---
Value | 0
Short description |

Trip | O.Ld1
--- | ---
Value | 26
Short description |

This trip indicates that the total current drawn from the AI adaptor 24V or from the digital output has exceeded the limit.

Sub-trip | Reason
1 | Digital output or 24V supply load on control terminal is too high.
2 | AI adptor 24V load is too high

Recommended actions:

- Check total loads on digital outputs and 24V.
- Check control wiring is correct.
- Check output wiring is undamaged

Trip | O.Spd
--- | ---
Value | 7
Short description |

If the Post Ramp Reference (02.001) exceeds the threshold set in Over Frequency Threshold (03.008) in either direction, a Reserved trip is produced.

If Over Frequency Threshold (03.008) is set to 0.0 the threshold is based on the variable minimum/maximum for the references and is equal to 1.2 x VM_SPEED_FREQ_REF[MAX].

Recommended actions:

- Reduce the Frequency Controller Proportional Gain Kp1 (03.010) to reduce the frequency overshoot.

Trip | Oh.dc
--- | ---
Value | 27
Short description |

This trip indicates a DC bus component over temperature based on a firmware thermal model. The drive includes a thermal protection system to protect the DC bus components within the drive. This includes the effects of the output current and DC bus ripple. The estimated temperature is displayed as a percentage of the trip level in Percentage Of d.c. Link Thermal Trip Level (07.035). If this parameter reaches 100% then an OHt dc bus trip is initiated. The drive will attempt to stop the motor before tripping. If the motor does not stop in 10 seconds then the drive trips immediately.

Source | xx | y | zz
Control system | 00 | 2 | 00: D.c. link thermal model gives OHt dc bus trip with sub-trip 0.

Recommended actions:

- Check the AC supply voltage balance and levels.
- Check the DC bus ripple level.
- Reduce duty cycle.
- Reduce motor load.
- Check output current stability. If unstable;

- Check the motor map settings with motor nameplate (Motor Rated Frequency (05.006), Motor Rated Current (05.007), Motor Rated Speed (05.008), Motor Rated Voltage (05.009), Motor Rated Power Factor (05.010) and Number Of Motor Poles (05.011)
- Disable slip compensation (Slip Compensation Level (05.027) = 0.0%)
- Disable dynamic V to F operation (Flux Optimisation Select, Dynamic V To F Select (05.013) = Off (0))
- Select fixed boost (Control Mode (05.014) = Fixed (2))
- Select high stability space vector modulation ( High Stability Space Vector Modulation (05.019) = On (1))
- Disconnect the load and complete a rotating auto-tune (Auto-tune (05.012) = 2)
- Reduce frequency loop gains (Frequency Controller Proportional Gain Kp1 (03.010), Frequency Controller Integral Gain Ki1 (03.011) and Frequency Controller Differential Feedback Gain Kd1 (03.012))
- Add a current demand filter (Current Reference Filter 1 Time Constant (04.012))

Trip | Oht.C
--- | ---
Value | 219
Short description |

This trip indicates that a control stage over-temperature has been detected if Cooling Fan control (06.045) = 0.

This trip causes the option module to go to standby and Potential Drive Damage Conditions (10.106) bit 1 to be set.

Recommended actions:

- Increase ventilation by setting Cooling Fan control (06.045) > 0.

Trip | Oht.I
--- | ---
Value | 21
Short description |

This trip indicates that an IGBT junction over-temperature has been detected based on a firmware thermal model.

Source | xx | y | zz
Control system | 00 | 1 | 00: Inverter thermal model gives OHt Inverter trip with sub-trip 0.

Recommended actions:

- Reduce the selected drive switching frequency.
- Ensure Auto-switching Frequency Change Disable (05.035) is set to Off.
- Reduce duty cycle.
- Decrease acceleration / deceleration rates.
- Reduce motor load.
- Check DC bus ripple.
- Ensure all three input phases are present and balanced

Trip | Oht.P
--- | ---
Value | 22
Short description |

This trip indicates that a power stage over-temperature has been detected. From the sub-trip "xxyzz", the thermistor location is identified by "zz".

Source | xx | y | zz
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power system gives OHt Power trip with sub-trip xx0zz.

Recommended actions:

- Check enclosure / drive fans are still functioning correctly.
- Force the heatsink fans to run at maximum speed.
- Check enclosure ventilation paths.
- Check enclosure door filters.
- Increase ventilation.
- Reduce duty cycle.
- Decrease acceleration / deceleration rates.
- Reduce motor loads.
- Check the derating tables and confirm the drive is correctly sized for the application.
- Use a drive with larger current / power rating.

Trip | OI.A1
--- | ---
Value | 189
Short description |

Analogue input 1 over current.

Trip | OI.A2
--- | ---
Value | 190
Short description |

Not supported

Trip | OI.aC
--- | ---
Value | 3
Short description |

This trip indicates that the instantaneous drive output current has exceeded the drive over current threshold.

Source | xx | y | zz
Control system | 00 | 0 | 00: Instantaneous over-current trip when the measured a.c. current exceeds the over current threshold.

The over current threshold is the maximum current the drive can measure and is defined by VM_DRIVE_CURRENT[MAX]

Recommended actions:

- Acceleration / deceleration rate is too short.
- If seen during auto-tune reduce the voltage boost.
- Check for short circuit on the output cabling.
- Check integrity of the motor insulation using a Megger.
- Check motor cable is within limits for the frame size.
- Reduce frequency loop gains (Frequency Controller Proportional Gain Kp1 (03.010), Frequency Controller Integral Gain Ki1 (03.011) and Frequency Controller Differential Feedback Gain Kd1 (03.012))
- Reduce the current loop gains.

Trip | OI.br
--- | ---
Value | 4
Short description |

This trip indicates that an over-current has been detected in braking IGBT or braking IGBT protection has been activated.

Source | xx | y | zz
Power system | 01 | 0 | 00: Braking IGBT instantaneous over-current trip

Recommended actions:

- Check brake resistor wiring.
- Check braking resistor value is greater than or equal to the minimum resistance value.
- Check braking resistor insulation.

Trip | OI.SC
--- | ---
Value | 228
Short description |

Output phase short circuit.

Recommended actions:

- Check motor and connection to motor

Trip | OI.Sn
--- | ---
Value | 92
Short description |

This trip indicates that an over-current condition has been detected in the rectifier snubbing circuit, The exact cause of the trip can be identified by the sub-trip number.

Source | xx | y | zz
Power system | 01 | 1 | 00: Rectifier snubber over-current trip detected.

Recommended actions:

- Ensure the internal EMC filter is installed.
- Ensure the motor cable length does not exceed the maximum for selected switching frequency.
- Check for supply voltage imbalance.
- Check for supply disturbance such as notching from a DC drive.
- Check the motor and motor cable insulation with a Megger.
- Fit an output line reactor or sinusoidal filter

Trip | Out.P
--- | ---
Value | 98
Short description |

Output phase loss detected. A test can be made for output phase loss when the drive is enabled or the output phase loss condition can be detected while the drive is running as defined by Output Phase Loss Detection Enable (06.059).

Sub-trip | Reason
1 | Phase U is not connected when drive is enabled
2 | Phase V is not connected when drive is enabled
3 | Phase W is not connected when drive is enabled
4 | The drive output frequency is above 4Hz and a phase is disconnected for the time specified by Output Phase Loss Detection Time (06.058)

Recommended actions:

- Check motor and drive connections.
- To disable the trip set Output Phase Loss Detection Enable (06.059) to Off.

Trip | OV
--- | ---
Value | 2
Short description |

This trip indicates the the DC bus voltage has exceeded VM_DC_VOLTAGE[MAX] instantaneously or VM_DC_VOLTAGE_SET[MAX] for 15s. The trip threshold varies depending on voltage rating of the drive as shows below.

Voltage rating | VM_DC_VOLTAGE[MAX] | VM_DC_VOLTAGE_SET[MAX]
200 | 415 | 410
400 | 830 | 815
575 | 990 | 970

The exact cause of the trip can be identified by the sub-trip number.

Source | xx | y | zz
Control system | 00 | 0 | 01: Instantaneous trip when the d.c. link voltage exceeds VM_DC_VOLTAGE[MAX].
Control system | 00 | 0 | 02: Time delayed trip indicating that the d.c. link voltage is above VM_DC_VOLTAGE_SET[MAX].
Power system | 01 | 0 | 00: Instantaneous trip when the d.c. link voltage exceeds VM_DC_VOLTAGE[MAX].

Recommended actions:

- Increase deceleration ramp.
- Decrease the braking resistor value (staying above the minimum value).
- Check nominal AC supply level.
- Check for supply disturbances which could cause the DC bus level to rise.
- Check motor insulation using a Megger.

Trip | P.Dat
--- | ---
Value | 220
Short description |

This trip can be generated either from the drive control system or from the power system.

This trip is produced if there is an error in the configuration data stored in the power system. If the source of the trip is the control system then the trip related to the table that is uploaded from the power system at power-up.

Source | xx | y | zz
Control system | 00 | 0 | 01: No data was obtained because this was skipped.
Control system | 00 | 0 | 02: There is no data table in node 1.
Control system | 00 | 0 | 03: The power system data table is bigger than the space available in the control pod to store it.
Control system | 00 | 0 | 04: The size of the table given in the table is incorrect
Control system | 00 | 0 | 05: Table CRC error.
Control system | 00 | 0 | 06: The version number of the generator software that produced the table is too low, i.e. a table from a newer generator is required that includes features that have been added to the table that may not be present.
Control system | 00 | 0 | 07: The power data table failed to be stored in the power board.
Power system | 01 | 0 | 00: The power data table used internally by the power module has an error.
Power system | 01 | 0 | 01: The power data table that is uploaded to the control system on power up has an error.
Power system | 01 | 0 | 02: The power data table used internally by the power module does not match the hardware identification of the power module.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Pad
--- | ---
Value | 34
Short description |

If keypad reference mode is enabled (Reference Selected Indicator (01.049) = 4 or 6) (i.e. Reference Selector (01.014) is set to 4 or 6 if motor map 1 is selected, or M2 Reference Selector (21.003) is set to 4 or 6 if motor map 2 is selected) and the keypad removed, then this trip is initiated.

Recommended actions:

- Re-install keypad and reset.
- Change Reference Selector (01.014) to select the reference from another source.

Trip | Pb.bt
--- | ---
Value | 245
Short description |

Power board is in its bootloader

Recommended actions:

- Send power board firmware file to reprogram the power board and power cycle drive.

Trip | Pb.Er
--- | ---
Value | 93
Short description |

Communication between the flavour and the olympian power board was lost. The exact cause of the trip can be identified by the sub-trip number.

Sub-trip number | Reason
1 | PLL operating region out of lock
2 | Power board lost communication with user board
3 | User board lost communication with power board
4 | Communication CRC error

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Pb.HF
--- | ---
Value | 235
Short description |

Reserved trip number.

Trip | Pd.S
--- | ---
Value | 37
Short description |

This trip indicates that an error has been detected in the power down save parameters stored in non-volatile memory.

Recommended actions:

- Perform a 1001 save in Pr mm.000 to ensure that the trip doesn't occur the next time the drive is powered up.

Trip | PH.Lo
--- | ---
Value | 32
Short description |

This trip indicates that the drive has detected an input phase loss or large supply imbalance. The drive will attempt to stop the motor before the trip is initiated. If the motor cannot be stopped in 10 seconds the trip occurs immediately. This trip works by monitoring the ripple voltage on the DC bus of the drive, if the DC buss ripple exceeds the threshold, the drive will trip on Phase Loss. Potential causes of the DC bus ripple are input phase loss, large supply impedance and severe output current instability.

Source | xx | y | zz
Control system | 00 | 0 | 00: Phase loss detected based on control system feedback. The drive attempts to stop the drive before tripping unless bit 2 of Action On Trip Detection (10.037) is set to one.
Power system | 01 | 0 | 00: Phase loss has been detected by the rectifier module.
Control system | 01 | 1 | 01: Supply loss has been detected by the rectifier module in a multi-power module system, where this must be treated as a phase loss condition to prevent damage to the drive.

Input phase loss detection can be disabled when the drive required to operate from the DC supply or from a single phase supplpy in Input Phase Loss Detection Mode (06.047).

Recommended actions:

- Check the AC supply voltage balance and level at full load.
- Check the DC bus ripple level with an isolated oscilloscope.
- Check the output current stability.
- Reduce the duty cycle.
- Reduce the motor load.
- Disable the phase loss detection by setting Input Phase Loss Detection Mode (06.047) to Disabled.

Trip | PSU
--- | ---
Value | 5
Short description |

This trip indicates that one or more internal power supply rails are outside limits or overloaded.

Source | xx | y | zz
Control system | 00 | 0 | 00: Internal power supply overload
Power system | 01 | 1 | 00: Internal power supply overload

Recommended actions:

- Remove any option modules and perform a reset.
- Hardware fault within the drive - return the drive to the supplier.

Trip | r.All
--- | ---
Value | 227
Short description |

An option module, derivative image or user program image has requested more parameter RAM than is allowed. The RAM allocation is checked in order of resulting sub-trip numbers, and so the failure with the highest sub-trip number is given. The sub-trip is calculated as (parameter size x 1000) + (parameter type x 100) + sub-array number. Note that if this trip occurs, all menu customisation provided by option modules, the derivative image or the user program image is not used. The tables below show the values corresponding to the parts of the sub-trip number.

Parameter size | Value
1 bit | 1
8 bit | 2
16 bit | 3
32 bit | 4
64 bit | 5

Parameter type | Value
Volatile | 0
User save | 1
Power-down save | 2

Derivatives can customise menus 18 and 20.

Sub-array | Menus | Value
Applications menus | 18-20 | 1
Derivative image | 29 | 2
User program image | 30 | 3
Option slot 1 set-up | 15 | 4
Option slot 1 applications | 25 | 5

Trip | R.b.ht
--- | ---
Value | 250
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 1
Short description |

The under voltage condition is now a drive state, and so this trip is no longer used by the drive.

Trip | Res
--- | ---
Value | 9
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 12
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 14
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 15
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 16
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 17
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 23
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 38
Short description |

Reserved

Trip | Res
--- | ---
Value | 39
Short description |

Indicates that a current loss was detected in current mode on Analog Input 3. In 4-20mA and 20-4mA modes. loss of input is detected if the current falls below 3mA. See Analogue I/O 3 Mode (07.015) for further details.

Recommended actions:

- Check control wiring is correct.
- Check control wiring is undamaged.
- Check Analogue I/O 3 Mode (07.015)
- Check that the current signal is present and greater than 3mA

Trip | Res
--- | ---
Value | 91
Short description |

Reserved

Trip | Res
--- | ---
Value | 94
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 95
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 99
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 101
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 102
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 103
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 104
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 105
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 106
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 107
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 108
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 109
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 111
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 168
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 169
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 170
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 171
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 172
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 176
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 177
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 191
Short description |

Not supported

Trip | Res
--- | ---
Value | 192
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 193
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 194
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 195
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 196
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 197
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 198
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 205
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 206
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 207
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 208
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 209
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 210
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 211
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 212
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 213
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 214
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 215
Short description |

During drive mode changeover option modules must acknowledge that they have stopped accessing the communications system between the option slots and the drive. If an option module does not do this in the allowed time then this trip is produced.

Recommended actions:

- Reset the trip.
- If the trip persists, replace the option module.

Trip | Res
--- | ---
Value | 216
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 217
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 222
Short description |

Reserved

Trip | Res
--- | ---
Value | 223
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 224
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 229
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 230
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 233
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 238
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 239
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 240
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 241
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 242
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 243
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 244
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 251
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 252
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 253
Short description |

Reserved trip number.

Trip | Res
--- | ---
Value | 254
Short description |

Reserved trip number.

Trip | Reset
--- | ---
Value | 100
Short description |

This is not a valid trip number as this value is used in User Trip (10.038) to reset the drive.

Trip | rS
--- | ---
Value | 33
Short description |

During auto-tune it is possible to attempt to measure the resistance of the motor connected to the drive. If the measured value or a value written to this parameter by the user exceeds (VFS / v2) / Full Scale Current Kc (11.061), where VFS is the full scale d.c. link voltage then this trip is initiated.

Recommended actions:

- Check the motor cable / connections.
- Check the integrity of the motor stator winding using an insulation tester.
- Check the motor phase to phase resistance at the drive terminals.
- Check the motor phase to phase resistance at the motor terminals.
- Ensure the stator resistance of the motor falls within the range of the drive model.
- Select fixed boost mode (Control Mode (05.014) = Fixed) and verify the output current waveforms with an oscilloscope.
- Replace the motor.

Trip | Rst.L
--- | ---
Value | 255
Short description |

This is not a valid trip number as this value is used in User Trip (10.038) to reset the trip logs.

Trip | SCL
--- | ---
Value | 30
Short description |

This trip indicates that the control word watchdog has been enabled and has timed out.

Trip | SL.dF
--- | ---
Value | 204
Short description |

If the option module fitted in option slot 1 is different to the option module present at the last power-down then this trip is produced. The sub-trip number gives the identification code of the module that was originally fitted. Drive user parameters must be saved to prevent this trip on the next power-up if the module has changed. If the menus have been changed, but not the module, the trip will not occur on the next power-up. The sub-trip number gives the following indications of the reason for the trip.

Sub-trip | Reason
1 | No module was fitted previously
2 | A module with the same identifier is fitted, but the set-up menu for this option slot has been changed, and so default parameters have been loaded for this menu.
3 | A module with the same identifier is fitted, but the applications menu for this option slot has been changed, and so default parameters have been loaded for this menu.
4 | A module with the same identifier is fitted, but the set-up and applications menu for this option slot have been changed, and so default parameters have been loaded for these menus.
>99 | Shows the identifier of the module previously fitted.

Recommended actions:

- Turn off the power, ensure the correct option modules are installed in the correct option slots and re-apply the power.
- Confirm that the currently installed option module is correct, ensure option module parameters are set correctly and perform a user save in Pr mm.000.

Trip | SL.Er
--- | ---
Value | 202
Short description |

The option module in option slot 1 has indicated an error. The option module can give the reason for the error and this is shown in the sub-trip number. As default the sub-trip number is shown as a number on the display, however, it is possible for the option module to supply sub-trip number strings which will be displayed instead of the number if available.

Recommended actions:

- See relevant Option Module User Guide for details of the trip.

Trip | SL.HF
--- | ---
Value | 200
Short description |

This trip indicates that there is a fault with the option module in option slot 1 that means that this module cannot operate. The possible causes of the trip are given by the sub-trip value.

Sub-trip | Reason
1 | The module category cannot be identified
2 | All the required customisable menu table information has not been supplied or the tables supplied are corrupt
3 | There is insufficient memory available to allocate the comms buffers for this module.
4 | The module has not indicated that it is running correctly during drive power-up
5 | The module has been removed after power-up or it has ceased to indicate to the drive processor that it is still active.
6 | The module has not indicated that it has stopped accessing drive parameters during a drive mode change
7 | The module has failed to acknowledge that a request has been made to reset the drive processor.
8 | The drive failed to read correctly the menu table from the module during drive power-up.
9 | The drive failed to upload menu tables from the module and timed-out (5s).
10 | Menu table CRC invalid.

Recommended actions:

- Ensure the option module is installed correctly.
- Replace the option module.
- Replace the drive.

Trip | SL.nF
--- | ---
Value | 203
Short description |

Each option module fitted in the drive is identified at power-up and the option fitted is stored by the drive in its non-volatile memory. If an option module was fitted in slot 1 at power-down, but that option module has subsequently been removed before power up then this trip is produced. The sub-trip number gives the identification code of the option module that has been removed. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Ensure the option module is installed correctly.
- Re-install the option module.
- To confirm that the removed option module is no longer required perform a save function in Pr mm.000.

Trip | SL.tO
--- | ---
Value | 201
Short description |

This trip indicates that the option module in option slot 1 has started the option watchdog function and then failed to service this watchdog correctly.

Recommended actions:

- Replace the option module.

Trip | So.St
--- | ---
Value | 226
Short description |

This trip indicates that the soft soft start system has remained active when it should be inactive. For a resistor based soft start this means that the soft start shorting relay has not closed.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | St.HF
--- | ---
Value | 221
Short description |

If an HF01 to HF17 trip occurs then a Stored HF trip occurs each time the drive is powered up until this trip is reset. The sub-trip code is the number of the original HF trip. The Stored HF trip can only be reset by first writing 1299 to Pr mm.000 and resetting the drive.

Recommended actions:

- Enter 1299 into Pr mm.000 and press reset to clear the trip.

Trip | STO
--- | ---
Value | 234
Short description |

STO board not fitted.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | t040
--- | ---
Value | 40
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t041
--- | ---
Value | 41
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t042
--- | ---
Value | 42
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t043
--- | ---
Value | 43
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t044
--- | ---
Value | 44
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t045
--- | ---
Value | 45
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t046
--- | ---
Value | 46
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t047
--- | ---
Value | 47
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t048
--- | ---
Value | 48
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t049
--- | ---
Value | 49
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t050
--- | ---
Value | 50
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t051
--- | ---
Value | 51
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t052
--- | ---
Value | 52
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t053
--- | ---
Value | 53
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t054
--- | ---
Value | 54
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t055
--- | ---
Value | 55
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t056
--- | ---
Value | 56
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t057
--- | ---
Value | 57
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t058
--- | ---
Value | 58
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t059
--- | ---
Value | 59
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t060
--- | ---
Value | 60
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t061
--- | ---
Value | 61
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t062
--- | ---
Value | 62
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t063
--- | ---
Value | 63
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t064
--- | ---
Value | 64
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t065
--- | ---
Value | 65
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t066
--- | ---
Value | 66
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t067
--- | ---
Value | 67
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t068
--- | ---
Value | 68
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t069
--- | ---
Value | 69
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t070
--- | ---
Value | 70
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t071
--- | ---
Value | 71
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t072
--- | ---
Value | 72
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t073
--- | ---
Value | 73
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t074
--- | ---
Value | 74
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t075
--- | ---
Value | 75
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t076
--- | ---
Value | 76
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t077
--- | ---
Value | 77
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t078
--- | ---
Value | 78
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t079
--- | ---
Value | 79
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t080
--- | ---
Value | 80
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t081
--- | ---
Value | 81
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t082
--- | ---
Value | 82
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t083
--- | ---
Value | 83
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t084
--- | ---
Value | 84
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t085
--- | ---
Value | 85
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t086
--- | ---
Value | 86
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t087
--- | ---
Value | 87
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t088
--- | ---
Value | 88
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t089
--- | ---
Value | 89
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t112
--- | ---
Value | 112
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t113
--- | ---
Value | 113
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t114
--- | ---
Value | 114
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t115
--- | ---
Value | 115
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t116
--- | ---
Value | 116
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t117
--- | ---
Value | 117
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t118
--- | ---
Value | 118
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t119
--- | ---
Value | 119
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t120
--- | ---
Value | 120
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t121
--- | ---
Value | 121
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t122
--- | ---
Value | 122
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t123
--- | ---
Value | 123
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t124
--- | ---
Value | 124
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t125
--- | ---
Value | 125
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t126
--- | ---
Value | 126
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t127
--- | ---
Value | 127
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t128
--- | ---
Value | 128
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t129
--- | ---
Value | 129
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t130
--- | ---
Value | 130
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t131
--- | ---
Value | 131
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t132
--- | ---
Value | 132
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t133
--- | ---
Value | 133
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t134
--- | ---
Value | 134
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t135
--- | ---
Value | 135
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t136
--- | ---
Value | 136
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t137
--- | ---
Value | 137
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t138
--- | ---
Value | 138
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t139
--- | ---
Value | 139
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t140
--- | ---
Value | 140
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t141
--- | ---
Value | 141
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t142
--- | ---
Value | 142
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t143
--- | ---
Value | 143
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t144
--- | ---
Value | 144
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t145
--- | ---
Value | 145
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t146
--- | ---
Value | 146
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t147
--- | ---
Value | 147
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t148
--- | ---
Value | 148
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t149
--- | ---
Value | 149
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t150
--- | ---
Value | 150
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t151
--- | ---
Value | 151
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t152
--- | ---
Value | 152
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t153
--- | ---
Value | 153
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t154
--- | ---
Value | 154
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t155
--- | ---
Value | 155
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t156
--- | ---
Value | 156
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t157
--- | ---
Value | 157
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t158
--- | ---
Value | 158
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t159
--- | ---
Value | 159
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t160
--- | ---
Value | 160
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t161
--- | ---
Value | 161
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t162
--- | ---
Value | 162
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t163
--- | ---
Value | 163
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t164
--- | ---
Value | 164
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t165
--- | ---
Value | 165
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t166
--- | ---
Value | 166
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | t167
--- | ---
Value | 167
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | th
--- | ---
Value | 24
Short description |

This trip indicates that the motor thermistor has indicated a motor over-temperature.

If Digital input 5 mode (08.035) is 2 then a Thermistor trip is initiated if the feedback value is higher than Thermistor Trip Threshold (07.048).

Recommended actions:

- Check motor temperature.
- Check thermistor continuity.

Trip | Th.br
--- | ---
Value | 10
Short description |

If hardware based braking resistor thermal monitoring is provided and the resistor overheats this trip is initiated. If the braking resistor is not present then this trip must be disabled with bit 3 of Action On Trip Detection (10.037) to prevent this trip.

Recommended actions:

- Check braking resistor wiring.
- Check braking resistor value is greater than or equal to the minimum resistance value.
- Check braking resistor insulation.

Trip | TH.fb
--- | ---
Value | 218
Short description |

This trip indicates a fault with a thermistor in the drive (i.e. open circuit or short circuit).

Source | xx | y | zz
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power system
Power system | 01 | 1 | zz: Thermistor location defined by zz in the rectifier

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | thS
--- | ---
Value | 25
Short description |

This trip indicates that the motor thermistor is short circuited or has a low impedance.

Digital input 5 mode (08.035) and the resistance of the thermistor connected to DI 5 is less than 50O.

Recommended actions:

- Check thermistor continuity.
- Replace motor / motor thermistor

Trip | Tun.1
--- | ---
Value | 11
Short description |

The drive has tripped during an auto-tune. The cause of the trip can be identified from the sub-trip number.

Sub-trip | Reason
1 | Reserved
2 | The motor did not reach the required speed during rotating auto-tune or mechanical load measurement.

Recommended actions:

- Ensure the motor is free to turn i.e. mechanical brake is realeased.

Trip | Tun.S
--- | ---
Value | 18
Short description |

The drive was prevented from completing an auto-tune, because either the Final drive enable or the Final drive run were removed.

Recommended actions:

- Check the drive enable signal (Terminal 31&34) was active during the auto-tune.
- Check the run command was active in Digital Input 5 State (08.005) during the auto-tune.

Trip | U.OI
--- | ---
Value | 8
Short description |

Reserved trip number.

Trip | U.S
--- | ---
Value | 36
Short description |

This trip indicates that an error has been detected in the user save parameters saved in non-volatile memory. For example, following a user save command, if the power to the drive was removed when the user parameters were being saved.

Recommended actions:

- Perform a user save in Pr mm.000 to ensure that the trip doesn't occur the next time the drive is powered up.
- Ensure that the drive has enough time to complete the save before removing the power to the drive.

Trip | UP.us
--- | ---
Value | 96
Short description |

This trip can be initiated from within an onboard user program using a function call which defines the sub-trip number.

Recommended actions:

- Check the user program

Trip | UPrG
--- | ---
Value | 249
Short description |

Not supported