# Menu 7 Single Line Descriptions − Analog I/O

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
07.001 | Analogue Input 1 | ±100.00 % |  | RO | Num | ND | NC | PT | FI
07.002 | Analogue Input 2 | 0.00 to 100.00 % |  | RO | Num | ND | NC | PT | FI
07.004 | Stack Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.005 | Auxiliary Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.007 | Analogue Input 1 Mode | 4‑20.S (‑6), 20‑4.S (‑5), 4‑20.L (‑4), 20‑4.L (‑3), 4‑20.H (‑2), 20‑4.H (‑1), 0‑20 (0), 20‑0 (1), 4‑20.tr (2), 20‑4.tr (3), 4‑20 (4), 20‑4 (5), Volt (6) | Volt (6) | RW | Txt |  |  |  | US
07.008 | Analogue Input 1 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
07.009 | Analogue Input 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
07.010 | Analogue Input 1 Destination A | 0.000 to 30.999 | 1.036 | RW | Num | DE |  | PT | US
07.011 | Analogue Input 2 Mode | Volt (6), dig (7) | Volt (6) | RW | Txt |  |  |  | US
07.012 | Analogue Input 2 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
07.013 | Analogue Input 2 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
07.014 | Analogue Input 2 Destination A | 0.000 to 30.999 | 1.037 | RW | Num | DE |  | PT | US
07.019 | Analogue Output 1 Source A | 0.000 to 30.999 | 2.001 | RW | Num |  |  | PT | US
07.020 | Analogue Output 1 Scaling | 0.000 to 40.000 | 1.000 | RW | Num |  |  |  | US
07.026 | Analog Input 1 Preset on Current Loss | 4.00 to 20.00 mA | 4.00 mA | RW | Num |  |  |  | US
07.028 | Analogue Input 1 Current Loop Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
07.030 | Analogue Input 1 Offset | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.031 | Analogue Input 2 Offset | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.034 | Inverter Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.035 | Percentage Of d.c. Link Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.036 | Percentage Of Drive Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.037 | Temperature Nearest To Trip Level | 0 to 29999 |  | RO | Num | ND | NC | PT |
07.046 | Thermistor Type | D44081 (0), 84 (1), PT1000 (2), PT2000 (3), other (4) | D44081 (0) | RW | Txt |  |  |  | US
07.047 | Thermistor Feedback | 0 to 4000 Ω |  | RO | Num | ND | NC | PT | FI
07.048 | Thermistor Trip Threshold | 0 to 4000 Ω | 3300 Ω | RW | Num |  |  |  | US
07.049 | Thermistor Reset Threshold | 0 to 4000 Ω | 1800 Ω | RW | Num |  |  |  | US
07.050 | Thermistor Temperature | -50 to 300 °C |  | RO | Num | ND | NC | PT | FI
07.051 | Analogue Input 1 Control | 0 to 5 | 0 | RW | Num |  |  |  | US
07.052 | Analogue Input 2 Control | 0 to 5 | 0 | RW | Num |  |  |  | US
07.055 | Analogue Output 1 Control | 0 to 15 | 0 | RW | Num |  |  |  | US
07.061 | Analogue Input 1 Minimum Reference | 0.00 to 100.00 % | 0.00 % | RW | Num |  |  |  | US
07.062 | Analogue Input 1 At Minimum Reference | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.063 | Analogue Input 1 Maximum Reference | 0.00 to 100.00 % | 100.00 % | RW | Num |  |  |  | US
07.064 | Analogue Input 1 At Maximum Reference | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.065 | Analogue Input 2 Minimum Reference | 0.00 to 100.00 % | 0.00 % | RW | Num |  |  |  | US
07.066 | Analogue Input 2 At Minimum Reference | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.067 | Analogue Input 2 Maximum Reference | 0.00 to 100.00 % | 100.00 % | RW | Num |  |  |  | US
07.068 | Analogue Input 2 At Maximum Reference | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.090 | Analogue Input 1 Destination B | 0.000 to 30.999 | 0.000 | RO | Num | DE |  | PT | US
07.094 | Analogue Input 2 Destination B | 0.000 to 30.999 | 0.000 | RO | Num | DE |  | PT | US
07.099 | Analogue Output 1 Source B | 0.000 to 30.999 | 0.000 | RO | Num |  |  | PT | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |