# Menu 8 − Digital I/O

Mode: RFC‑A

Parameter | 08.001 Digital I/O 1 State
--- | ---
Short description | Displays the state for digtial input/output1
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital I/O 1 State (08.001) represents the digital input/output 1 state whether it is a digital input or an output.

If Digital I/O 01 mode (08.031) = 0 then it is a digital input:

- Comply with IEC 61131-2. Positive logic only.
- Digital I/O 1 State (08.001) = 0 if the digital I/O is low (<9V)
- Digital I/O 1 State (08.001) = 1 if the digital I/O is high (>11V).

If Digital I/O 01 mode (08.031) = 1 then it is a digital output:

- 200mA total current including +24Vout; (50mA max per output).
- Positive logic only (with 6-7kΩ pull down).
- Digital I/O 1 State (08.001) = 0 if the source parameter value less than 50% of its range.
- Digital I/O 1 State (08.001) = 1 if the source parameter value more than 50% of its range.

If Digital I/O 01 mode (08.031) = 2 then it is a frequency output.

If Digital I/O 01 mode (08.031) = 3 then it is a PWM output.

Parameter | 08.002 Digital I/O 2 State
--- | ---
Short description | Displays the state for digtial input/output 2
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital I/O 2 State (08.002) represents the digital input 2 state.

- Comply with IEC 61131-2. Positive logic only.
- Digital I/O 2 State (08.002) = 0 if the digital input is low (<9V)
- Digital I/O 2 State (08.002) = 1 if the digital input is high (>11V).

Parameter | 08.003 Digital Input 3 State
--- | ---
Short description | Displays the state for digtial input 3
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital Input 3 State (08.003) represents the digital input 3 state.

- Comply with IEC 61131-2. Positive logic only.
- Digital Input 3 State (08.003) = 0 if the digital input is low (<9V)
- Digital Input 3 State (08.003) = 1 if the digital input is high (>11V).

Parameter | 08.004 Digital Input 4 State
--- | ---
Short description | Displays the state for digtial input 4
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital Input 4 State (08.004) represents the digital input 4 state.

- Comply with IEC 61131-2. Positive logic only.
- Digital Input 4 State (08.004) = 0 if the digital input is low (<9V)
- Digital Input 4 State (08.004) = 1 if the digital input is high (>11V).

Parameter | 08.005 Digital Input 5 State
--- | ---
Short description | Displays the state for digtial input 5
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital Input 5 State (08.005) represents the digital input 5 state if Digital input 5 mode (08.035) = 0.

- Comply with IEC 61131-2. Positive logic only.
- Digital Input 5 State (08.005) = 0 if the digital input is low (<9V)
- Digital Input 5 State (08.005) = 1 if the digital input is high (>11V).

Parameter | 08.008 Relay 1 Output State
--- | ---
Short description | Displays the state for relay 1
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Relay 1 Output State (08.008) shows the state of Relay 1.

Parameter | 08.011 Digital I/O 1 Invert
--- | ---
Short description | Set to 1 to invert digital input/output 1
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Digital I/O 1 Invert (08.011) allows the I/O state to be non-inverted(0) or inverted(1) respectively.

If Digital I/O 01 mode (08.031) = 0 (Input) then Digital I/O 1 Invert (08.011) inverts the destination parameter Digital IO1 Source/Destination A (08.021) or DI/O 01 Source/Destination B (08.121).

If Digital I/O 01 mode (08.031) = 1 (Output) then Digital I/O 1 Invert (08.011) inverts Digital I/O 1 State (08.001) and the voltage on the output terminal.

If Digital I/O 01 mode (08.031) = 2 or 3 (Frequency or PWM output) then Digital I/O 1 Invert (08.011) has no effect.

Parameter | 08.012 Digital I/O 2 Invert
--- | ---
Short description | Set to 1 to invert digital input/output 2
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Digital I/O 2 Invert (08.012) allows the input state to be non-inverted(0) or inverted(1) respectively.

Digital I/O 2 Invert (08.012) inverts the destination parameter Digital IO2 Source/Destination A (08.022) or DI/O 02 Source/Destination B (08.122).

Parameter | 08.013 Digital Input 3 Invert
--- | ---
Short description | Set to 1 to invert digital input 3
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Digital Input 3 Invert (08.013) allows the input state to be non-inverted(0) or inverted(1) respectively.

Digital Input 3 Invert (08.013) inverts the destination parameter Digital Input 03 Destination A (08.023) or DI 03 Destination B (08.123).

Parameter | 08.014 Digital Input 4 Invert
--- | ---
Short description | Set to 1 to invert digital input 4
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Digital Input 4 Invert (08.014) allows the input state to be non-inverted(0) or inverted(1) respectively.

Digital Input 4 Invert (08.014) inverts the destination parameter Digital Input 04 Destination A (08.024) or DI 04 Destination B (08.124).

Parameter | 08.015 Digital Input 5 Invert
--- | ---
Short description | Set to 1 to invert digital input 5
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Digital Input 5 Invert (08.015) allows the input state to be non-inverted(0) or inverted(1) respectively.

If Digital input 5 mode (08.035) = 0 then Digital Input 5 Invert (08.015) inverts the destination parameter Digital Input 05 Destination A (08.025) or DI 05 Destination B (08.125).

If Digital input 5 mode (08.035) > 0 then Digital Input 5 Invert (08.015) has no effect.

Parameter | 08.018 Relay 1 Invert
--- | ---
Short description | Set to 1 to invert relay 1
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

A value of 0 or 1 in Relay 1 Invert (08.018) allows the input state to be non-inverted(0) or inverted(1) respectively.

Parameter | 08.020 Digital I/O Read Word
--- | ---
Short description | Displays the states for the digital I/O
Mode | RFC‑A
Minimum | 0 (Display: 000000000000) | Maximum | 2048 (Display: 100000000000)
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Binary | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital I/O Read Word (08.020) reflects the state of DI/O 01 to DI 04, both STO and the relay as given below. Each bit matches the value of the state parameter for the respective digital input or output so the bit value for digital inputs will be the state of the actual input before any inversion or toggle selections are applied. The bit value for digital outputs will include the state inversion if selected in the invert/toggle parameter for the output.

Name | Digital I/O Read Word (08.020) bit
DI/O 01 | 0
DI 02 | 1
DI 03 | 2
DI 04 | 3
DI 05 | 4
Reserved | 5
Reserved | 6
STO 01 | 7
STO 02 | 8
RLY 01 | 9
Reserved | 10

Parameter | 08.021 Digital IO1 Source/Destination A
--- | ---
Short description | Defines the source or destination parameter for digital I/O 1
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 10.003 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

Digital IO1 Source/Destination A (08.021) provides the destination parameter if DI/O 1 is an input and DI1 Control (08.081) = 0.

Digital IO1 Source/Destination A (08.021) provides the source parameter if DI/O 1 is an output and DO1 Control (08.091) = 0.

Parameter | 08.022 Digital IO2 Source/Destination A
--- | ---
Short description | Defines the source or destination parameter for digital I/O 2
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

Digital IO2 Source/Destination A (08.022) provides the destination parameter if DI2 Control (08.082) = 0.

Parameter | 08.023 Digital Input 03 Destination A
--- | ---
Short description | Defines the destination parameter for digital Input 3
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 6.030 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

Digital Input 03 Destination A (08.023) provides the destination parameter if DI3 Control (08.083) = 0.

Parameter | 08.024 Digital Input 04 Destination A
--- | ---
Short description | Defines the destination parameter for digital input 4
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 6.032 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

Digital Input 04 Destination A (08.024) provides the destination parameter if DI4 Control (08.084) = 0.

Parameter | 08.025 Digital Input 05 Destination A
--- | ---
Short description | Defines the destination parameter for digital input 5
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 1.041 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

Digital Input 05 Destination A (08.025) provides the destination parameter if DI5 Control (08.085) = 0.

Parameter | 08.028 Relay 1 Output Source A
--- | ---
Short description | Defines the source parameter for relay 1
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 10.001 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT

Relay 1 Output Source A (08.028) provides the source parameter if Relay 1 Control (08.098) = 0.

Parameter | 08.031 Digital I/O 01 mode
--- | ---
Short description | Defines the mode for the functionality of digital input/output 1
Mode | RFC‑A
Minimum | 0 | Maximum | 3
Default | 1 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text | Description
0 | Input | Digital input
1 | Output | Digital output
2 | Fr | Frequency output
3 | Pulse | PWM output

This parameter selects the function of input/output DI/O 1.

See also Digital I/O 1 State (08.001).

Parameter | 08.035 Digital input 5 mode
--- | ---
Short description | Defines the function for digital input 5
Mode | RFC‑A
Minimum | 0 | Maximum | 4
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text | Description
0 | Input | Input
1 | Th.Sct | Temperature measurement input with short circuit detection (Resistance <50Ohm)
2 | th | Temperature measurement input without short circuit detection but with Th trip
3 | Th.NoTr | Temperature measurement input with no trips
4 | Fr | Frequency Input

This parameter selects the function of input DI 05.

See also Digital Input 5 State (08.005).

The motor thermistor should be connected between terminal 14 and terminal 1 (0 V).

Parameter | 08.039 STO Input 01 State
--- | ---
Short description | Displays the state of safe torque off channel 1
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

STO 01 and STO 02 correspond to two safe torque off channels within the drive.

Both channels must be in the high state for the drive to be enabled. The state parameters are 0 (OFF), if the digital input is low or 1 (ON) if the digital input is high

Parameter | 08.040 STO Input 02 State
--- | ---
Short description | Displays the state of safe torque off channel 2
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | 1ms
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See STO Input 01 State (08.039).

Parameter | 08.041 Keypad Run Button State
--- | ---
Short description | Displays the state for the Keypad Run Forward button
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Digital Input 11 (Keypad Run Button), Digital Input 12 (Keypad Auxiliary Button) and Digital Input 14 (Keypad Stop Button) represent the state of the Run, Auxiliary and Stop buttons on any keypad fitted to the drive; the input state is determined by ORing the state of the button on each keypad connected to the drive, if the button is pressed the state parameter is one otherwise it is zero. If a keypad is not fitted the state parameters are zero.

Digital Input 13 (24V Supply Input) is an external 24V supply input that is monitored and can be used as a 24V digital input if an external 24V supply is not required. The state parameter is low for the voltage range from 0V to 17V and high for the voltage range above 18V. As the input is a power supply it will consume significant current if the level is taken above 24V when the drive is running from its internal power supply, or at any voltage level if this input is the only power supply to the drive. The 24V Input is available on the AI SD card adaptor. The 24V alarm is triggered if 24V Alarm Loss Enable (11.098) = 1 and 24V Supply Input State (08.043) = 0.

Parameter | 08.042 Keypad Auxiliary Button State
--- | ---
Short description | Displays the state for the Keypad Auxilary button
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Keypad Run Button State (08.041).

Parameter | 08.043 24V Supply Input State
--- | ---
Short description | Displays the state for the 24V Supply Input
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Keypad Run Button State (08.041).

Parameter | 08.044 Keypad Stop Button State
--- | ---
Short description | Displays the state for the Keypad Stop button
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Keypad Run Button State (08.041).

Parameter | 08.051 Keypad Run Button Invert/Toggle
--- | ---
Short description | Set to invert/toggle Keypad Run Button
Mode | RFC‑A
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert
2 | Toggle

A value of 0 or 1 allows the input state to be non-inverted or inverted respectively.

An additional toggle function is provided for Keypad Run and Auxiliary button inputs. The toggle function output changes state on each rising edge (0 to 1 change) at its input.

Parameter | 08.052 Keypad Auxiliary Button Invert/Toggle
--- | ---
Short description | Set to invert/toggle Keypad Auxiliary Button
Mode | RFC‑A
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert
2 | Toggle

See Keypad Run Button Invert/Toggle (08.051).

Parameter | 08.053 24V Supply Input Invert
--- | ---
Short description | Set to invert 24V Supply Input
Mode | RFC‑A
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | Not.Inv
1 | Invert

See Keypad Run Button Invert/Toggle (08.051).

Parameter | 08.061 Keypad Run Button Destination
--- | ---
Short description | Defines the destination parameter for digital input 11
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

These destination parameters provide the routing for the Run (DI 11), Auxiliary (DI 12) and 24V Input(DI 13) inputs.

The Auxiliary button is available on the remote KI-Keypad. The 24V Input is available on the AI SD card adaptor.

Parameter | 08.062 Keypad Auxiliary Button Destination
--- | ---
Short description | Defines the destination parameter for digital input 12
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT

See Keypad Run Button Destination (08.061).

Parameter | 08.063 24V Supply Input Destination
--- | ---
Short description | Defines the destination paramter for DI 13
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

See Keypad Run Button Destination (08.061).

Parameter | 08.081 DI1 Control
--- | ---
Short description | Defines the behaviour of digital input 1
Mode | RFC‑A
Minimum | 0 | Maximum | 26
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

Value | Description | DI/O xx Source/Destination B | Other setup
0 | User defined by Digital IO1 Source/Destination A (08.021) to Digital Input 05 Destination A (08.025) | 00.000 |
1 | Multi preset ref selection 1 | 01.045 |
2 | Multi preset ref selection 2 | 01.046 |
3 | Multi preset ref selection 3 | 01.047 |
4 | External stop command | 06.039 |
5 | Acc time selection 1 | 02.032 |
6 | Acc time selection 2 | 02.033 |
7 | Acc time selection 3 | 02.034 |
8 | Speed control and torque control switcher | 04.011 |
9 | External fault N.C. contact input | 10.032 |
10 | External reset | 10.033 |
11 | External jog fwd | 06.031 |
12 | External jog rev | 06.037 |
13 | Drive enable | 06.015 |
14 | Ramp hold | 02.003 |
15 | RUN FWD | 06.030 |
16 | RUN REV | 06.032 |
17 | 3-line run control (Latching) | 06.040 |
18 | Forward limit switch | 06.035 |
19 | Reverse limit switch | 06.036 |
20 | Main ref channel selection 3 | 01.043 |
21 | Main ref channel selection 2 | 01.042 |
22 | Main ref channel selection 3 | 01.041 |
23 | PID1 Enable | 14.008 |
24 | Motor 1/2 switcher | 11.045 |
25 | Motorised pot UP | 09.026 |
26 | Motorised pot DOWN | 09.027 |

This offers a simple control of DI/O 01 Source/Destination B (08.121) to DI 05 Destination B (08.125), to change the digital input destination.If DIx Control (08.08x) is more than 0 then the destination is defined by DI/O 0x Source/Destination (08.12x). DI/O 0x Source/Destination (08.12x) is written by DIx Control (08.08x) selection. (e.g. If DI1 Control (08.081) = 13 then DI/O 01 Source/Destination B (08.121) = 06.015)

If DIx Control (08.08x) is 0 then the destination is defined by DI/O 0x Source/Destination (08.02x).

Parameter | 08.082 DI2 Control
--- | ---
Short description | Defines the behaviour of digital input 2
Mode | RFC‑A
Minimum | 0 | Maximum | 26
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

See DI1 Control (08.081).

Parameter | 08.083 DI3 Control
--- | ---
Short description | Defines the behaviour of digital input 3
Mode | RFC‑A
Minimum | 0 | Maximum | 26
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

See DI1 Control (08.081).

Parameter | 08.084 DI4 Control
--- | ---
Short description | Defines the behaviour of digital input 4
Mode | RFC‑A
Minimum | 0 | Maximum | 26
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

See DI1 Control (08.081).

Parameter | 08.085 DI5 Control
--- | ---
Short description | Defines the behaviour of digital input 5
Mode | RFC‑A
Minimum | 0 | Maximum | 26
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

See DI1 Control (08.081).

Parameter | 08.091 DO1 Control
--- | ---
Short description | Defines the behaviour of digital output 1
Mode | RFC‑A
Minimum | 0 | Maximum | 21
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

Value | Description | DI/O 01 Source/Destination B (08.121) or Relay 01 Source B (08.128)
0 | User defined by Digital IO1 Source/Destination A (08.021) or Relay 1 Output Source A (08.028) | 00.000
1 | Drive running signal (RUN) | 10.002
2 | Frequency arrived signal (FAR) | 10.006 (at frequency)
3 | Reserved | Reserved
4 | Reserved | Reserved
5 | Overload detection signal (OL) | 10.017
6 | Power off state (LU) | 10.016
7 | External fault stop (EXT) | 10.032
8 | Frequency upper limit (FHL) | 10.007
9 | Frequency lower limit (FLL) | 10.004
10 | Drive running at zero frequency | 10.003
11 | Reserved | Reserved
12 | Reserved | Reserved
13 | Reserved | Reserved
14 | Drive (RDY) | 10.090
15 | Drive healthy | 10.001
16 | Reserved | Reserved
17 | Reserved | Reserved
18 | Brake release | 12.040
19 | Torque limiting (Valid while the torque is limited by torque limiting value 1/2) | 10.009
20 | Forward or reverse | 10.014
21 | Motor 1 or 2 | 11.045

This offers a simple control of parameter DI/O 01 Source/Destination B (08.121) or Relay 01 Source B (08.128) to change the source.

If the control parameter (08.09x) is more than 0 then the source is defined by the relevant source parameter B (08.12x). The source parameter is written by the control selection. (e.g. If DO1 Control (08.091) = 10 then DI/O 01 Source/Destination B (08.121) = 10.003)

If the control parameter is 0 then the source is defined by the relevant source parameter A (08.02x).

Parameter | 08.098 Relay 1 Control
--- | ---
Short description | Defines the behaviour of relay 1
Mode | RFC‑A
Minimum | 0 | Maximum | 21
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Action on exit from edit and reset
Display Format | Standard | Decimal Places | 0
Coding | RW

See DO1 Control (08.091).

Parameter | 08.121 DI/O 01 Source/Destination B
--- | ---
Short description | Defines the secondary source or destination parameter for digital input/output 1
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

Refer to control parameters ( DI1 Control (08.081) and DO1 Control (08.091)) for more information.

Parameter | 08.122 DI/O 02 Source/Destination B
--- | ---
Short description | Defines the secondary source or destination parameter for digital input/output 2
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See DI/O 01 Source/Destination B (08.121).

Parameter | 08.123 DI 03 Destination B
--- | ---
Short description | Defines the secondary destination parameter for digital input 3
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See DI/O 01 Source/Destination B (08.121).

Parameter | 08.124 DI 04 Destination B
--- | ---
Short description | Defines the secondary destination parameter for digital input 4
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See DI/O 01 Source/Destination B (08.121).

Parameter | 08.125 DI 05 Destination B
--- | ---
Short description | Defines the secondary destination parameter for digital input 5
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RO, DE, PT

See DI/O 01 Source/Destination B (08.121).

Parameter | 08.128 Relay 01 Source B
--- | ---
Short description | Defines the secondary source parameter for relay 1
Mode | RFC‑A
Minimum | 0.000 | Maximum | 30.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive Reset Read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT

See DO1 Control (08.091).