# Menu 10 Single Line Descriptions − Status and Trips

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
10.001 | Drive Healthy | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.002 | Drive Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.003 | Zero Frequency | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.004 | Running At Or Below Minimum Frequency | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.005 | Below Set Frequency | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.006 | At Frequency | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.007 | Above Set Frequency | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.008 | Rated Load Reached | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.009 | Current Limit Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.010 | Regenerating | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.011 | Braking IGBT Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.012 | Braking Resistor Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.013 | Reverse Direction Commanded | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.014 | Reverse Direction Running | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.015 | Supply Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.016 | Under Voltage Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.017 | Motor Overload Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.018 | Drive Over‑temperature Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.019 | Drive Warning | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.020 | Trip 0 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.021 | Trip 1 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.022 | Trip 2 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.023 | Trip 3 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.024 | Trip 4 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.025 | Trip 5 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.026 | Trip 6 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.027 | Trip 7 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.028 | Trip 8 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.029 | Trip 9 | 0 to 255 |  | RO | Txt | ND | NC | PT | PS
10.030 | Braking Resistor Rated Power | 0.0 to 99999.9 kW | 0.0 kW | RW | Num |  |  |  | US
10.031 | Braking Resistor Thermal Time Constant | 0.00 to 1500.00 s | 0.00 s | RW | Num |  |  |  | US
10.032 | External Trip | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.033 | Drive Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
10.034 | Number Of Auto‑reset Attempts | None (0), 1 (1), 2 (2), 3 (3), 4 (4), 5 (5), Infinite (6) | None (0) | RW | Txt |  |  |  | US
10.035 | Auto‑reset Delay | 1.0 to 600.0 s | 1.0 s | RW | Num |  |  |  | US
10.036 | Auto‑reset Hold Drive Healthy | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.037 | Action On Trip Detection | 00000 to 11111 | 00000 | RW | Bin |  |  |  | US
10.038 | User Trip | 0 to 255 |  | RW | Num | ND | NC |  |
10.039 | Braking Resistor Thermal Accumulator | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
10.040 | Status Word | 000000000000000 to 111111111111111 |  | RO | Bin | ND | NC | PT |
10.041 | Trip 0 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.042 | Trip 0 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.043 | Trip 1 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.044 | Trip 1 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.045 | Trip 2 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.046 | Trip 2 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.047 | Trip 3 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.048 | Trip 3 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.049 | Trip 4 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.050 | Trip 4 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.051 | Trip 5 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.052 | Trip 5 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.053 | Trip 6 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.054 | Trip 6 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.055 | Trip 7 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.056 | Trip 7 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.057 | Trip 8 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.058 | Trip 8 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.059 | Trip 9 Date | 00-00-00 to 31-12-99 |  | RO | Date | ND | NC | PT | PS
10.060 | Trip 9 Time | 00:00:00 to 23:59:59 |  | RO | Time | ND | NC | PT | PS
10.061 | Braking Resistor Resistance | 0.00 to 10000.00 Ω | 0.00 Ω | RW | Num |  |  |  | US
10.064 | Remote Keypad Battery Low | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.065 | Auto‑tune Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.066 | Limit Switch Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.068 | Hold Drive Healthy on Under Voltage | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
10.069 | Additional Status Bits | 00000000000 to 11111111111 |  | RO | Bin | ND | NC | PT |
10.070 | Trip 0 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.071 | Trip 1 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.072 | Trip 2 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.073 | Trip 3 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.074 | Trip 4 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.075 | Trip 5 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.076 | Trip 6 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.077 | Trip 7 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.078 | Trip 8 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.079 | Trip 9 Sub‑trip Number | 0 to 65535 |  | RO | Num | ND | NC | PT | PS
10.080 | Stop Motor | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.081 | Phase Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.090 | Drive Ready | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.101 | Drive Status | Inhibit (0), Ready (1), Stop (2), Scan (3), Run (4), Supply Loss (5), Deceleration (6), dc Injection (7), Reserved (8), Trip (9), Active (10), Heat (14), Under Voltage (15) |  | RO | Txt | ND | NC | PT |
10.102 | Trip Reset Source | 0 to 1023 |  | RO | Num | ND | NC | PT | PS
10.103 | Trip Time Identifier | -2147483648 to 2147483647 ms |  | RO | Num | ND | NC | PT |
10.104 | Active Alarm | None (0), Brake Resistor (1), Motor Overload (2), Reserved (3), Drive Overload (4), Auto Tune (5), Limit Switch (6), Reserved (8), Option Slot 1 (9), Reserved (10), Reserved (11), Reserved (12), Low AC (13), Current limit (14), 24V Backup Lost (15) |  | RO | Txt | ND | NC | PT |
10.106 | Potential Drive Damage Conditions | 00 to 11 |  | RO | Bin | ND | NC | PT | PS
10.107 | Low AC Alarm | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
10.108 | Reversed cooling fan detected | Off (0) or On (1) |  | RO | Bit | ND |  | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |