# Menu 3 Single Line Descriptions − Frequency Monitoring and Speed Feedback

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
03.001 | Final Demand Reference | ±VM_FREQ Hz |  | RO | Num | ND | NC | PT | FI
03.005 | Zero Frequency Threshold | 0.00 to 20.00 Hz | 2.00 Hz | RW | Num |  |  |  | US
03.006 | At Frequency Lower Limit | 0.00 to 550.00 Hz | 1.00 Hz | RW | Num |  |  |  | US
03.007 | At Frequency Upper Limit | 0.00 to 550.00 Hz | 1.00 Hz | RW | Num |  |  |  | US
03.008 | Over Frequency Threshold | 0.00 to 550.00 Hz | 0.00 Hz | RW | Num |  |  |  | US
03.009 | Absolute At Frequency Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
03.022 | Hard Frequency Reference | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
03.023 | Hard Frequency Reference Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
03.029 | Position | 0 to 65535 |  | RO | Num | ND | NC | PT | FI
03.032 | Position Counter Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
03.035 | Position Scaling Numerator | 0.000 to 1.000 | 1.000 | RW | Num |  |  |  | US
03.036 | Position Scaling Denominator | 0.000 to 100.000 | 1.000 | RW | Num |  |  |  | US
03.037 | Frequency Output or PWM Output Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
03.038 | Maximum Output Frequency | 1 (0), 2 (1), 5 (2), 10 (3) kHz | 5 (2) kHz | RW | Txt |  |  |  | US
03.042 | Frequency Input High Precision | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
03.043 | Maximum Reference Frequency | 0.00 to 100.00 kHz | 10.00 kHz | RW | Num |  |  |  | US
03.044 | Frequency Reference Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
03.045 | Frequency Reference | ±100.00 % |  | RO | Num | ND | NC | PT | FI
03.047 | Two Point Minimum Frequency | ±100.00 % | -100.00 % | RW | Num |  |  |  | US
03.048 | Drive Reference at Minimum Frequency | ±100.00 % | -100.00 % | RW | Num |  |  |  | US
03.049 | Two Point Maximum Frequency | 0.00 to 100.00 % | 100.00 % | RW | Num |  |  |  | US
03.050 | Drive Reference at Maximum Frequency | 0.00 to 100.00 % | 100.00 % | RW | Num |  |  |  | US
03.072 | Motor speed percent | ±150.0 % |  | RO | Num | ND | NC | PT | FI
03.127 | Frequency feedback | ±VM_SPEED_FREQ_REF Hz |  | RO | Num | ND | NC | PT |
03.128 | Revolution Counter | 0 to 65535 Revs |  | RO | Num | ND | NC | PT | FI
03.134 | Rotary Lines Per Revolution | 512 (0), 1024 (1), 2048 (2), 4096 (3) | 1024 (1) | RW | Txt |  |  |  | US
03.142 | Encoder feedback filter | 1 to 31 ms | 3 ms | RW | Num |  |  |  | US
03.143 | Maximum Frequency Feedback | ±VM_SPEED_FREQ_REF Hz | 50Hz: 50.00 Hz 60Hz: 60.00 Hz | RW | Num |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |