# Menu 7 Single Line Descriptions − Analog I/O

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
07.001 | Analogue Input 1 | ±100.00 % |  | RO | Num | ND | NC | PT | FI
07.002 | Analogue Input 2 | 0.00 to 100.00 % |  | RO | Num | ND | NC | PT | FI
07.004 | Stack Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.005 | Auxiliary Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.007 | Analogue Input 1 Mode | 4‑20mA Stop (‑6), 20‑4mA Stop (‑5), 4‑20mA Low (‑4), 20‑4mA Low (‑3), 4‑20mA Hold (‑2), 20‑4mA Hold (‑1), 0‑20mA (0), 20‑0mA (1), 4‑20mA Trp (2), 20‑4mA Trp (3), 4‑20mA (4), 20‑4mA (5), Voltage (6) | Voltage (6) | RW | Txt |  |  |  | US
07.008 | Analogue Input 1 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
07.009 | Analogue Input 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
07.010 | Analogue Input 1 Destination A | 0.000 to 30.999 | 1.036 | RW | Num | DE |  | PT | US
07.011 | Analogue Input 2 Mode | 4‑20mA Stop (‑6), 20‑4mA Stop (‑5), 4‑20mA Low (‑4), 20‑4mA Low (‑3), 4‑20mA Hold (‑2), 20‑4mA Hold (‑1), 0‑20mA (0), 20‑0mA (1), 4‑20mA Trp (2), 20‑4mA Trp (3), 4‑20mA (4), 20‑4mA (5), Voltage (6), Digital (7) | Voltage (6) | RW | Txt |  |  |  | US
07.012 | Analogue Input 2 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
07.013 | Analogue Input 2 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
07.014 | Analogue Input 2 Destination A | 0.000 to 30.999 | 1.037 | RW | Num | DE |  | PT | US
07.019 | Analogue Output 1 Source A | 0.000 to 30.999 | 2.001 | RW | Num |  |  | PT | US
07.020 | Analogue Output 1 Scaling | 0.000 to 40.000 | 1.000 | RW | Num |  |  |  | US
07.021 | Analogue Output 1 Mode | Voltage (0), 0‑20mA (1), 4‑20mA (2), Digital (3) | Voltage (0) | RW | Txt |  |  |  | US
07.022 | Analogue Output 2 Source A | 0.000 to 30.999 | 4.002 | RW | Num |  |  | PT | US
07.023 | Analogue Output 2 Scaling | 0.000 to 40.000 | 1.000 | RW | Num |  |  |  | US
07.024 | Analogue Output 2 Mode | Voltage (0), 0‑20mA (1), 4‑20mA (2), Digital (3) | Voltage (0) | RW | Txt |  |  |  | US
07.026 | Analog Input 1 Preset on Current Loss | 4.00 to 20.00 mA | 4.00 mA | RW | Num |  |  |  | US
07.027 | Analog Input 2 Preset on Current Loss | 4.00 to 20.00 mA | 4.00 mA | RW | Num |  |  |  | US
07.028 | Analogue Input 1 Current Loop Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
07.029 | Analogue Input 2 Current Loop Loss | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
07.030 | Analogue Input 1 Offset | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.031 | Analogue Input 2 Offset | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.034 | Inverter Temperature | ±250 °C |  | RO | Num | ND | NC | PT |
07.035 | Percentage Of d.c. Link Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.036 | Percentage Of Drive Thermal Trip Level | 0 to 100 % |  | RO | Num | ND | NC | PT |
07.037 | Temperature Nearest To Trip Level | 0 to 29999 |  | RO | Num | ND | NC | PT |
07.046 | Thermistor Type | DIN44081 (0), KTY84 (1), PT1000 (2), PT2000 (3), Other (4) | DIN44081 (0) | RW | Txt |  |  |  | US
07.047 | Thermistor Feedback | 0 to 4000 Ω |  | RO | Num | ND | NC | PT | FI
07.048 | Thermistor Trip Threshold | 0 to 4000 Ω | 3300 Ω | RW | Num |  |  |  | US
07.049 | Thermistor Reset Threshold | 0 to 4000 Ω | 1800 Ω | RW | Num |  |  |  | US
07.050 | Thermistor Temperature | -50 to 300 °C |  | RO | Num | ND | NC | PT | FI
07.051 | Analogue Input 1 Control | 0 to 5 | 0 | RW | Num |  |  |  | US
07.052 | Analogue Input 2 Control | 0 to 5 | 0 | RW | Num |  |  |  | US
07.055 | Analogue Output 1 Control | 0 to 15 | 0 | RW | Num |  |  |  | US
07.056 | Analogue Output 2 Control | 0 to 15 | 0 | RW | Num |  |  |  | US
07.061 | Analogue Input 1 Minimum Reference | ±100.00 % | -100.00 % | RW | Num |  |  |  | US
07.062 | Analogue Input 1 At Minimum Reference | ±100.00 % | -100.00 % | RW | Num |  |  |  | US
07.063 | Analogue Input 1 Maximum Reference | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.064 | Analogue Input 1 At Maximum Reference | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.065 | Analogue Input 2 Minimum Reference | 0.00 to 100.00 % | 0.00 % | RW | Num |  |  |  | US
07.066 | Analogue Input 2 At Minimum Reference | ±100.00 % | 0.00 % | RW | Num |  |  |  | US
07.067 | Analogue Input 2 Maximum Reference | 0.00 to 100.00 % | 100.00 % | RW | Num |  |  |  | US
07.068 | Analogue Input 2 At Maximum Reference | ±100.00 % | 100.00 % | RW | Num |  |  |  | US
07.090 | Analogue Input 1 Destination B | 0.000 to 30.999 | 0.000 | RO | Num | DE |  | PT | US
07.094 | Analogue Input 2 Destination B | 0.000 to 30.999 | 0.000 | RO | Num | DE |  | PT | US
07.099 | Analogue Output 1 Source B | 0.000 to 30.999 | 0.000 | RO | Num |  |  | PT | US
07.102 | Analogue Output 2 Source B | 0.000 to 30.999 | 0.000 | RO | Num |  |  | PT | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |