# Menu 19 Single Line Descriptions − Application Menu 2

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
19.001 | Application Menu 2 Power‑down Save Integer | -32768 to 32767 | 0 | RW | Num |  |  |  | PS
19.002 | Application Menu 2 Read‑only Integer 2 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.003 | Application Menu 2 Read‑only Integer 3 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.004 | Application Menu 2 Read‑only Integer 4 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.005 | Application Menu 2 Read‑only Integer 5 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.006 | Application Menu 2 Read‑only Integer 6 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.007 | Application Menu 2 Read‑only Integer 7 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.008 | Application Menu 2 Read‑only Integer 8 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.009 | Application Menu 2 Read‑only Integer 9 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.010 | Application Menu 2 Read‑only Integer 10 | -32768 to 32767 |  | RO | Num | ND | NC |  |
19.011 | Application Menu 2 Read‑write Integer 11 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.012 | Application Menu 2 Read‑write Integer 12 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.013 | Application Menu 2 Read‑write Integer 13 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.014 | Application Menu 2 Read‑write Integer 14 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.015 | Application Menu 2 Read‑write Integer 15 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.016 | Application Menu 2 Read‑write Integer 16 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.017 | Application Menu 2 Read‑write Integer 17 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.018 | Application Menu 2 Read‑write Integer 18 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.019 | Application Menu 2 Read‑write Integer 19 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.020 | Application Menu 2 Read‑write Integer 20 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.021 | Application Menu 2 Read‑write Integer 21 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.022 | Application Menu 2 Read‑write Integer 22 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.023 | Application Menu 2 Read‑write Integer 23 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.024 | Application Menu 2 Read‑write Integer 24 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.025 | Application Menu 2 Read‑write Integer 25 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.026 | Application Menu 2 Read‑write Integer 26 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.027 | Application Menu 2 Read‑write Integer 27 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.028 | Application Menu 2 Read‑write Integer 28 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.029 | Application Menu 2 Read‑write Integer 29 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.030 | Application Menu 2 Read‑write Integer 30 | -32768 to 32767 | 0 | RW | Num |  |  |  | US
19.031 | Application Menu 2 Read‑write bit 31 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.032 | Application Menu 2 Read‑write bit 32 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.033 | Application Menu 2 Read‑write bit 33 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.034 | Application Menu 2 Read‑write bit 34 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.035 | Application Menu 2 Read‑write bit 35 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.036 | Application Menu 2 Read‑write bit 36 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.037 | Application Menu 2 Read‑write bit 37 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.038 | Application Menu 2 Read‑write bit 38 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.039 | Application Menu 2 Read‑write bit 39 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.040 | Application Menu 2 Read‑write bit 40 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.041 | Application Menu 2 Read‑write bit 41 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.042 | Application Menu 2 Read‑write bit 42 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.043 | Application Menu 2 Read‑write bit 43 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.044 | Application Menu 2 Read‑write bit 44 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.045 | Application Menu 2 Read‑write bit 45 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.046 | Application Menu 2 Read‑write bit 46 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.047 | Application Menu 2 Read‑write bit 47 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.048 | Application Menu 2 Read‑write bit 48 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.049 | Application Menu 2 Read‑write bit 49 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.050 | Application Menu 2 Read‑write bit 50 | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
19.051 | Application Menu 2 Power‑down Save Long Integer 51 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  | PS
19.052 | Application Menu 2 Power‑down Save Long Integer 52 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  | PS
19.053 | Application Menu 2 Power‑down Save Long Integer 53 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  | PS
19.054 | Application Menu 2 Power‑down Save Long Integer 54 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  | PS

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |