# Menu 9 Single Line Descriptions − User Functions 1

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
09.001 | Logic Function 1 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.002 | Logic Function 2 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.003 | Motorised Pot Output | ±100.00 % |  | RO | Num | ND | NC | PT | PS
09.004 | Logic Function 1 Source 1 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.005 | Logic Function 1 Source 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.006 | Logic Function 1 Source 2 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.007 | Logic Function 1 Source 2 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.008 | Logic Function 1 Output Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.009 | Logic Function 1 Delay | ±25.0 s | 0.0 s | RW | Num |  |  |  | US
09.010 | Logic Function 1 Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.014 | Logic Function 2 Source 1 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.015 | Logic Function 2 Source 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.016 | Logic Function 2 Source 2 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.017 | Logic Function 2 Source 2 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.018 | Logic Function 2 Output Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.019 | Logic Function 2 Delay | ±25.0 s | 0.0 s | RW | Num |  |  |  | US
09.020 | Logic Function 2 Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.021 | Motorised Pot Mode | 0 to 4 | 0 | RW | Num |  |  |  | US
09.022 | Motorised Pot Bipolar Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.023 | Motorised Pot Rate | 0 to 250 s | 20 s | RW | Num |  |  |  | US
09.024 | Motorised Pot Scaling | 0.000 to 4.000 | 1.000 | RW | Num |  |  |  | US
09.025 | Motorised Pot Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.026 | Motorised Pot Up | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.027 | Motorised Pot Down | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.028 | Motorised Pot Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.029 | Binary Sum Ones | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.030 | Binary Sum Twos | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.031 | Binary Sum Fours | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.032 | Binary Sum Output | 0 to 255 |  | RO | Num | ND | NC | PT |
09.033 | Binary Sum Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.034 | Binary Sum Offset | 0 to 248 | 0 | RW | Num |  |  |  | US
09.035 | Timer 1 Start Date | 00-00-00 to 31-12-99 | 00-00-00 | RW | Date |  |  |  | US
09.036 | Timer 1 Start Time | 00:00:00 to 23:59:59 | 00:00:00 | RW | Time |  |  |  | US
09.037 | Timer 1 Stop Date | 00-00-00 to 31-12-99 | 00-00-00 | RW | Date |  |  |  | US
09.038 | Timer 1 Stop Time | 00:00:00 to 23:59:59 | 00:00:00 | RW | Time |  |  |  | US
09.039 | Timer 1 Repeat Function | None (0), Hour (1), Day (2), Week (3), Month (4), Year (5), One off (6), Minute (7) | None (0) | RW | Txt |  |  |  | US
09.040 | Timer 1 Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.041 | Timer 1 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.042 | Timer 1 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.043 | Timer 1 Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.045 | Timer 2 Start Date | 00-00-00 to 31-12-99 | 00-00-00 | RW | Date |  |  |  | US
09.046 | Timer 2 Start Time | 00:00:00 to 23:59:59 | 00:00:00 | RW | Time |  |  |  | US
09.047 | Timer 2 Stop Date | 00-00-00 to 31-12-99 | 00-00-00 | RW | Date |  |  |  | US
09.048 | Timer 2 Stop Time | 00:00:00 to 23:59:59 | 00:00:00 | RW | Time |  |  |  | US
09.049 | Timer 2 Repeat Function | None (0), Hour (1), Day (2), Week (3), Month (4), Year (5), One off (6), Minute (7) | None (0) | RW | Txt |  |  |  | US
09.050 | Timer 2 Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.051 | Timer 2 Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.052 | Timer 2 Output | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.053 | Timer 2 Destination | 0.000 to 59.999 | 0.000 | RW | Num | DE |  | PT | US
09.055 | Scope Trace 1 Source | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.056 | Scope Trace 2 Source | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.057 | Scope Trace 3 Source | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.058 | Scope Trace 4 Source | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.059 | Scope Trigger | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
09.060 | Scope Trigger Source | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
09.061 | Scope Trigger Threshold | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  | US
09.062 | Scope Trigger Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
09.063 | Scope Mode | Single (0), Normal (1), Auto (2) | Single (0) | RW | Txt |  |  |  | US
09.064 | Scope Arm | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
09.065 | Scope Data Not Ready | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.066 | Scope Saving Data | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
09.067 | Scope Sample Time | 1 to 200 | 1 | RW | Num |  |  |  | US
09.068 | Scope Trigger Delay | 0 to 100 % | 0 % | RW | Num |  |  |  | US
09.069 | Scope Time Period | 0.00 to 200000.00 ms |  | RO | Num | ND | NC | PT |
09.070 | Scope Auto‑save Mode | Disabled (0), Overwrite (1), Keep (2) | Disabled (0) | RW | Txt |  |  |  | US
09.071 | Scope Auto‑save File Number | 0 to 99 | 0 | RO | Num |  |  |  | PS
09.072 | Scope Auto‑save Reset | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
09.073 | Scope Auto‑save Status | Disabled (0), Active (1), Stopped (2), Failed (3) | Disabled (0) | RO | Txt |  |  |  | PS

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |