# Trips

Mode: Regeneration

Trip 0 (10.020) to Trip 9 (10.029) store the most recent 10 trips that have occurred where Trip 0 (10.020) is the most recent and Trip 9 (10.029) is the oldest. When a new trip occurs it is written to Trip 0 (10.020) and all the other trips move down the log, with oldest being lost. The date and time when each trip occurs are also stored in the date and time log, i.e. Trip 0 Date (10.041) to Trip 9 Time (10.060). The date and time are taken from Date (06.016) and Time (06.017). Some trips have sub-trip numbers which give more detail about the reason for the trip. If a trip has a sub-trip number its value is stored in the sub-trip log, i.e. Trip 0 Sub-trip Number (10.070) to Trip 9 Sub-trip Number (10.079). If the trip does not have a sub-trip number then zero is stored in the sub-trip log.

Trip categories and priorities
Trips are grouped into the categories given in the table below. A trip can only occur when the drive is not tripped, or if it is already tripped and the new trip has a higher priority than the active trip (i.e. lower priority number). Unless otherwise stated a trip cannot be reset until 1.0s after it has been initiated.

Priority | Category | Trips | Comments
1 | Internal faults | HF01 – HF20 | These are fatal problems that cannot be reset. All drive features are inactive after any of these trips occur. If a basic keypad is fitted it will show the trip, but the keypad will not function. These trips are not stored in the trip log.
1 | Stored HF trip | Stored HF | This trip cannot be cleared unless 1299 is entered into Parameter mm.000 (mm.000) and a reset is initiated.
2 | Non-resettable trips | Trip numbers 218 to 247, Slot1 HF, Slot2 HF, Slot3 HF or Slot4 HF | These trips cannot be reset.
3 | Volatile memory failure | EEPROM Fail | This can only be reset if Parameter mm.000 (mm.000) is set to 1233 or 1244, or if Load Defaults (11.043) is set to a non-zero value.
4 | Internal 24V power supply | PSU 24V |
5 | Non-volatile media trips | Trip numbers 174, 175 and 177 to 188 | These trips are priority 6 during power-up.
5 | Position feedback interface power supply | Encoder 1 | This trip can override Encoder 2 to Encoder 6 trips.
6 | Trips with extended reset times | OI ac, OI Brake, and OI dc | These trips cannot be reset until 10s after the trip was initiated.
6 | Phase loss and d.c. link power circuit protection | Phase Loss and OHt dc bus | The drive will attempt to stop the motor before tripping if a Phase Loss.000 trip occurs unless this feature has been disabled (see Action On Trip Detection (10.037). The drive will always attempt to stop the motor before tripping if an OHt dc bus occurs.
6 | Standard trips | All other trips |

Internal faults
Trips {HF01} to {HF20} are internal faults that do not have trip numbers. If one of these trips occurs, the main drive processor has detected an irrecoverable error. All drive functions are stopped and the trip message will be displayed on the drive keypad. The error can only be reset by powering the drive down and up again. The table below gives the reasons for internal faults and their corresponding trip.

Trip | Reason
{HF01} | CPU has detected an address error
{HF02} | CPU DMAC has detected an address error
{HF03} | CPU has detected an Illegal opcode
{HF04} | CPU has detected an Illegal slot instruction
{HF05} | An interrupt has occurred that does not have a defined function (Undefined exception)
{HF06} | An interrupt has occurred which is reserved (Reserved exception)
{HF07} | Watchdog failure
{HF08} | CPU Interrupt crash
{HF09} | Free store overflow
{HF10} | Parameter routing system error
{HF11} | Non-volatile memory comms error
{HF12} | Stack overflow. Sub-trip is shown to indicate which stack: 1 – background tasks 2 – timed tasks 3 – main system interrupts
{HF13} | The control hardware is not compatible with the firmware. The sub-trip number gives the actual ID code of the control board hardware.
{HF14} | CPU register bank error
{HF15} | CPU divide error
{HF16} | RTOS error (the background task has returned)
{HF17} | The clock supplied to the control board logic is out of specification
{HF18} | The internal flash memory has failed when writing option module parameter data. Sub-trip is shown to indicate which failure: 1 - Programming error while writing menu in flash 2 - Erase flash block containing setup menus failed 3 - Erase flash block containing application menus failed
{HF19} | Invalid main application firmware CRC. Reprogramming required.
{HF20} | The ASIC is not compatible with the firmware. The sub-trip number displayed is the ASIC version.
{HF23} | If this trip occurs please consult the drive supplier.
{HF24} | If this trip occurs please consult the drive supplier.
{HF25} | If this trip occurs please consult the drive supplier.

When the drive is subsequently powered up a Stored HF trip is initiated where the sub-trip number is the number of the HF trip that last occurred. This trip will occur at every power-up until it is reset. The trip can only be reset by first entering 1299 into Parameter mm.000 (mm.000). If the drive is powered up and a Stored HF trip occurs, Onboard User Program: Enable (11.047) is reset to zero to prevent the on-board user program from running. This ensures that the user program can be changed or erased in case it causes an HF trip at every power-up. Once the Stored HF is cleared, it is necessary to power cycle the drive or to re-download the user program to allow the program to restart.

Similar trips that can be initiated by the control system or the power system
Trips shown in the table below can be generated either from the drive control system or from the power system. The sub-trip number which is in the form xxyzz is used to identify the source of the trip. The digits xx are 00 for a trip generated by the control system or the number of a power module if generated by the power system. If the drive is not a multi-power module drive then xx will always have a value of 1 the trip is related to the power system. The y digit is used to identify the location of a trip which is generated by a rectifier module connected to a power module. Where the y digit is relevant it will have a value of 1 or more, otherwise it will be 0. The zz digits give the reason for the trip and are defined in each trip description.

Over Volts | OHt dc bus
OI ac | Phase Loss
OI Brake | Power Comms
PSU | OI Snubber
OHt Inverter | Reserved 102
OHt Power | Temp Feedback
OHt Control | Power Data

Braking IGBT
The list below gives conditions that will disable the braking IGBT:

1. Braking IGBT Upper Threshold (06.074) = 0, or Low Voltage Braking IGBT Threshold Select (06.076) = 1 and Low Voltage Braking IGBT Threshold (06.075) = 0.
2. The drive is in the under-voltage state.
3. A priority 1, 2 or 3 trip is active (see Trip 0 (10.020)).
4. One of the following trips is active or would be active if another trip is not already active: OI Brake, PSU, Th Brake Res or OHt Inverter.
5. Percentage Of Drive Thermal Trip Level (07.036) = 100%. This is an indication that some part of the drive is too hot and is used to indicate if an internally fitted braking resistor is too hot.
6. Brake R Too Hot is active or the system has been set up to disable the braking IGBT based on the braking resistor temperature and the resistor is too hot (i.e. bit 2 of Action On Trip Detection (10.037) is set).

Trips Summary (numerical order)

Value | Trip
--- | ---
0 | None
1 | Reserved 001
2 | Over Volts
3 | OI ac
4 | OI Brake
5 | PSU
6 | External Trip
7 | Over Speed
8 | Inductance
9 | PSU 24V
10 | Th Brake Res
11 | Autotune 1
12 | Autotune 2
13 | Autotune 3
14 | Autotune 4
15 | Autotune 5
16 | Autotune 6
17 | Autotune 7
18 | Autotune Stopped
19 | Brake R Too Hot
20 | Motor Too Hot
21 | OHt Inverter
22 | OHt Power
23 | OHt Control
24 | Thermistor
25 | Th Short Circuit
26 | I/O Overload
27 | OHt dc bus
28 | An Input 1 Loss
29 | An Input 2 Loss
30 | Watchdog
31 | EEPROM Fail
32 | Phase Loss
33 | Resistance
34 | Keypad Mode
35 | Control Word
36 | User Save
37 | Power Down Save
38 | Low Load
39 | Line Sync
40 | User Trip 40
41 | User Trip 41
42 | User Trip 42
43 | User Trip 43
44 | User Trip 44
45 | User Trip 45
46 | User Trip 46
47 | User Trip 47
48 | User Trip 48
49 | User Trip 49
50 | User Trip 50
51 | User Trip 51
52 | User Trip 52
53 | User Trip 53
54 | User Trip 54
55 | User Trip 55
56 | User Trip 56
57 | User Trip 57
58 | User Trip 58
59 | User Trip 59
60 | User Trip 60
61 | User Trip 61
62 | User Trip 62
63 | User Trip 63
64 | User Trip 64
65 | User Trip 65
66 | User Trip 66
67 | User Trip 67
68 | User Trip 68
69 | User Trip 69
70 | User Trip 70
71 | User Trip 71
72 | User Trip 72
73 | User Trip 73
74 | User Trip 74
75 | User Trip 75
76 | User Trip 76
77 | User Trip 77
78 | User Trip 78
79 | User Trip 79
80 | User Trip 80
81 | User Trip 81
82 | User Trip 82
83 | User Trip 83
84 | User Trip 84
85 | User Trip 85
86 | User Trip 86
87 | User Trip 87
88 | User Trip 88
89 | User Trip 89
90 | Power Comms
91 | User 24V
92 | OI Snubber
93 | Inductor Too Hot
94 | Rectifier Set-up
95 | Reserved 095
96 | User Prog Trip
97 | Data Changing
98 | Out Phase Loss
99 | CAM
100 | Reset
101 | OHt Brake
102 | Reserved 102
103 | Inter-connect
104 | Reserved 104
105 | Reserved 105
106 | Reserved 106
107 | Reserved 107
108 | Reserved 108
109 | OI dc
110 | Undefined
111 | Configuration
112 | User Trip 112
113 | User Trip 113
114 | User Trip 114
115 | User Trip 115
116 | User Trip 116
117 | User Trip 117
118 | User Trip 118
119 | User Trip 119
120 | User Trip 120
121 | User Trip 121
122 | User Trip 122
123 | User Trip 123
124 | User Trip 124
125 | User Trip 125
126 | User Trip 126
127 | User Trip 127
128 | User Trip 128
129 | User Trip 129
130 | User Trip 130
131 | User Trip 131
132 | User Trip 132
133 | User Trip 133
134 | User Trip 134
135 | User Trip 135
136 | User Trip 136
137 | User Trip 137
138 | User Trip 138
139 | User Trip 139
140 | User Trip 140
141 | User Trip 141
142 | User Trip 142
143 | User Trip 143
144 | User Trip 144
145 | User Trip 145
146 | User Trip 146
147 | User Trip 147
148 | User Trip 148
149 | User Trip 149
150 | User Trip 150
151 | User Trip 151
152 | User Trip 152
153 | User Trip 153
154 | User Trip 154
155 | User Trip 155
156 | User Trip 156
157 | User Trip 157
158 | User Trip 158
159 | User Trip 159
160 | Island
161 | Reserved 161
162 | Encoder 12
163 | Encoder 13
164 | Reserved 164
165 | Reserved 165
166 | Reserved 166
167 | Reserved 167
168 | Reserved 168
169 | Voltage Range
171 | Reserved 171
172 | Reserved 172
173 | Reserved 173
174 | Card Slot
175 | Card Product
176 | Name Plate
177 | Card Boot
178 | Card Busy
179 | Card Data Exists
180 | Card Option
181 | Card Read Only
182 | Card Error
183 | Card No Data
184 | Card Full
185 | Card Access
186 | Card Rating
187 | Card Drive Mode
188 | Card Compare
189 | Encoder 1
190 | Encoder 2
191 | Encoder 3
192 | Encoder 4
193 | Encoder 5
194 | Encoder 6
195 | Encoder 7
196 | Encoder 8
197 | Encoder 9
198 | Phasing Error
199 | Destination
200 | Slot1 HF
201 | Slot1 Watchdog
202 | Slot1 Error
203 | Slot1 Not Fitted
204 | Slot1 Different
205 | Slot2 HF
206 | Slot2 Watchdog
207 | Slot2 Error
208 | Slot2 Not Fitted
209 | Slot2 Different
210 | Slot3 HF
211 | Slot3 Watchdog
212 | Slot3 Error
213 | Slot3 Not Fitted
214 | Slot3 Different
215 | Option Disable
216 | Slot App Menu
217 | App Menu Changed
218 | Temp Feedback
219 | An Output Calib
220 | Power Data
221 | Stored HF
222 | Reserved 222
223 | Rating Mismatch
224 | Drive Size
225 | Current Offset
226 | Soft Start
227 | Sub-array RAM
228 | Reserved 228
229 | Reserved 229
230 | Reserved 230
231 | Reserved 231
232 | Reserved 232
233 | Reserved 233
234 | Reserved 234
235 | Reserved 235
236 | Reserved 236
237 | Reserved 237
238 | Reserved 238
239 | Reserved 239
240 | Reserved 240
241 | Reserved 241
242 | Reserved 242
243 | Reserved 243
244 | Reserved 244
245 | Reserved 245
246 | Reserved 246
247 | Derivative ID
248 | Derivative Image
249 | User Program
250 | Slot4 HF
251 | Slot4 Watchdog
252 | Slot4 Error
253 | Slot4 Not Fitted
254 | Slot4 Different
255 | Reset Logs

Trips (alphabetical order)

Trip | An Input 1 Loss
--- | ---
Value | 28
Short description |

Indicates that a current loss was detected in current mode on Analog Input 1 (Terminal 5, 6). In 4-20mA and 20-4mA modes. loss of input is detected if the current falls below 3mA. See Analog Input 1 Mode (07.007) for further details.

Recommended actions:

- Check control wiring is correct.
- Check control wiring is undamaged.
- Check Analog Input 1 Mode (07.007).
- Check that the current signal is present and greater than 3mA.

Trip | An Input 2 Loss
--- | ---
Value | 29
Short description |

Indicates that a current loss was detected in current mode on Analog Input 2 (Terminal 7). In 4-20mA and 20-4mA modes. loss of input is detected if the current falls below 3mA. See Analog Input 2 Mode (07.011) for further details.

Recommended actions:

- Check control wiring is correct.
- Check control wiring is undamaged.
- Check Analog Input 2 Mode (07.011).
- Check that the current signal is present and greater than 3mA.

Trip | An Output Calib
--- | ---
Value | 219
Short description |

The zero offset calibration of one or both of the analogue outputs has failed. This indicates that the drive hardware has failed or a voltage has been applied to the output via a low impedance.

Sub-trip | Reason
1 | Output 1 failed
2 | Output 2 failed

Recommended actions:

- Check the wiring associated with analog outputs.
- Remove all the wiring that is connected to analog outputs and perform the calibration.
- If trip persists, replace the drive.

Trip | App Menu Changed
--- | ---
Value | 217
Short description |

The customisation table for an application menu has been changed. The sub-trip indicates which menu has changed:

Sub-trip | Reason
1 | Menu 18
2 | Menu 19
3 | Menu 20

If more than one menu has changed the lowest menu has priority. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Reset the trip and perform a parameter save to accept the new settings.

Trip | Autotune 1
--- | ---
Value | 11
Short description |

The drive has tripped during an auto-tune. The cause of the trip can be identified from the sub-trip number.

Sub-trip | Reason | Recommended actions
1 | The position feedback did not change when position feedback is being used during rotating auto-tune. | Ensure that the motor is free to turn (i.e. mechanical brake is released). Check that the position feedback is selected correctly and operates correctly.
2 | The motor did not reach the required speed during mechanical load measurement. | Ensure that the motor is free to turn and that the static load plus inertia is not too large for the drive to accelerate within the test time.
3 | The required commutation signal edge could not be found during a rotating auto-tune with a Commutation Only position feedback device. | Check that the position feedback signals are connected correctly.
4 | The required movement angle cannot be produced during a minimal movement test. | Reduce the angular movement required.
5 | The second part of the minimal movement test during auto-tuning cannot locate the motor flux position accurately. | Reduce the angular movement required.
6 | The phasing offset angle is measured twice during a stationary auto-tune and the results are not within 30o of each other. | If a minimal movement test is being used and excessive motor movement is occurring during the test reduce the required angle movement. Otherwise try and increase the required angle movement.
7 | The motor is moving when a phasing test on enable is selected and the drive is enabled, but the motor is still moving at a speed above the zero speed threshold. | Ensure that the motor is stationary before the drive is enabled.
8 | An auto-tune has been attemped while the AMC is selected. | Set AMC Select (31.001) to zero to deselect the AMC.

Trip | Autotune 2
--- | ---
Value | 12
Short description |

The drive has tripped during a rotating auto-tune. The cause of the trip can be identified from the associated sub-trip number.

Sub-trip | Reason
1 | The position feedback direction is incorrect when position feedback is being used during a rotating auto-tune.
2 | A SINCOS encoder with comms is being used for position feedback and the comms position is rotating in the opposite direction to the sine wave based position.

Recommeded actions:

- Check motor cable wiring is correct.
- Check feedback device wiring is correct.
- Swap any two motor phases.

Trip | Autotune 3
--- | ---
Value | 13
Short description |

The drive has tripped during a rotating auto-tune or mechanical load measurement. The cause of the trip can be identified from the associated sub-trip number.

Sub-trip | Reason
1 | Measured inertia has exceeded the parameter range during a mechanical load measurement.
2 | The commutation signals changed in the wrong direction during a rotating auto-tune.
3 | The mechanical load test has been unable to identify the motor inertia.

Recommended actions for sub-trip 2:

- Check motor cable wiring is correct.
- Check feedback device U, V and W commutation signal wiring is correct.

Recommended actions for sub-trip 3:

- Increase the test level.
- If the test was carried out at standstill repeat the test with the motor rotating within the recommended speed range.

Trip | Autotune 4
--- | ---
Value | 14
Short description |

A position feedback device with commutation signals is being used (i.e AB Servo, FD Servo, FR Servo, SC Servo or Commutation Only encoder) and the U commutation signal did not change during a rotating auto-tune.

Recommended actions:

- Check feedback device U commutation signal wiring is correct (Encoder terminals 7 and 8).

Trip | Autotune 5
--- | ---
Value | 15
Short description |

A position feedback device with commutation signals is being used (i.e AB Servo, FD Servo, FR Servo, SC Servo or Commutation Only encoder) and the V commutation signal did not change during a rotating auto-tune.

Recommended actions:

- Check feedback device V commutation signal wiring is correct (Encoder terminals 9 and 10).

Trip | Autotune 6
--- | ---
Value | 16
Short description |

A position feedback device with commutation signals is being used (i.e AB Servo, FD Servo, FR Servo, SC Servo or Commutation Only encoder) and the W commutation signal did not change during a rotating auto-tune.

Recommended actions:

- Check feedback device W commutation signal wiring is correct (Encoder terminals 11 and 12).

Trip | Autotune 7
--- | ---
Value | 17
Short description |

An Autotune 7 trip is initiated during a rotating auto-tune, if the number of motor poles or the position feedback resolution have been set up incorrectly where position feedback is being used.

Recommeded actions:

- Check the lines per revolution for the feedback device.
- Check the number of poles in Number Of Motor Poles (05.011).

Trip | Autotune Stopped
--- | ---
Value | 18
Short description |

The drive was prevented from completing an auto-tune, because either the Final drive enable or the Final drive run were removed.

Recommended actions:

- Check the drive enable signal (Terminal 31) was active during the auto-tune.
- Check the run command was active in Digital Input 05 State (08.005) during the auto-tune.

Trip | Brake R Too Hot
--- | ---
Value | 19
Short description |

This trip indicates that braking resistor overload has timed out. The value in Braking Resistor Thermal Accumulator (10.039) is calculated using Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061). This trip is initiated when Braking Resistor Thermal Accumulator (10.039) reaches 100%.

Recommended actions:

- Ensure the values entered in Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061) are correct.
- If an external thermal protection device is being used and the braking resistor software overload protection is not required, set Braking Resistor Rated Power (10.030), Braking Resistor Thermal Time Constant (10.031) and Braking Resistor Resistance (10.061) to 0 to disable the trip.

Trip | CAM
--- | ---
Value | 99
Short description |

Advanced motion controller cam failure.

Sub-trip | Reason
1 | AMC Cam Start Index (35.001) > AMC Cam Size (35.003) or AMC Cam Start Position In Segment (35.002) > Cam Table In for the start index
2 | AMC Cam Index (35.007) has change by more than 2 in one sample
3 | The rate of change at a segment boundary has exceeded the maximum value
4 | The sum of the AMC Cam Position In Segment (35.008) and the change of master position has exceeded the maximum value

Trip | Card Access
--- | ---
Value | 185
Short description |

A communications failure has occurred with a NV media card. If this occurs during a data transfer to the card then the file being written may be corrupted. If this occurs when data is being transferred from the card then the data transfer may be incomplete. If a parameter file is transferred to the drive and this trip occurs during the transfer the parameters are not saved to non-volatile memory, and so the original parameters can be restored by powering the drive down and up again.

Recommended actions:

- Check the NV media card is installed / located correctly.
- Replace the NV media card.

Trip | Card Boot
--- | ---
Value | 177
Short description |

A write to a Menu 0 parameter has been initiated via the keypad by exiting edit mode and Parameter Cloning (11.042) is set up for auto or boot mode, but the necessary boot file has not been created on the NV media card fitted to the drive to take the new parameter value. This occurs when Parameter Cloning (11.042) is changed to auto or boot mode, but the drive is not subsequently reset. The action of resetting the trip will create the necessary file and prevent further trips.

Recommended actions:

- Ensure that Parameter Cloning (11.042) is correctly set, and then reset the drive to create the necessary file on the NV media card.
- Re-attempt the parameter write to the Menu 0 parameter.

Trip | Card Busy
--- | ---
Value | 178
Short description |

An attempt has been made to access a file on a NV media card, but the file is already being accessed be an Option Module, such as one of the Applications modules. No data is transferred.

Recommended actions:

- Wait for the Option Module to finish accessing the NV media card and re-attempt the required function.

Trip | Card Compare
--- | ---
Value | 188
Short description |

A compare has been carried out between a file on a NV media card and the drive and these are different and no other NV media card related trips have occurred.

Recommended actions:

- Set Pr mm.000 to 0 to reset the trip.
- Check to ensure the correct data block on the NV media card has been used for the compare.

Trip | Card Data Exists
--- | ---
Value | 179
Short description |

An attempt has been made to store data on a NV media card, but the file already exists. No data is transferred. The file should be erased first to prevent this trip.

Recommended actions:

- Erase the data in data location.
- Write data to an alternative data location.

Trip | Card Drive Mode
--- | ---
Value | 187
Short description |

This trip is produced during a compare if the drive mode in the file on the NV media card is different from the current drive mode and the file is a parameter file. This trip is also produced if an attempt is made to transfer a parameter file where the source and target drive modes are different and the drive mode is outside the range allowed for the target drive.

Recommended actions:

- Ensure the destination drive supports the drive operating mode in the parameter file.
- Clear the value in Pr mm.000 and reset the drive.
- Ensure destination derive operating mode is the same as the source parameter file.

Trip | Card Error
--- | ---
Value | 182
Short description |

An attempt has been made to access a NV media card, but an error has been detected in the data structure on the card. Resetting this trip will cause the drive to erase the <MCDF> folder from the NV media card (if it exists) and create the correct folder structure. On an SD card, whilst this trip is still present, missing directories will be created, and if the header file is missing it will be created. The following sub-trip numbers are used with this trip.

Sub-trip | Reason
1 | The required folder and file structure is not present.
2 | The <000> file is corrupted.
3 | Two or more files in the <MCDF\> folder have the same file identification number.

Recommended actions:

- Erase all the data blocks and re-attempt the process.
- Ensure the card is located correctly.
- Replace the NV media card.

Trip | Card Full
--- | ---
Value | 184
Short description |

An attempt has been made to write to a NV media card, but there is insufficient space available. No data is transferred.

Recommended actions:

- Delete a data block or the entire NV media card to create space.
- Replace the NV media card.

Trip | Card No Data
--- | ---
Value | 183
Short description |

An attempt has been made to access a non-existent file on a NV media card. No data is transferred.

Recommended actions:

- Ensure data block number is correct.

Trip | Card Option
--- | ---
Value | 180
Short description |

A parameter file has been transferred from a NV media card to the drive, but at least one of the option modules are difference between source and target drives. This trip does not stop the data transfer, but is a warning that the data for the option modules that are different will be set to the default values and not the values from the card. This trip also applies if a compare is performed between a parameter file on a card and the drive and the option modules fitted are different between the source and target.

Recommended actions:

- Ensure the correct option modules are installed.
- Ensure the option modules are in the same option module slot as the parameter set stored.
- Press the red reset button to acknowledge that the parameters for one or more of the option modules installed will be at their default vaules.
- This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.

Trip | Card Product
--- | ---
Value | 175
Short description |

If Drive Derivative (11.028) or Product Type (11.063) are different between the source and target drives then this trip is initiated either at power-up or when the card is accessed. It will have one of the following sub-trip numbers:

Sub-trip | Reason
1 | If Drive Derivative (11.028) is different between the source and target drives, this trip is initiated either at power-up or when the SD Card is accessed. Data is still transferred, since this is a warning trip; the trip can be suppressed by entering code 9666 in parameter xx.000, and reseting the drive (this applies the warning suppression flag to the card).
2 | If Product Type (11.063) is different between the source and target drives or if corruption is detected in the parameter file, this trip is initiated either at power-up or when the SD Card is accessed. This trip can be reset but no data are transferred in either direction between the drive and the card.
3 | A Unidrive SP parameter value was found that has no equivalent parameter on the destination drive. Data is still transferred, since this is a warning trip; the trip can be suppressed by entering code 9666 in parameter xx.000, and reseting the drive (this applies the warning suppression flag to the card).

Recommended actions:

- Use a different NV media card.
- This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.

Trip | Card Rating
--- | ---
Value | 186
Short description |

A parameter file has been transferred from a NV media card to the drive, but the current and/or voltage rating are different between source and target drive. This trip does not stop the data transfer, but is a warning that the data for rating dependent parameters may not be the same on the target as the source drive. This trip also applies if a compare (using Pr mm.000 set to 8yyy) is performed between a parameter file on the card on the drive.

Recommended actions:

- Reset the drive to clear the trip.
- This trip can be suppressed by setting Pr mm.000 to 9666 and resetting the drive.

Trip | Card Read Only
--- | ---
Value | 181
Short description |

An attempt has been made to modify data on a read-only NV media card or to modify a read-only file (i.e. erase the card, erase a file or create a file). No data is transferred.

Recommended actions:

- Clear the read only flag by setting Pr mm.000 to 9777 and reset the drive. This will clear the read only flag for all data blocks in the NV media card.

Trip | Card Slot
--- | ---
Value | 174
Short description |

The transfer of an option module application program to or from an application module can fail because the option module does not respond correctly. If this happens this trip is produced with the sub-trip indicating the option module slot number.

Sub-trip number | Reason
1 | Error in option slot 1
2 | Error in option slot 2
3 | Error in option slot 3
4 | Error in option slot 4

Recommended actions:

- Ensure the source / destination option module is installed on the correct slot.

Trip | Configuration
--- | ---
Value | 111
Short description |

The Number Of Power Modules Detected (11.071) is different from the number expected. The sub-trip value indicates the number of power modules expected.

Recommended actions:

- Ensure that all the power modules are correctly connected and powered up.
- Ensure that the value in Number Of Power Modules Detected (11.071) is set to the number of power modules connected.
- Set Number Of Power Modules Test (11.035) to 0 to disable the trip if not required.

This trip is also initiated if the number of external rectifiers connected to each power module is less than the number defined by Number Of Rectifiers Expected (11.096). If this is the reason for the trip the sub-trip is 10x where x is the number of external rectifiers that should be connected.

Recommended actions:

- Ensure that all the external rectifiers are connected correctly.
- Ensure that the value in Number Of Rectifiers Expected (11.096) is correct.

Trip | Control Word
--- | ---
Value | 35
Short description |

This trip is initiated by setting bit 12 on the control word in Control Word (06.042) when the control word is enabled (Control Word Enable (06.043) = On).

Recommended actions:

- Check the value of Control Word (06.042).
- Disable the control word in Control Word Enable (06.043).

Trip | Current Offset
--- | ---
Value | 225
Short description |

The current feedback offset is too large to be trimmed correctly. The sub-trip relates to the output phase for which the offset error has been detected.

Sub-trip | Phase
1 | U
2 | V
3 | W

Recommended actions:

- Ensure that there is no possibility of current flowing in the output phase of the drive when the drive is not enabled.
- Hardware fault - contact the supplier of the drive.

Trip | Data Changing
--- | ---
Value | 97
Short description |

A user action or a file system write is active that is changing the drive parameters and the drive has become active, i.e. Drive Active (10.002) = 1. The user actions that change drive parameters are loading defaults, changing drive mode, or transferring data from an NV memory card or a position feedback device to the drive. The file system actions that will cause this trip to be initiated if the drive is enabled during the transfer are writing a parameter or macro file to the drive, or transferring a derivative or user program to the drive. It should be noted that none of these actions can be started if the drive is active, and so the trip only occurs if the action is started and then the drive is enabled.

Recommended actions:

- Ensure the drive is not enabled when one of the following is being carried out:

- Loading defaults
- Changing drive mode
- Transferring data from a NV media card or position feedback device
- Transferring user programs

Trip | Derivative ID
--- | ---
Value | 247
Short description |

There is a problem with the identifier associated with derivative image which customises the drive. The reason for the trip is given by the sub-trip as follows.

Sub-trip | Reason for trip
1 | There should be a derivative image in the product but this has been erased.
2 | The identifer is out of range.
3 | The derivative image has been changed.

Trip | Derivative Image
--- | ---
Value | 248
Short description |

An error has been detected in the derivative product image. The sub-trip indicated the reason for the trip.

Sub-trip | Reason | Comments
1 | Divide by zero |
2 | Undefined trip |
3 | Attempted fast parameter access set-up with non-existent parameter |
4 | Attempted access to non-existent parameter |
5 | Attempted write to read-only parameter |
6 | Attempted and over-range write |
7 | Attempted read from write-only parameter |
30 | The image has failed because either its CRC is incorrect, or there are less than 6 bytes in the image or the image header version is less than 5. | Occurs when the drive powers-up or the image is programmed. The image tasks will not run.
31 | The image requires more RAM for heap and stack than can be provided by the drive. | As 30.
32 | The image requires an OS function call that is higher than the maximum allowed. | As 30.
40 | The timed task has not completed in time and has been suspended. |
41 | Undefined function called, i.e. a function in the host system vector table that has not been assigned. | As 40.
51 | Core menu customisation table CRC check failed | As 30.
52 | Customisable menu table CRC check failed | As 30.
53 | Customisable menu table changed | Occurs when the drive powers-up or the image is programmed and the table has changed. Defaults are loaded for the derivative menu and the trip will keep occurring until drive parameters are saved.
61 | The option module fitted in slot 1 is not allowed with the derivative image. | As 30.
62 | The option module fitted in slot 2 is not allowed with the derivative image. | As 30.
63 | The option module fitted in slot 3 is not allowed with the derivative image. | As 30.
64 | The option module fitted in slot 4 is not allowed with the derivative image. | As 30.
70 | An option module that is required by the derivative image is not fitted in any slot. | As 30.
71 | An option module specifically required to be fitted in slot 1 not present. | As 30.
72 | An option module specifically required to be fitted in slot 2 not present. | As 30.
73 | An option module specifically required to be fitted in slot 3 not present. | As 30.
74 | An option module specifically required to be fitted in slot 4 not present. | As 30.
80 | *Image is not compatible with the control board | Initiated from within the image code.
81 | *Image is not compatible with the control board serial number | As 80.

Recommended actions:

- Contact the supplier of the drive.

Trip | Destination
--- | ---
Value | 199
Short description |

This trip indicated that destination output parameters of two or more logic functions (Menus 05, 07, 08, 09, 12 or 14) within the drive are writing to the same parameter.

Recommended actions:

- Set Pr mm.000 to "Destinations" or 12001 and check all visible parameters in all menus for parameter write conflicts.

Trip | Drive Size
--- | ---
Value | 224
Short description |

This trip indicates that the control PCB has not recognized the drive size of the power circuit to which it is connected.

Recommended actions:

- Ensure the drive is programmed to the latest software version.
- Hardware fault - return drive to supplier.

Trip | EEPROM Fail
--- | ---
Value | 31
Short description |

EEPROM Fail trip indicates that default parameters have been loaded because of the reasons given below.

Sub-trip | Reason
1 | The most significant digit of the internal parameter database version number has changed.
2 | The CRC’s applied to the parameter data stored in internal non-volatile memory indicate that a valid set of parameters cannot be loaded.
3 | The drive mode restored from internal non-volatile memory is outside the allowed range for the product or the derivative image does not allow the previous drive mode.
4 | The drive derivative image has been changed and it has changed the customisation of the drive core menus.
5 | The power stage hardware has been change and changed the customisation of the drive core menus.
6 | The internal I/O hardware has been change and changed the customisation of the drive core menus.
7 | The position feedback interface hardware has been change and changed the customisation of the drive core menus.
8 | The control board hardware has been change and changed the customisation of the drive core menus.
9 | The checksum on the non-parameter area of the EEPROM has failed.

The drive holds two banks of user save parameters and two banks of power down save parameters in non-volatile memory. If the last bank of either set of parameters that was saved is corrupted a User Save or Power Down Save trip is produced. If one of these trips occurs the parameters values that were last saved successfully are used. It can take some time to save parameters when requested by the user and if the power is removed from the drive during this process it is possible to corrupt the data in the non-volatile memory.

If both banks of user save parameters or both banks of power down save parameters are corrupted or one of the other conditions given in the table above occurs EEPROM Fail.xxx trip is produced. If this trip occurs it is not possible to use the data that has been saved previously, and so the drive will be in lowest allowed drive mode with default parameters. The trip can only be reset if Parameter mm.000 (mm.000) is set to 10, 11, 1233 or 1244 or if Load Defaults (11.043) is set to a non-zero value.

Recommended actions:

- Default the drive and perform a drive reset.
- Allow sufficient time to perform a save before the supply to the drive is removed.
- If the trip persists, return drive to the supplier.

Trip | Encoder 1
--- | ---
Value | 189
Short description |

Drive position feedback interface power supply overloaded. Terminals 13 & 14 of the 15 way D-type connector can supply a maximum current of 200mA at 15V or 300mA at 5V.

Recommended actions:

- Check encoder power supply wiring.
- Disable the termination resistors (P1 Termination Select (03.039) set to 0) to reduce current consumption.
- For 5V encoders with long cables, select 8V (P1 Supply Voltage (03.036)) and fit a 5V voltage regulator close to the encoder.
- Check the encoder specification to confirm it is compatible with the encoder port power supply current capability.
- Replace the encoder.
- Use an external power supply with higher current capability.

Trip | Encoder 2
--- | ---
Value | 190
Short description |

The drive has detected a wire break on the 15 way D-type connector on the drive. The exact cause of the trip can be identified from the sub-trip number.

Sub-trip | Reason
1 | Drive position feedback interface 1 on any input
2 | Drive position feedback interface 2 on any input
11 | Drive position feedback interface 1 on the A channel
12 | Drive position feedback interface 1 on the B channel
13 | Drive position feedback interface 1 on the Z channel

Recommended actions:

- If wire break detection on the drive encoder input is not required, set bit 0 of P1 Error Detection Level (03.040) to 0 to disable the Encoder 2 trip.
- Check cable continuity.
- Check wiring of feedback signals is correct.
- Check encoder power supply is set correctly (P1 Supply Voltage (03.036)).
- Replace the encoder.

Trip | Encoder 3
--- | ---
Value | 191
Short description |

The drive has detected an incorrect UVW phase angle while running (RFC-S mode only) or SINCOS phase error. The feedback device which has caused the trip can be identified by the sub-trip number.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- Check encoder shield connections.
- Ensure the encoder cable is one uninterrupted cable.
- Check the encoder signal for noise with an oscilloscope.
- Check the integrity of the encoder mechanical mounting.
- For a UVW servo encoder, ensure that the phase rotation of the UVW commutation signals is the same asthe phase rotation of the motor.
- For a SINCOS encoder, ensure that motor and incremental SINCOS connections are correct and that for forward rotation of the motor, the encoder rotates clockwise (when looking at the shaft of the encoder).
- Repeat the offset measurement test.

Trip | Encoder 4
--- | ---
Value | 192
Short description |

This trip indicates that the encoder communications has timed out or the communications position message transfer time is too long. This trip can also be caused due to a wire break in the communication channel between the drive and the encoder. The feedback device which has caused the trip can be identified by the sub-trip number.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- Ensure the encoder power supply setting (P1 Supply Voltage (03.036)) is correct.
- Complete encoder auto-configuration (P1 Auto-configuration Select (03.041) = Enabled).
- Check the encoder wiring.
- Replace the feedback device.

Trip | Encoder 5
--- | ---
Value | 193
Short description |

This trip indicates that there is a checksum or CRC error, or the SSI encoder is not ready. The Encoder 5 trip can also indicate a wire break to a communications based encoder.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- Check the encoder cable shield connections.
- Ensure the cable is one uninterrupted cable - remove any connector blocks or if unavoidable minimise the length of any shield pigtails to the connector block.
- Check the encoder signal for noise with an oscilloscope.
- Check P1 Comms Bits (03.035).
- If using a Hiperface, EnDat or BiSS encoder, carry out an encoder auto-configuration (P1 Auto-configuration Select (03.041) = Enabled).
- Replace the encoder.

Trip | Encoder 6
--- | ---
Value | 194
Short description |

This trip indicates that the encoder has indicated an error or that the power supply has failed to an SSI encoder. This trip can also indicate a wire break to an SSI encoder.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- For SSI encoders, check the wiring and encoder power supply setting (P1 Supply Voltage (03.036)).
- Replace the encoder / contact the supplier of the encoder.

Trip | Encoder 7
--- | ---
Value | 195
Short description |

A set-up parameter for the position feedback device has been changed. See P1 Error Detection Level (03.040).

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Trip | Encoder 8
--- | ---
Value | 196
Short description |

This trip indicates that the position feedback interface communications time exceeds 250µs. The feedback device which has caused the trip can be indentified by the sub-trip number.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- Ensure the encoder is connected correctly.
- Ensure that the encoder is compatible.
- Increase baud rate.

Trip | Encoder 9
--- | ---
Value | 197
Short description |

- This indicates that the position feedback selected from an option slot that does not contain a position feedback category option module.

Recommended action:

- Check the setting of Motor Control Feedback Select (03.026) (or M2 Motor Control Feedback Select (21.021) if the second motor parameters have been enabled).
- Ensure that the option slot selected in Motor Control Feedback Select (03.026) has a feedback option module installed.

Trip | Encoder 12
--- | ---
Value | 162
Short description |

This trip indicates that the drive is communicating with the encoder but the encoder type is not recognised.

Sub-trip | Reason
1 | Drive position feedback interface 1
2 | Drive position feedback interface 2

Recommended actions:

- Enter the encoder setup parameters manually.
- Check to see if the encoder supports auto-configuration.

Trip | Encoder 13
--- | ---
Value | 163
Short description |

This trip indicates that the data read from the encoder was out of range during auto-configuration. No parameters will be modified with data read from the encoder as a result of auto-configuration. The tens in the sub-trip number indicate the interface number (i.e. 1 for P1 interface and 2 for P2 interface).

Sub-trip | Reason
x1 | Rotary lines per revolution error
x2 | Linear comms pitch error
x3 | Linear line pitch error
x4 | Rotary turns bits error
x5 | Communcations bits error
x6 | Calculation time is too long
x7 | Line delay measured is longer than 5µs

Recommended actions:

- Enter the encoder setup parameters manually.
- Check to see if the encoder supports auto-configuration.

Trip | External Trip
--- | ---
Value | 6
Short description |

External trip is initiated as shown in the table below.

Sub-trip | Reason
1 | External Trip Mode (08.010) = 1 or 3 and SAFE TORQUE OFF Input 1 is low
2 | External Trip Mode (08.010) = 2 or 3 and SAFE TORQUE OFF Input 2 is low
3 | External Trip (10.032) = 1

Recommended actions:

- Check the SAFE TORQUE OFF signal voltage on terminal 31 is 24V.
- Check the value of STO Input 01 State (08.009) which indicates the digital state of terminal 31.
- If external trip detection of the SAFE TORQUE OFF input is not required, set External Trip Mode (08.010) to Off (0).
- Checl the value of External Trip (10.032).
- Select "Destinations" (or enter 12001) in Pr mm.000 and check for a parameter controlling External Trip (10.032).
- Ensure External Trip (10.032) or User Trip (10.038) (=6) is not being used by serial comms.

Trip | I/O Overload
--- | ---
Value | 26
Short description |

This trip indicates that the total current drawn from the 24V user supply or from the digital output has exceeded the limit. A trip is initiated if one or more of the following conditions:

- Maximum output current from one digital output is 100mA.
- The combined maximum output current from outputs 1 and 2 is 100mA.
- The combined maximum output current from output 3 and +24V output is 100mA.

Recommended actions:

- Check total loads on digital outputs.
- Check control wiring is correct.
- Check output wiring is undamaged.

Trip | Inductance
--- | ---
Value | 8
Short description |

This trip occurs in RFC-S mode when the drive has detected that the motor inductances are not suitable for the operation being attempted. The trip is either caused because the ratio or difference between Ld and Lq is too small or because the saturation characteristic of the motor cannot be measured.

If the inductance ratio or difference is too small this is because one of the following conditions is true:

(No-load Lq (05.072)- Ld (05.024)) / Ld (05.024) < 0.1

(No-load Lq (05.072) - Ld (05.024)) < (K / Full Scale Current Kc (11.061))H

where:

Drive Rated Voltage (11.033) | K
200V | 0.0073
400V | 0.0146
575V | 0.0174
690V | 0.0209

If the saturation characteristic of the motor cannot be measured this is because when the flux in the motor is changed the measured value of Ld does change sufficiently due to saturation to be measured. When half of Rated Current (05.007) is applied in the d axis of the motor in each direction the inductance must fall change at least (K / (2 x Full Scale Current Kc (11.061))) H.

The specific reasons for each of the sub-trips are given in the table below.

Sub-trip | Reason
1 | The inductance ratio or difference is too small when the drive has been started in sensorless mode.
2 | The saturation characteristic of the motor cannot be measured when the drive has been started in sensorless mode.
3 | The inductance ratio or difference is too small when an attempt is made to determine the location of the motor flux during a stationary auto-tune in RFC-S mode. This trip is also produced when the inductance ratio or inductance difference is too small when carrying out a phasing test on starting in RFC-S mode. If position feedback is being used the measured value for Position Feedback Phase Angle (03.025) may not be reliable. Also the measured values of Ld (05.024) and No-load Lq (05.072) may not correspond to the d and q axis respectively.
4 | The direction of the flux in the motor is detected by the change of inductance with different currents. This trip is initiated if the change cannot be detected when an attempt is made to perform a stationary auto-tune when position feedback is being used, or to perform a phasing test on starting in RFC-S mode.

Trip | Inductor Too Hot
--- | ---
Value | 93
Short description |

Regen inductor overload. See Inductor Thermal Time Constant (04.015).

Trip | Inter-connect
--- | ---
Value | 103
Short description |

Multi-power module drive interconnection cable error. The sub-trip "xx.0.00" indicates which power module has detected the fault where xx is the power module number. It should be noted that this trip is also initiated if the communication fails either when a rectifier signals a fault or a trip us reset. In this case the sub-trip is the number of modules that are still communicating correctly.

Trip | Island
--- | ---
Value | 160
Short description |

This trip indicates that a regen system is connected to an islaned supply. The sub-trips indicate the reason for the trip.

Sub-trip | Reason
1 | Island detection system has been enabled and detected an island condition
2 | The minimum synchronisation voltage is non-zero and the supply voltage has been below this threshold and been simulating its own supply synchronisation for more than 2.0s.

Recommended actions:

- Check the supply / supply connections to the regen drive.

Trip | Keypad Mode
--- | ---
Value | 34
Short description |

If keypad reference mode is enabled (Reference Selected Indicator (01.049) = 4 or 6) (i.e. Reference Selector (01.014) is set to 4 or 6 if motor map 1 is selected, or M2 Reference Selector (21.003) is set to 4 or 6 if motor map 2 is selected) and the keypad removed, then this trip is initiated.

Recommended actions:

- Re-install keypad and reset.
- Change Reference Selector (01.014) to select the reference from another source.

Trip | Line Sync
--- | ---
Value | 39
Short description |

This trip indicates that the inverter has lost the synchronization with the ac supply in Regen mode.

Recommended actions:

- Check the supply / supply connections to the regen drive.

Trip | Low Load
--- | ---
Value | 38
Short description |

This trip is initiated if the low load detector is set up to produce a trip on low load detection and this condition occurs. See Enable Trip On Low Load (04.029).

Trip | Motor Too Hot
--- | ---
Value | 20
Short description |

This trip indicates a motor thermal overload based on the Rated Current (05.007) and Motor Thermal Time Constant 1 (04.015). Motor Protection Accumulator (04.019) displays the motor temperature as a percentage of the maximum value. The drive will trip on Motor Too Hot when Motor Protection Accumulator (04.019) gets to 100%.

Recommended actions:

- Ensure the load is not jammed / sticking.
- Check the load on the motor has not changed.
- If seen during an auto-tune test in RFC-S mode, ensure the Rated Current (05.007) is = Heavy duty current rating of the drive.
- Tune the Rated Speed (05.008) (RFC-A mode only).
- Check feedback signal for noise.
- Ensure the motor rated current is not zero.

Trip | Name Plate
--- | ---
Value | 176
Short description |

This trip is initiated if an electronic name plate transfer between the drive and the motor has failed. The exact cause of the trip can be identified from the sub-trip number.

Sub-trip | Reason
1 | Not enough memory space to complete the transfer
2 | Communication with encoder failed
3 | The transfer has failed
4 | The checksum of the stored object has failed

Recommended actions:

- Ensure that the device encoder memory has at least 128 bytes to store the nameplate data
- When writing the motor object (xx.000 = 11000), ensure that the device encoder memory has at least 256 bytes to store all the nameplate data.
- When transferring between option module and encoder, ensure that the option slot has a feedback option module installed.
- Check if the encoder has been iniitalised Position Feedback Initialized (03.076).
- Verify the encoder wiring.

Trip | None
--- | ---
Value | 0
Short description |

No trip has been stored in this position in the trip log.

Trip | OHt Brake
--- | ---
Value | 101
Short description |

This trip indicates that braking IGBT over-temperature has been detected based on firmware thermal model.

Recommended actions:

- Check braking resistor value is greater than or equal to the minimum resistance value.

Trip | OHt Control
--- | ---
Value | 23
Short description |

This trip indicates that a control stage over-temperature has been detected. From the sub-trip "xxyzz", the cause of the trip can be identified as follows:

Source | xx | y | zz
Control system | 00 | 0 | 01: Control board thermistor 1
Control system | 00 | 0 | 02: Control board thermistor 2
Control system | 00 | 0 | 03: I/O board thermistor

Recommended actions:

- Check enclosure / drive fans are still functioning correctly.
- Check enclosure ventilation paths.
- Check enclosure door filters.
- Increase ventilation.
- Reduce the drive switching frequency.
- Check ambient temperature.

Trip | OHt dc bus
--- | ---
Value | 27
Short description |

This trip indicates a DC bus component over temperature based on a firmware thermal model. The drive includes a thermal protection system to protect the DC bus components within the drive. This includes the effects of the output current and DC bus ripple. The estimated temperature is displayed as a percentage of the trip level in Percentage Of d.c. Link Thermal Trip Level (07.035). If this parameter reaches 100% then an OHt dc bus trip with sub-trip 200 is initiated. The drive will attempt to stop the motor before tripping. If the motor does not stop in 10 seconds then the drive trips immediately.

Source | xx | y | zz
Control system | 00 | 2 | 00: D.c. link thermal model gives {OHt dc bus} trip with sub-trip 0.

It is also possible in a multi-power module system for d.c. link over-temperature to be detected from within the power stage. From this source the estimated temperature as a percentage of trip is not available and the trip is indicated as follows:

Source | xx | y | zz
Control system | 01 | 0 | 00: Power stage gives {OHt dc bus} trip with sub-trip 0.

Recommended actions:

- Check the AC supply voltage balance and levels.
- Check the DC bus ripple level.
- Reduce duty cycle.
- Reduce motor load.
- Check output current stability. If unstable;

- Check the motor map settings with motor nameplate (Rated Frequency (05.006), Rated Current (05.007), Rated Speed (05.008), Rated Voltage (05.009), Rated Power Factor (05.010) and Number Of Motor Poles (05.011)) - (All modes).
- Disable slip compensation (Enable Slip Compensation (05.027) = Off (0)) - (Open-loop).
- Disable dynamic V to F operation (Dynamic V To F Select (05.013) = Off (0)) - (Open-loop).
- Select fixed boost (Open-loop Control Mode (05.014) = Fixed (2)) - (Open-loop).
- Select high stability space vector modulation (High Stability Space Vector Modulation (05.019) = On (1)) - (Open-loop).
- Disconnect the load and complete a rotating auto-tune (Auto-tune (05.012) = 2) - (RFC-A and RFC-S).
- Auto-tune the rated speed value (Rated Speed Optimisation Select (05.016) = 1) - (RFC-A and RFC-S).
- Reduce speed loop gains (Speed Controller Proportional Gain Kp1 (03.010), Speed Controller Integral Gain Ki1 (03.011) and Speed Controller Differential Feedback Gain Kd1 (03.012)) - (RFC-A and RFC-S).
- Add a speed feedback filter value (P1 Feedback Filter (03.042)) - (RFC-A and RFC-S).
- Add a current demand filter (Current Reference Filter 1 Time Constant (04.012)) - (RFC-A and RFC-S).
- Check encoder signals for noise with an oscilloscope - (RFC-A and RFC-S).
- Check encoder mechanical coupling - (RFC-A and RFC-S).

Trip | OHt Inverter
--- | ---
Value | 21
Short description |

This trip indicates that an IGBT junction over-temperature has been detected based on a firmware thermal model. The sub-trip indicates which model has initiated the trip in the form xxyzz as given below.

Source | xx | y | zz
Control system | 00 | 1 | 00: Inverter thermal model
Control system | 00 | 3 | 00: Braking IGBT thermal model

Recommended actions with sub-trip 100:

- Reduce the selected drive switching frequency.
- Ensure Auto-switching Frequency Change (05.035) is set to Off.
- Reduce duty cycle.
- Decrease acceleration / deceleration rates.
- Reduce motor load.
- Check DC bus ripple.
- Ensure all three input phases are present and balanced.

Recommended actions with sub-trip 300:

- Reduce the braking load.

Trip | OHt Power
--- | ---
Value | 22
Short description |

This trip indicates that a power stage over-temperature has been detected. The sub-trip "xxyzz" indicates which thermistor is indicating the over-temperature. The thermsitor numbering is different for a single module type drive (i.e. no parallel board fitted) and a multi-module type drive (i.e. parallel board fitted with one or more power modules) as shown below:

Single module type drive:

Source | xx | y | zz
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power board
Power system | 01 | Rectifier number | zz: Thermistor location defined by zz in the rectifier

Multi-module type system:

Source | xx | y | zz
Power system | Power module number | 0 | 01: U phase power device
Power System | Power module number | 0 | 02: V phase power device
Power system | Power module number | 0 | 03: W phase power device
Power system | Power module number | 0 | 04: Rectifier
Power system | Power module number | 0 | 05: General power system
Power system | Power module number | 0 | 00: Braking IGBT

Note that the power module that has caused the trip cannot be identified except for the braking IGBT temperature measurement

Recommended actions:

- Check enclosure / drive fans are still functioning correctly.
- Force the heatsink fans to run at maximum speed.
- Check enclosure ventilation paths.
- Check enclosure door filters.
- Increase ventilation.
- Reduce duty cycle.
- Decrease acceleration / deceleration rates.
- Reduce motor loads.
- Check the derating tables and confirm the drive is correctly sized for the application.
- Use a drive with larger current / power rating.

Trip | OI ac
--- | ---
Value | 3
Short description |

This trip indicates that the instantaneous drive output current has exceeded the drive over current threshold.

Source | xx | y | zz
Control system | 00 | 0 | 00: Instantaneous over-current trip when the measured a.c. current exceeds over current threshold
Power system | Power module number | 0 | 00: Instantaneous over-current trip when the measured a.c. current exceeds over current threshold.

The over current threshold is the maximum current the drive can measure and is defined by VM_DRIVE_CURRENT[MAX].

Recommended actions:

- Acceleration / deceleration rate is too short.
- If seen during auto-tune reduce the voltage boost.
- Check for short circuit on the output cabling.
- Check integrity of the motor insulation using a Megger.
- Check feedback device wiring.
- Check feedback drive mechanical coupling.
- Check feedback signals are free from noise.
- Check motor cable is within limits for the frame size.
- Reduce the speed loop gains (Speed Controller Proportional Gain Kp1 (03.010), Speed Controller Integral Gain Ki1 (03.011), Speed Controller Differential Feedback Gain Kd1 (03.012)).
- Check that the phase angle auto-tune has been completed (RFC-S mode only).
- Reduce the current loop gains (RFC-A and RFC-S modes only).

Trip | OI Brake
--- | ---
Value | 4
Short description |

This trip indicates that an over-current has been detected in braking IGBT or braking IGBT protection has been activated.

Source | xx | y | zz
Power system | Power module number | 0 | 00: Braking IGBT instantaneous over-current trip

Recommended actions:

- Check brake resistor wiring.
- Check braking resistor value is greater than or equal to the minimum resistance value.
- Check braking resistor insulation.

Trip | OI dc
--- | ---
Value | 109
Short description |

This trip indicates that the short circuit protection for the drive output stage has been activated. The table below shows where the trip has been detected.

Source | xx | y | zz
Control system | 00 | 0 | 00
Power system | Power module number | 0 | 00

Recommended actions:

- Disconnect the motor cable at the drive end and check the motor and cable insulation with a Megger.
- Replace the drive.

Trip | OI Snubber
--- | ---
Value | 92
Short description |

This trip indicates that an over-current condition has been detected in the rectifier snubbing circuit, The exact cause of the trip can be identified by the sub-trip number.

Source | xx | y | zz
Power system | 01 | Rectifier number* | 00: Rectifier snubber over-current trip detected.

*For a parallel power-module system the rectifier number will be one as it is not possible to determine which rectifier has detected the fault.

Recommended actions:

- Ensure the internal EMC filter is installed.
- Ensure the motor cable length does not exceed the maximum for selected switching frequency.
- Check for supply voltage imbalance.
- Check for supply disturbance such as notching from a DC drive.
- Check the motor and motor cable insulation with a Megger.
- Fit an output line reactor or sinusoidal filter.

Trip | Option Disable
--- | ---
Value | 215
Short description |

During drive mode changeover option modules must acknowledge that they have stopped accessing the communications system between the option slots and the drive. If an option module does not do this in the allowed time then this trip is produced.

Recommended actions:

- Reset the trip.
- If the trip persists, replace the option module.

Trip | Out Phase Loss
--- | ---
Value | 98
Short description |

This trip indicates that phase loss has been detected at the drive output.

Sub-trip | Reason
1 | U phase detected as disconnected when drive enabled to run
2 | V phase detected as disconnected when drive enabled to run
3 | W phase detected as disconnected when drive enabled to run
4 | Output phase loss detected when the drive is running

Note that if Reverse Output Phase Sequence (05.042) = 1 the physical output phases are reversed, and so sub-trip 3 refers to physical output phase V and sub-trip 2 refers to physical output phase W.

Recommended actions:

- Check motor and drive connections.
- To disable the trip set Output Phase Loss Detection Enable (06.059) to zero.

Trip | Over Speed
--- | ---
Value | 7
Short description |

In open-loop mode, if the Output Frequency (05.001) exceeds the threshold set in Over Speed Threshold (03.008) in either direction, an Over Speed trip is produced. In RFC-A and RFC-S modes, if the Speed Feedback (03.002) exceeds the threshold set in Over Speed Threshold (03.008) in either direction, an Over Speed trip is produced. If Over Speed Threshold (03.008) is set to 0.0 the threshold is then equal to 1.2 x the value set in Maximum Reference Clamp (01.006).

In RFC-A and RFC-S modes if an SSI encoder is being used and P1 SSI Incremental Mode (03.047) is set to Off, an Over Speed trip will beproduced when the encoder passes through the boundary between its maximum position and zero.

Recommended actions:

- Reduce the Speed Controller Proportional Gain Kp1 (03.010) to reduce the speed overshoot (RFC-A and RFC-S modes only).
- If an SSI encoder is being used, set P1 SSI Incremental Mode (03.047) to On.

The above description relates to a standard over speed trip, however in RFC-S mode it is possible to produce an Overspeed trip with sub-trip 1. This is caused if the speed is allowed to exceed the safe level in RFC-S mode with flux weakening. See Enable High Speed Mode (05.022) for details.

Trip | Over Volts
--- | ---
Value | 2
Short description |

This trip indicates that the DC bus voltage has exceeded VM_DC_VOLTAGE[MAX] or VM_DC_VOLTAGE_SET[MAX] for 15s. The trip threshold varies depending on voltage rating of the drive drive as shown below.

Voltage rating | VM_DC_VOLTAGE[MAX] | VM_DC_VOLTAGE_SET[MAX]
200 | 415 | 410
400 | 830 | 815
575 | 990 | 970
690 | 1190 | 1175

The exact cause of the trip can be identified by the sub-trip number.

Source | xx | y | zz
Control system | 00 | 0 | 01: Instantaneous trip when the d.c. link voltage exceeds VM_DC_VOLTAGE[MAX].
Control system | 00 | 0 | 02: Time delayed trip indicating that the d.c. link voltage is above VM_DC_VOLTAGE_SET[MAX].

Recommended actions:

- Increase deceleration ramp.
- Decrease the braking resistor value (staying above the minimum value).
- Check nominal AC supply level.
- Check for supply disturbances which could cause the DC bus level to rise.
- Check motor insulation using a Megger.

Trip | Phase Loss
--- | ---
Value | 32
Short description |

This trip does not occur in Regen mode.

Trip | Phasing Error
--- | ---
Value | 198
Short description |

This indicates that the phase offset angle in Position Feedback Phase Angle (03.025) (or M2 Position Feedback Phase Angle (21.020) if the second motor map is being used) is incorrect if position feedback is being used and the drive is unable to control the motor correctly.

Recommended actions:

- Check the encoder wiring.
- Check the encoder signals for noise with an oscilloscope.
- Check encoder mechanical coupling.
- Perform an auto-tune to measure the encoder phase angle or manually enter the correct phase angle into Position Feedback Phase Angle (03.025).
- Spurious Phasing Error trips can sometimes be seen in very dynamic applications. This trip can be disabled by setting Over Speed Threshold (03.008) to a value greater than zero.

If sensorless control is being used this indicates that significant instability has occurred and the motor has accelerated without control.

Recommended actions:

- Ensure that the motor parameters are set-up correctly.
- Reduce the speed controller gains.

Trip | Power Comms
--- | ---
Value | 90
Short description |

A Power Comms trip indicates a communications problem within the power system of the drive. The reason for the trip can be identified by the sub-trip number.

Type of drive | xx | y | zz
Single power module system | 01 | Rectifier number* | 00: Excessive communications errors detected by the rectifier module.

*For a parallel power-module system the rectifier number will be one as it is not possible to determine which rectifier has detected the fault.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Power Data
--- | ---
Value | 220
Short description |

This trip can be generated either from the drive control system or from the power system.

This trip is produced if there is an error in the configuration data stored in the power system. If the source of the trip is the control system then the trip related to the table that is uploaded from the power system at power-up.

Source | xx | y | zz
Control system | 00 | 0 | 02: There is no data table to be uploaded to the control board.
Control system | 00 | 0 | 03: The power system data table is bigger than the space available in the control pod to store it.
Control system | 00 | 0 | 04: The size of the table given in the table is incorrect
Control system | 00 | 0 | 05: Table CRC error.
Control system | 00 | 0 | 06: The version number of the generator software that produced the table is too low, i.e. a table from a newer generator is required that includes features that have been added to the table that may not be present.
Control system | 00 | 0 | 07: The power board data table does not match the power board hardware identifier.
Power system | 01 | 0 | 00: The power data table used internally by the power module has an error. (For a multi-power module drive this indicates any error with the code tables in the power system.)
Power system | 01 | 0 | 01: The power data table that should be uploaded to the control system on power up has an error.
Power system | 01 | 0 | 02: The power data table used internally by the power module does not match the hardware identification of the power module.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Power Down Save
--- | ---
Value | 37
Short description |

This trip indicates that an error has been detected in the power down save parameters stored in non-volatile memory.

Recommended actions:

- Perform a 1001 save in Pr mm.000 to ensure that the trip doesn't occur the next time the drive is powered up.

Trip | PSU
--- | ---
Value | 5
Short description |

This trip indicates that one or more internal power supply rails are outside limits or overloaded.

Source | xx | Y | zz
Control system | 00 | 0 | 00: Internal power supply overload.
Power system | Power module number | Rectifier number* | 00: Rectifier internal power supply overload.

*For a parallel power-module system the rectifier number will be zero as it is not possible to determine which rectifier has detected the fault.

Recommended actions:

- Remove any option modules and perform a reset.
- Remove encoder connection and perform a reset.
- Hardware fault within the drive - return the drive to the supplier.

Trip | PSU 24V
--- | ---
Value | 9
Short description |

The total user load of the drive and option modules has exceeded the internal 24V power supply limit. The user load consists of the drive digital outputs and main encoder supply.

Recommended actions:

- Reduce the load and reset.
- Provide an external 24V power supply on control terminal 2.
- Remove all option modules.

Trip | Rating Mismatch
--- | ---
Value | 223
Short description |

This trip indicates that there is a voltage rating or current rating mismatch in a multi-module drive system. This trip is only applicable to modular drives that are connected in parallel. A mixture of power modules with different voltage or current ratings within the same multi-module drive system is not allowed and will cause a Rating Mismatch trip.

Recommended actions:

- Ensure that all modules in a multi-modular drive system are of the same frame size and rating (voltage and current).
- Hardware fault - contact the supplier of the drive.

Trip | Rectifier Set-up
--- | ---
Value | 94
Short description |

A rectifier has not been set-up correctly in a multi-power module system.

Recommended actions:

- Check the inter-power module wiring

Trip | Reserved 001
--- | ---
Value | 1
Short description |

This trip value is used in Unidrive SP for an under voltage trip. The under voltage condition is now a drive state, and so this trip is no longer used by the drive.

Trip | Reserved 095
--- | ---
Value | 95
Short description |

Reserved trip number.

Trip | Reserved 102
--- | ---
Value | 102
Short description |

Reserved trip number.

Trip | Reserved 104
--- | ---
Value | 104
Short description |

Reserved trip number.

Trip | Reserved 105
--- | ---
Value | 105
Short description |

Reserved trip number.

Trip | Reserved 106
--- | ---
Value | 106
Short description |

Reserved trip number.

Trip | Reserved 107
--- | ---
Value | 107
Short description |

Reserved trip number.

Trip | Reserved 108
--- | ---
Value | 108
Short description |

Reserved trip number.

Trip | Reserved 161
--- | ---
Value | 161
Short description |

Reserved trip number.

Trip | Reserved 164
--- | ---
Value | 164
Short description |

Reserved trip number.

Trip | Reserved 165
--- | ---
Value | 165
Short description |

Reserved trip number.

Trip | Reserved 166
--- | ---
Value | 166
Short description |

Reserved trip number.

Trip | Reserved 167
--- | ---
Value | 167
Short description |

Reserved trip number.

Trip | Reserved 168
--- | ---
Value | 168
Short description |

Reserved trip number.

Trip | Reserved 171
--- | ---
Value | 171
Short description |

Reserved trip number.

Trip | Reserved 172
--- | ---
Value | 172
Short description |

Reserved trip number.

Trip | Reserved 173
--- | ---
Value | 173
Short description |

Reserved trip number.

Trip | Reserved 222
--- | ---
Value | 222
Short description |

If this trip occurs please consult the drive supplier.

Trip | Reserved 228
--- | ---
Value | 228
Short description |

If this trip occurs please consult the drive supplier.

Trip | Reserved 229
--- | ---
Value | 229
Short description |

Reserved trip number.

Trip | Reserved 230
--- | ---
Value | 230
Short description |

Reserved trip number.

Trip | Reserved 231
--- | ---
Value | 231
Short description |

Reserved trip number.

Trip | Reserved 232
--- | ---
Value | 232
Short description |

Reserved trip number.

Trip | Reserved 233
--- | ---
Value | 233
Short description |

Reserved trip number.

Trip | Reserved 234
--- | ---
Value | 234
Short description |

Reserved trip number.

Trip | Reserved 235
--- | ---
Value | 235
Short description |

Reserved trip number.

Trip | Reserved 236
--- | ---
Value | 236
Short description |

Reserved trip number.

Trip | Reserved 237
--- | ---
Value | 237
Short description |

Reserved trip number.

Trip | Reserved 238
--- | ---
Value | 238
Short description |

Reserved trip number.

Trip | Reserved 239
--- | ---
Value | 239
Short description |

Reserved trip number.

Trip | Reserved 240
--- | ---
Value | 240
Short description |

Reserved trip number.

Trip | Reserved 241
--- | ---
Value | 241
Short description |

Reserved trip number.

Trip | Reserved 242
--- | ---
Value | 242
Short description |

Reserved trip number.

Trip | Reserved 243
--- | ---
Value | 243
Short description |

Reserved trip number.

Trip | Reserved 244
--- | ---
Value | 244
Short description |

Reserved trip number.

Trip | Reserved 245
--- | ---
Value | 245
Short description |

Reserved trip number.

Trip | Reserved 246
--- | ---
Value | 246
Short description |

Reserved trip number.

Trip | Reset
--- | ---
Value | 100
Short description |

This is not a valid trip number as this value is used in User Trip (10.038) to reset the drive.

Trip | Reset Logs
--- | ---
Value | 255
Short description |

This is not a valid trip number as this value is used in User Trip (10.038) to reset the trip logs.

Trip | Resistance
--- | ---
Value | 33
Short description |

This trip indicates that either the value being used for motor stator resistance is too high or that an attempt to do a test involving measuring motor stator resistance has failed. The maximum for the stator resistance parameters is generally higher than the maximum value that can be used in the control algorithms. If the value exceeds (VFS / v2) / Full Scale Current Kc (11.061), where VFS is the full scale d.c. link voltage then this trip is initiated. If the value is the result of a measurement made by the drive then sub-trip 1 is applied, or if it is because the parameter has been changed by the user then sub-trip 3 is applied. During the stator resistance section of auto-tuning an additional test is performed to measured the drive inverter characteristics to provide the compensation necessary for dead-times. If the inverter characteristic measurement fails then sub-trip 2 is applied.

Sub-trip | Reason
1 | Measured stator resistance exceeded the allowed range
2 | It was not possible to measure the inverter characteristic
3 | The stator resistance associated with the presently selected motor map exceeds the allowed range

Recommended actions:

- Check that a value has not been entered in the stator resistance for the presently selected motor map does not exceed the alloed range.
- Check the motor cable / connections.
- Check the integrity of the motor stator winding using an insulation tester.
- Check the motor phase to phase resistance at the drive terminals.
- Check the motor phase to phase resistance at the motor terminals.
- Ensure the stator resistance of the motor falls within the range of the drive model.
- Select fixed boost mode (Open-loop Control Mode (05.014) = Fixed) and verify the output current waveforms with an oscilloscope.
- Replace the motor.

Trip | Slot1 Different
--- | ---
Value | 204
Short description |

If the option module fitted in option slot 1 is different to the option module present at the last power-down then this trip is produced. The sub-trip number gives the identification code of the module that was originally fitted. The priority order for the option module different trips is Slot1 Different highest, then Slot2 Different, then Slot3 Different then Slot4 Different. Drive user parameters must be saved to prevent this trip on the next power-up if the module has changed. If the menus have been changed, but not the module, the trip will not occur on the next power-up. The sub-trip number gives the following indications of the reason for the trip.

Sub-trip | Reason
1 | No module was fitted previously
2 | A module with the same identifier is fitted, but the set-up menu for this option slot has been changed, and so default parameters have been loaded for this menu.
3 | A module with the same identifier is fitted, but the applications menu for this option slot has been changed, and so default parameters have been loaded for this menu.
4 | A module with the same identifier is fitted, but the set-up and applications menu for this option slot have been changed, and so default parameters have been loaded for these menus.
>99 | Shows the identifier of the module previously fitted.

Recommended actions:

- Turn off the power, ensure the correct option modules are installed in the correct option slots and re-apply the power.
- Confirm that the currently installed option module is correct, ensure option module parameters are set correctly and perform a user save in Pr mm.000.

Trip | Slot1 Error
--- | ---
Value | 202
Short description |

The option module in option slot 1 has indicated an error. The option module can give the reason for the error and this is shown in the sub-trip number. As default the sub-trip number is shown as a number on the display, however, it is possible for the option module to supply sub-trip number strings which will be displayed instead of the number if available.

Recommended actions:

- See relevant Option Module User Guide for details of the trip.

Trip | Slot1 HF
--- | ---
Value | 200
Short description |

This trip indicates that there is a fault with the option module in option slot 1 that means that this module cannot operate. The possible causes of the trip are given by the sub-trip value.

Sub-trip | Reason
1 | The module category cannot be identified
2 | All the required customisable menu table information has not been supplied or the tables supplied are corrupt
3 | There is insufficient memory available to allocate the comms buffers for this module.
4 | The module has not indicated that it is running correctly during drive power-up
5 | The module has been removed after power-up or it has ceased to indicate to the drive processor that it is still active.
6 | The module has not indicated that it has stopped accessing drive parameters during a drive mode change
7 | The module has failed to acknowledge that a request has been made to reset the drive processor.
8 | The drive failed to read correctly the menu table from the module during drive power-up.
9 | The drive failed to upload menu tables from the module and timed-out (5s).
10 | Menu table CRC invalid.

Recommended actions:

- Ensure the option module is installed correctly.
- Replace the option module.
- Replace the drive.

Trip | Slot1 Not Fitted
--- | ---
Value | 203
Short description |

Each option module fitted in the drive is identified at power-up and the option fitted is stored by the drive in its non-volatile memory. If an option module was fitted in slot 1 at power-down, but that option module has subsequently been removed before power up then this trip is produced. The sub-trip number gives the identification code of the option module that has been removed. The priority order for the option module not fitted trips is Slot1 Not Fitted highest, then Slot2 Not Fitted, then Slot3 Not Fitted then Slot4 Not Fitted. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Ensure the option module is installed correctly.
- Re-install the option module.
- To confirm that the removed option module is no longer required perform a save function in Pr mm.000.

Trip | Slot1 Watchdog
--- | ---
Value | 201
Short description |

This trip indicates that the option module in option slot 1 has started the option watchdog function and then failed to service this watchdog correctly.

Recommended actions:

- Replace the option module.

Trip | Slot2 Different
--- | ---
Value | 209
Short description |

If the option module fitted in option slot 2 is different to the option module present at the last power-down then this trip is produced. The sub-trip number gives the identification code of the module that was originally fitted. The priority order for the option module different trips is Slot1 Different highest, then Slot2 Different, then Slot3 Different then Slot4 Different. Drive user parameters must be saved to prevent this trip on the next power-up if the module has changed. If the menus have been changed, but not the module, the trip will not occur on the next power-up. The sub-trip number gives the following indications of the reason for the trip.

Sub-trip | Reason
1 | No module was fitted previously
2 | A module with the same identifier is fitted, but the set-up menu for this option slot has been changed, and so default parameters have been loaded for this menu.
3 | A module with the same identifier is fitted, but the applications menu for this option slot has been changed, and so default parameters have been loaded for this menu.
4 | A module with the same identifier is fitted, but the set-up and applications menu for this option slot have been changed, and so default parameters have been loaded for these menus.
>99 | Shows the identifier of the module previously fitted.

Recommended actions:

- Turn off the power, ensure the correct option modules are installed in the correct option slots and re-apply the power.
- Confirm that the currently installed option module is correct, ensure option module parameters are set correctly and perform a user save in Pr mm.000.

Trip | Slot2 Error
--- | ---
Value | 207
Short description |

The option module in option slot 2 has indicated an error. The option module can give the reason for the error and this is shown in the sub-trip number. As default the sub-trip number is shown as a number on the display, however, it is possible for the option module to supply sub-trip number strings which will be displayed instead of the number if available.

Recommended actions:

- See relevant Option Module User Guide for details of the trip.

Trip | Slot2 HF
--- | ---
Value | 205
Short description |

This trip indicates that there is a fault with the option module in option slot 2 that means that this module cannot operate. The possible causes of the trip are given by the sub-trip value.

Sub-trip | Reason
1 | The module category cannot be identified
2 | All the required customisable menu table information has not been supplied or the tables supplied are corrupt
3 | There is insufficient memory available to allocate the comms buffers for this module.
4 | The module has not indicated that it is running correctly during drive power-up
5 | The module has been removed after power-up or it has ceased to indicate to the drive processor that it is still active.
6 | The module has not indicated that it has stopped accessing drive parameters during a drive mode change
7 | The module has failed to acknowledge that a request has been made to reset the drive processor.
8 | The drive failed to read correctly the menu table from the module during drive power-up.
9 | The drive failed to upload menu tables from the module and timed-out (5s).
10 | Menu table CRC invalid.

Recommended actions:

- Ensure the option module is installed correctly.
- Replace the option module.
- Replace the drive.

Trip | Slot2 Not Fitted
--- | ---
Value | 208
Short description |

Each option module fitted in the drive is identified at power-up and the option fitted is stored by the drive in its non-volatile memory. If an option module was fitted in slot 2 at power-down, but that option module has subsequently been removed before power up then this trip is produced. The sub-trip number gives the identification code of the option module that has been removed. The priority order for the option module not fitted trips is Slot1 Not Fitted highest, then Slot2 Not Fitted, then Slot3 Not Fitted then Slot4 Not Fitted. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Ensure the option module is installed correctly.
- Re-install the option module.
- To confirm that the removed option module is no longer required perform a save function in Pr mm.000.

Trip | Slot2 Watchdog
--- | ---
Value | 206
Short description |

This trip indicates that the option module in option slot 2 has started the option watchdog function and then failed to service this watchdog correctly.

Recommended actions:

- Replace the option module.

Trip | Slot3 Different
--- | ---
Value | 214
Short description |

If the option module fitted in option slot 3 is different to the option module present at the last power-down then this trip is produced. The sub-trip number gives the identification code of the module that was originally fitted. The priority order for the option module different trips is Slot1 Different highest, then Slot2 Different, then Slot3 Different then Slot4 Different. Drive user parameters must be saved to prevent this trip on the next power-up if the module has changed. If the menus have been changed, but not the module, the trip will not occur on the next power-up. The sub-trip number gives the following indications of the reason for the trip.

Sub-trip | Reason
1 | No module was fitted previously
2 | A module with the same identifier is fitted, but the set-up menu for this option slot has been changed, and so default parameters have been loaded for this menu.
3 | A module with the same identifier is fitted, but the applications menu for this option slot has been changed, and so default parameters have been loaded for this menu.
4 | A module with the same identifier is fitted, but the set-up and applications menu for this option slot have been changed, and so default parameters have been loaded for these menus.
>99 | Shows the identifier of the module previously fitted.

Recommended actions:

- Turn off the power, ensure the correct option modules are installed in the correct option slots and re-apply the power.
- Confirm that the currently installed option module is correct, ensure option module parameters are set correctly and perform a user save in Pr mm.000.

Trip | Slot3 Error
--- | ---
Value | 212
Short description |

The option module in option slot 3 has indicated an error. The option module can give the reason for the error and this is shown in the sub-trip number. As default the sub-trip number is shown as a number on the display, however, it is possible for the option module to supply sub-trip number strings which will be displayed instead of the number if available.

Recommended actions:

- See relevant Option Module User Guide for details of the trip.

Trip | Slot3 HF
--- | ---
Value | 210
Short description |

This trip indicates that there is a fault with the option module in option slot 3 that means that this module cannot operate. The possible causes of the trip are given by the sub-trip value.

Sub-trip | Reason
1 | The module category cannot be identified
2 | All the required customisable menu table information has not been supplied or the tables supplied are corrupt
3 | There is insufficient memory available to allocate the comms buffers for this module.
4 | The module has not indicated that it is running correctly during drive power-up
5 | The module has been removed after power-up or it has ceased to indicate to the drive processor that it is still active.
6 | The module has not indicated that it has stopped accessing drive parameters during a drive mode change
7 | The module has failed to acknowledge that a request has been made to reset the drive processor.
8 | The drive failed to read correctly the menu table from the module during drive power-up.
9 | The drive failed to upload menu tables from the module and timed-out (5s).
10 | Menu table CRC invalid.

Recommended actions:

- Ensure the option module is installed correctly.
- Replace the option module.
- Replace the drive.

Trip | Slot3 Not Fitted
--- | ---
Value | 213
Short description |

Each option module fitted in the drive is identified at power-up and the option fitted is stored by the drive in its non-volatile memory. If an option module was fitted in slot 3 at power-down, but that option module has subsequently been removed before power up then this trip is produced. The sub-trip number gives the identification code of the option module that has been removed. The priority order for the option module not fitted trips is Slot1 Not Fitted highest, then Slot2 Not Fitted, then Slot3 Not Fitted then Slot4 Not Fitted. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Ensure the option module is installed correctly.
- Re-install the option module.
- To confirm that the removed option module is no longer required perform a save function in Pr mm.000.

Trip | Slot3 Watchdog
--- | ---
Value | 211
Short description |

This trip indicates that the option module in option slot 3 has started the option watchdog function and then failed to service this watchdog correctly.

Recommended actions:

- Replace the option module.

Trip | Slot4 Different
--- | ---
Value | 254
Short description |

If the option module fitted in option slot 4 is different to the option module present at the last power-down then this trip is produced. The sub-trip number gives the identification code of the module that was originally fitted. The priority order for the option module different trips is Slot1 Different highest, then Slot2 Different, then Slot3 Different then Slot4 Different. Drive user parameters must be saved to prevent this trip on the next power-up if the module has changed. If the menus have been changed, but not the module, the trip will not occur on the next power-up. The sub-trip number gives the following indications of the reason for the trip.

Sub-trip | Reason
1 | No module was fitted previously
2 | A module with the same identifier is fitted, but the set-up menu for this option slot has been changed, and so default parameters have been loaded for this menu.
3 | A module with the same identifier is fitted, but the applications menu for this option slot has been changed, and so default parameters have been loaded for this menu.
4 | A module with the same identifier is fitted, but the set-up and applications menu for this option slot have been changed, and so default parameters have been loaded for these menus.
>99 | Shows the identifier of the module previously fitted.

Recommended actions:

- Turn off the power, ensure the correct option modules are installed in the correct option slots and re-apply the power.
- Confirm that the currently installed option module is correct, ensure option module parameters are set correctly and perform a user save in Pr mm.000.

Trip | Slot4 Error
--- | ---
Value | 252
Short description |

The option module in option slot 4 has indicated an error. The option module can give the reason for the error and this is shown in the sub-trip number. As default the sub-trip number is shown as a number on the display, however, it is possible for the option module to supply sub-trip number strings which will be displayed instead of the number if available.

Recommended actions:

- See relevant Option Module User Guide for details of the trip.

Trip | Slot4 HF
--- | ---
Value | 250
Short description |

This trip indicates that there is a fault with the option module in option slot 4 that means that this module cannot operate. The possible causes of the trip are given by the sub-trip value.

Sub-trip | Reason
1 | The module category cannot be identified
2 | All the required customisable menu table information has not been supplied or the tables supplied are corrupt
3 | There is insufficient memory available to allocate the comms buffers for this module.
4 | The module has not indicated that it is running correctly during drive power-up
5 | The module has been removed after power-up or it has ceased to indicate to the drive processor that it is still active.
6 | The module has not indicated that it has stopped accessing drive parameters during a drive mode change
7 | The module has failed to acknowledge that a request has been made to reset the drive processor.
8 | The drive failed to read correctly the menu table from the module during drive power-up.
9 | The drive failed to upload menu tables from the module and timed-out (5s).
10 | Menu table CRC invalid.

Recommended actions:

- Ensure the option module is installed correctly.
- Replace the option module.
- Replace the drive.

Trip | Slot4 Not Fitted
--- | ---
Value | 253
Short description |

Each option module fitted in the drive is identified at power-up and the option fitted is stored by the drive in its non-volatile memory. If an option module was fitted in slot 4 at power-down, but that option module has subsequently been removed before power up then this trip is produced. The sub-trip number gives the identification code of the option module that has been removed. The priority order for the option module not fitted trips is Slot1 Not Fitted highest, then Slot2 Not Fitted, then Slot3 Not Fitted then Slot4 Not Fitted. Drive user parameters must be saved to prevent this trip on the next power-up.

Recommended actions:

- Ensure the option module is installed correctly.
- Re-install the option module.
- To confirm that the removed option module is no longer required perform a save function in Pr mm.000.

Trip | Slot4 Watchdog
--- | ---
Value | 251
Short description |

This trip indicates that the option module in option slot 4 has started the option watchdog function and then failed to service this watchdog correctly.

Recommended actions:

- Replace the option module.

Trip | Slot App Menu
--- | ---
Value | 216
Short description |

This trip indicates that more than one option slot has requested to customize application menus 18, 19 and 20. The sub-trip number indicates which option slot has been allowed to customize the menus.

Recommended actions:

- Ensure that only one of the Application modules is configured to customize the application menus 18, 19 and 20.

Trip | Soft Start
--- | ---
Value | 226
Short description |

This trip indicates that the soft start relay in the drive has failed to close or the soft start monitoring circuit has failed.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Stored HF
--- | ---
Value | 221
Short description |

If an HF01 to HF19 trip occurs then a Stored HF trip occurs each time the drive is powered up until this trip is reset. The sub-trip code is the number of the original HF trip. The Stored HF trip can only be reset by first writing 1299 to Pr mm.000 and resetting the drive.

Recommended actions:

- Enter 1299 into Pr mm.000 and press reset to clear the trip.

Trip | Sub-array RAM
--- | ---
Value | 227
Short description |

An option module, derivative image or user program image has requested more parameter RAM than is allowed. The RAM allocation is checked in order of resulting sub-trip numbers, and so the failure with the highest sub-trip number is given. The sub-trip is calculated as (parameter size x 1000) + (parameter type x 100) + sub-array number. Note that if this trip occurs, all menu customisation provided by option modules, the derivative image or the user program image is not used. The tables below show the values corresponding to the parts of the sub-trip number.

Parameter size | Value
1 bit | 1
8 bit | 2
16 bit | 3
32 bit | 4
64 bit | 5

Parameter type | Value
Volatile | 0
User save | 1
Power-down save | 2

Sub-array | Menus | Value
Applications menus | 18-20 | 1
Derivative image | 29 | 2
User program image | 30 | 3
Option slot 1 set-up | 15 | 4
Option slot 1 applications | 25 | 5
Option slot 2 set-up | 16 | 6
Option slot 2 applications | 26 | 7
Option slot 3 set-up | 17 | 8
Option slot 3 applications | 27 | 9
Option slot 4 set-up | 24 | 10
Option slot 4 applications | 28 | 11

Trip | Temp Feedback
--- | ---
Value | 218
Short description |

This trip indicates a fault with a thermistor in the drive (i.e. open circuit or short circuit).

Source | xx | y | zz
Control board | 00 | 00 | 01: Control board thermistor 1 02: Control board thermistor 2 03: I/O board thermistor:
Power system | Power module number | 0 | Zero for temperature feedback provided via power system comms. 21, 22 and 23 for direct ELV temperature feedback.
Power system | 01 | Rectifier number* | Always zero

*For a parallel power-module system the rectifier number will be one as it is not possible to determine which rectifier has detected the fault.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | Th Brake Res
--- | ---
Value | 10
Short description |

If hardware based braking resistor thermal monitoring is provided and the resistor overheats this trip is initiated. If the braking resistor is not present then this trip must be disabled with bit 3 of Action On Trip Detection (10.037) to prevent this trip.

Recommended actions:

- Check braking resistor wiring.
- Check braking resistor value is greater than or equal to the minimum resistance value.
- Check braking resistor insulation.

Trip | Th Short Circuit
--- | ---
Value | 25
Short description |

This trip indicates that a temperature sensor connected to an analogue input or terminal 15 on the position feedback interface has a low impedance (i.e. < 50 Ohms). The cause of the trip can be identified by the sub-trip number.

Sub-trip | Source
1 | Analogue input 1
2 | Analogue input 2
3 | Analogue input 3
4 | Position feedback interface

Recommended actions:

- Check temperature feedback connection.
- Replace sensor.

Trip | Thermistor
--- | ---
Value | 24
Short description |

This trip indicates that a temperature sensor connected to one of the analogue inputs or terminal 15 on the position feedback interface (15 way D-type connector) has indicated an over-temperature. The source of the trip can be identified by the sub-trip number.

Sub-trip | Source
1 | Analogue input 1
2 | Analogue input 2
3 | Analogue input 3
4 | Position feedback interface

Recommended actions:

- Check why the temperature measured by the sensor is too high temperature.
- Check temperature sensor connection.

Trip | Undefined
--- | ---
Value | 110
Short description |

This trip indicates that the power system has generated but did not identify the trip from the power system. The cause of the trip is unknown.

Recommended actions:

- Hardware fault - contact the supplier of the drive.

Trip | User 24V
--- | ---
Value | 91
Short description |

This trip is initiatied if User Supply Select (06.072) = 1 or Low Under Voltage Threshold Select (06.067) = 1 or Backup Supply Mode Enable (06.068) = 1 and no user 24V present on the user 24V input.

Recommended actions:

- Ensure that the user 24V supply is present on the control terminals.

Trip | User Prog Trip
--- | ---
Value | 96
Short description |

This trip can be initiated from within an onboard user program using a function call which defines the sub-trip number.

Recommended actions:

- Check the user program.

Trip | User Program
--- | ---
Value | 249
Short description |

An error has been detected in the onboard user program image. The sub-trip indicated the reason for the trip.

Sub-trip | Reason | Comments
1 | Divide by zero |
2 | Undefined trip |
3 | Attempted fast parameter access set-up with non-existent parameter |
4 | Attempted access to non-existent parameter |
5 | Attempted write to read-only parameter |
6 | Attempted an over-range write |
7 | Attempted read from write-only parameter |
30 | The image has failed because either its CRC is incorrect, or there are less than 6 bytes in the image or the image header version is less than 5. | Occurs when the drive powers-up or the image is programmed. The image tasks will not run.
31 | The image requires more RAM for heap and stack than can be provided by the drive. | As 30.
32 | The image requires an OS function call that is higher than the maximum allowed. | As 30.
33 | The ID code within the image is not valid | As 30.
40 | The timed task has not completed in time and has been suspended. | Onboard User Program: Enable (11.047) is reset to zero when the trip is initiated.
41 | Undefined function called, i.e. a function in the host system vector table that has not been assigned. | As 40.
52 | Customisable menu table CRC check failed | As 30.
53 | Customisable menu table changed | Occurs when the drive powers-up or the image is programmed and the table has changed. Defaults are loaded for the user program menu and the trip will keep occurring until drive parameters are saved.
80 | *Image is not compatible with the control board | Initiated from within the image code.
81 | *Image is not compatible with the control board serial number | As 80.
100 | Image has detected and prevented attempted pointer access outside of the IEC task’s heap area. |
101 | Image has detected and prevented misaligned pointer usage. |
102 | Image has detected an array bounds violation and prevented its access. |
103 | Image has attempted to convert a data type to or from an unknown data type, has failed and has shut itself down. |
104 | Image has attempted to use an unknown user service function. |
200 | User program has invoked a “divide” service with a denominator of zero. (Note that this is raised by the downloaded image and has therefore been given a distinct error code despite being the same fundamental problem as sub-trip 1.) |
201 | Parameter access is not supported. An attempt to read database other than the host drive. |
202 | Parameter does not exist. Database was host drive but the specified parameter does not exist. |
203 | Parameter is read-only. |
204 | Parameter is write-only. |
205 | Unknown parameter error. |
206 | Invalid bit present in parameter. The parameter does not contain the specified bit. |
207 | Parameter format lookup failed. Failed to get parameter information data. |
208 | An over-range write has been attempted. |

The following table gives the differences when compared to the derivative product image.

Sub-trip | Difference
40, 41 | Onboard User Program: Enable (11.047) is reset to zero when the trip is initiated.
51 | Not applicable as core menu customisation not allowed
6x | Not applicable as option module restrictions not allowed
7x | Not applicable as option module restrictions not allowed
100 | Image has detected and prevented attempted pointer access outside of the IEC task’s heap area.
101 | Image has detected and prevented misaligned pointer usage.
102 | Image has detected an array bounds violation and prevented its access.
103 | Image has attempted to convert a data type to or from an unknown data type, has failed and has shut itself down.
104 | Image has attempted to use an unknown user service function.
200 | User program has invoked a “divide” service with a denominator of zero. (Note that this is raised by the downloaded image and has therefore been given a distinct error code despite being the same fundamental problem as sub-trip 1.)

Trip | User Save
--- | ---
Value | 36
Short description |

This trip indicates that an error has been detected in the user save parameters saved in non-volatile memory. For example, fillowing a user save command, if the power to the drive was removed when the user parameters were being saved.

Recommended actions:

- Perform a user save in Pr mm.000 to ensure that the trip doesn't occur the next time the drive is powered up.
- Ensure that the drive has enough time to complete the save before removing the power to the drive.

Trip | User Trip 40
--- | ---
Value | 40
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 41
--- | ---
Value | 41
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 42
--- | ---
Value | 42
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 43
--- | ---
Value | 43
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 44
--- | ---
Value | 44
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 45
--- | ---
Value | 45
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 46
--- | ---
Value | 46
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 47
--- | ---
Value | 47
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 48
--- | ---
Value | 48
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 49
--- | ---
Value | 49
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 50
--- | ---
Value | 50
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 51
--- | ---
Value | 51
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 52
--- | ---
Value | 52
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 53
--- | ---
Value | 53
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 54
--- | ---
Value | 54
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 55
--- | ---
Value | 55
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 56
--- | ---
Value | 56
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 57
--- | ---
Value | 57
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 58
--- | ---
Value | 58
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 59
--- | ---
Value | 59
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 60
--- | ---
Value | 60
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 61
--- | ---
Value | 61
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 62
--- | ---
Value | 62
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 63
--- | ---
Value | 63
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 64
--- | ---
Value | 64
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 65
--- | ---
Value | 65
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 66
--- | ---
Value | 66
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 67
--- | ---
Value | 67
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 68
--- | ---
Value | 68
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 69
--- | ---
Value | 69
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 70
--- | ---
Value | 70
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 71
--- | ---
Value | 71
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 72
--- | ---
Value | 72
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 73
--- | ---
Value | 73
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 74
--- | ---
Value | 74
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 75
--- | ---
Value | 75
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 76
--- | ---
Value | 76
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 77
--- | ---
Value | 77
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 78
--- | ---
Value | 78
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 79
--- | ---
Value | 79
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 80
--- | ---
Value | 80
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 81
--- | ---
Value | 81
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 82
--- | ---
Value | 82
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 83
--- | ---
Value | 83
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 84
--- | ---
Value | 84
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 85
--- | ---
Value | 85
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 86
--- | ---
Value | 86
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 87
--- | ---
Value | 87
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 88
--- | ---
Value | 88
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 89
--- | ---
Value | 89
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 112
--- | ---
Value | 112
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 113
--- | ---
Value | 113
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 114
--- | ---
Value | 114
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 115
--- | ---
Value | 115
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 116
--- | ---
Value | 116
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 117
--- | ---
Value | 117
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 118
--- | ---
Value | 118
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 119
--- | ---
Value | 119
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 120
--- | ---
Value | 120
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 121
--- | ---
Value | 121
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 122
--- | ---
Value | 122
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 123
--- | ---
Value | 123
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 124
--- | ---
Value | 124
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 125
--- | ---
Value | 125
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 126
--- | ---
Value | 126
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 127
--- | ---
Value | 127
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 128
--- | ---
Value | 128
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 129
--- | ---
Value | 129
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 130
--- | ---
Value | 130
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 131
--- | ---
Value | 131
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 132
--- | ---
Value | 132
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 133
--- | ---
Value | 133
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 134
--- | ---
Value | 134
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 135
--- | ---
Value | 135
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 136
--- | ---
Value | 136
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 137
--- | ---
Value | 137
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 138
--- | ---
Value | 138
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 139
--- | ---
Value | 139
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 140
--- | ---
Value | 140
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 141
--- | ---
Value | 141
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 142
--- | ---
Value | 142
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 143
--- | ---
Value | 143
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 144
--- | ---
Value | 144
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 145
--- | ---
Value | 145
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 146
--- | ---
Value | 146
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 147
--- | ---
Value | 147
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 148
--- | ---
Value | 148
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 149
--- | ---
Value | 149
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 150
--- | ---
Value | 150
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 151
--- | ---
Value | 151
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 152
--- | ---
Value | 152
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 153
--- | ---
Value | 153
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 154
--- | ---
Value | 154
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 155
--- | ---
Value | 155
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 156
--- | ---
Value | 156
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 157
--- | ---
Value | 157
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 158
--- | ---
Value | 158
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | User Trip 159
--- | ---
Value | 159
Short description |

This trip is not used by the drive and can be used for a user trip.

Trip | Voltage Range
--- | ---
Value | 169
Short description |

This trip is initiated if the Regen Minimum Voltage (03.026) is set to a non-zero value and the supply voltage is outside the range defined by Regen Maximum Voltage (03.027) for more than 100ms.

Recommended actions:

- Ensure the supply voltage is operating within the drive specification.
- Ensure Regen Minimum Voltage (03.026) and Regen Maximum Voltage (03.027) are set correctly.
- Check the supply voltage waveform using an oscilloscope.
- Reduce the level of supply disturbance.
- Set Regen Maximum Voltage (03.027) to zero to disable this trip.

Trip | Watchdog
--- | ---
Value | 30
Short description |

This trip indicates that the control word watchdog has been enabled and has timed out.