# Menu 35 Single Line Descriptions − AMC Cam

Mode: RFC‑S

Parameter | Range | Default | Type
--- | --- | --- | ---
35.001 | AMC Cam Start Index | 0 to 19 | 0 | RW | Num |  |  |  | US
35.002 | AMC Cam Start Position In Segment | 0 to VM_AMC_POSITION_UNIPOLAR UU | 0 UU | RW | Num |  |  |  | US
35.003 | AMC Cam Size | 1 to 20 | 1 | RW | Num |  |  |  | US
35.004 | AMC Cam Single Shot Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
35.005 | AMC Cam Output Ratio Numerator | 1 to 2147483647 | 1000 | RW | Num |  |  |  | US
35.006 | AMC Cam Output Ratio Denominator | 1 to 2147483647 | 1000 | RW | Num |  |  |  | US
35.007 | AMC Cam Index | 0 to 19 |  | RO | Num | ND | NC | PT |
35.008 | AMC Cam Position In Segment | 0 to VM_AMC_POSITION_UNIPOLAR UU |  | RO | Num | ND | NC | PT |
35.009 | AMC Cam Final Speed Coefficient | -21474836.48 to 21474836.47 UU |  | RO | Num | ND | NC | PT |
35.010 | AMC Cam Complete | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
35.011 | AMC Force CAM Repeat | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |