# Menu 19 − Application Menu 2

Mode: RFC‑S

See the introduction to menu 18.

Parameter | 19.001 Application Menu 2 Power-down Save Integer
--- | ---
Short description | General power-down save integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.002 Application Menu 2 Read-only Integer 2
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.003 Application Menu 2 Read-only Integer 3
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.004 Application Menu 2 Read-only Integer 4
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.005 Application Menu 2 Read-only Integer 5
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.006 Application Menu 2 Read-only Integer 6
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.007 Application Menu 2 Read-only Integer 7
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.008 Application Menu 2 Read-only Integer 8
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.009 Application Menu 2 Read-only Integer 9
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.010 Application Menu 2 Read-only Integer 10
--- | ---
Short description | General read-only integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 19.011 Application Menu 2 Read-write Integer 11
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.012 Application Menu 2 Read-write Integer 12
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.013 Application Menu 2 Read-write Integer 13
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.014 Application Menu 2 Read-write Integer 14
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.015 Application Menu 2 Read-write Integer 15
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.016 Application Menu 2 Read-write Integer 16
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.017 Application Menu 2 Read-write Integer 17
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.018 Application Menu 2 Read-write Integer 18
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.019 Application Menu 2 Read-write Integer 19
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.020 Application Menu 2 Read-write Integer 20
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.021 Application Menu 2 Read-write Integer 21
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.022 Application Menu 2 Read-write Integer 22
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.023 Application Menu 2 Read-write Integer 23
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.024 Application Menu 2 Read-write Integer 24
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.025 Application Menu 2 Read-write Integer 25
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.026 Application Menu 2 Read-write Integer 26
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.027 Application Menu 2 Read-write Integer 27
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.028 Application Menu 2 Read-write Integer 28
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.029 Application Menu 2 Read-write Integer 29
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.030 Application Menu 2 Read-write Integer 30
--- | ---
Short description | General read-write integer application parameter
Mode | RFC‑S
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.031 Application Menu 2 Read-write bit 31
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.032 Application Menu 2 Read-write bit 32
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.033 Application Menu 2 Read-write bit 33
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.034 Application Menu 2 Read-write bit 34
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.035 Application Menu 2 Read-write bit 35
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.036 Application Menu 2 Read-write bit 36
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.037 Application Menu 2 Read-write bit 37
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.038 Application Menu 2 Read-write bit 38
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.039 Application Menu 2 Read-write bit 39
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.040 Application Menu 2 Read-write bit 40
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.041 Application Menu 2 Read-write bit 41
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.042 Application Menu 2 Read-write bit 42
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.043 Application Menu 2 Read-write bit 43
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.044 Application Menu 2 Read-write bit 44
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.045 Application Menu 2 Read-write bit 45
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.046 Application Menu 2 Read-write bit 46
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.047 Application Menu 2 Read-write bit 47
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.048 Application Menu 2 Read-write bit 48
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.049 Application Menu 2 Read-write bit 49
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.050 Application Menu 2 Read-write bit 50
--- | ---
Short description | General read-write bit application parameter
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.051 Application Menu 2 Power-down Save Long Integer 51
--- | ---
Short description | General power-down save long integer application parameter
Mode | RFC‑S
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.052 Application Menu 2 Power-down Save Long Integer 52
--- | ---
Short description | General power-down save long integer application parameter
Mode | RFC‑S
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.053 Application Menu 2 Power-down Save Long Integer 53
--- | ---
Short description | General power-down save long integer application parameter
Mode | RFC‑S
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 19.054 Application Menu 2 Power-down Save Long Integer 54
--- | ---
Short description | General power-down save long integer application parameter
Mode | RFC‑S
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW