# Menu 20 Single Line Descriptions − Application Menu 3

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
20.001 | Application Menu 3 Read‑write Integer 1 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.002 | Application Menu 3 Read‑write Integer 2 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.003 | Application Menu 3 Read‑write Integer 3 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.004 | Application Menu 3 Read‑write Integer 4 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.005 | Application Menu 3 Read‑write Integer 5 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.006 | Application Menu 3 Read‑write Integer 6 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.007 | Application Menu 3 Read‑write Integer 7 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.008 | Application Menu 3 Read‑write Integer 8 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.009 | Application Menu 3 Read‑write Integer 9 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.010 | Application Menu 3 Read‑write Integer 10 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.011 | Application Menu 3 Read‑write Integer 11 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.012 | Application Menu 3 Read‑write Integer 12 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.013 | Application Menu 3 Read‑write Integer 13 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.014 | Application Menu 3 Read‑write Integer 14 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.015 | Application Menu 3 Read‑write Integer 15 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.016 | Application Menu 3 Read‑write Integer 16 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.017 | Application Menu 3 Read‑write Integer 17 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.018 | Application Menu 3 Read‑write Integer 18 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.019 | Application Menu 3 Read‑write Integer 19 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.020 | Application Menu 3 Read‑write Integer 20 | -32768 to 32767 | 0 | RW | Num |  |  |  |
20.021 | Application Menu 3 Read‑write Long Integer 21 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.022 | Application Menu 3 Read‑write Long Integer 22 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.023 | Application Menu 3 Read‑write Long Integer 23 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.024 | Application Menu 3 Read‑write Long Integer 24 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.025 | Application Menu 3 Read‑write Long Integer 25 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.026 | Application Menu 3 Read‑write Long Integer 26 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.027 | Application Menu 3 Read‑write Long Integer 27 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.028 | Application Menu 3 Read‑write Long Integer 28 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.029 | Application Menu 3 Read‑write Long Integer 29 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.030 | Application Menu 3 Read‑write Long Integer 30 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.031 | Application Menu 3 Read‑write Long Integer 31 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.032 | Application Menu 3 Read‑write Long Integer 32 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.033 | Application Menu 3 Read‑write Long Integer 33 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.034 | Application Menu 3 Read‑write Long Integer 34 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.035 | Application Menu 3 Read‑write Long Integer 35 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.036 | Application Menu 3 Read‑write Long Integer 36 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.037 | Application Menu 3 Read‑write Long Integer 37 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.038 | Application Menu 3 Read‑write Long Integer 38 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.039 | Application Menu 3 Read‑write Long Integer 39 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |
20.040 | Application Menu 3 Read‑write Long Integer 40 | -2147483648 to 2147483647 | 0 | RW | Num |  |  |  |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |