# Slot 4 Menu 0 − Ethernet Setup

Mode: Regeneration

Parameter | 4.00.001 Module ID
--- | ---
Short description | Module ID
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

The Module ID. Ethernet Factory Fit Module (FFM) = 430.

Parameter | 4.00.002 Software Version
--- | ---
Short description | Software Version
Minimum | 0 | Maximum | 99999999
Default |  | Units |
Type | 32 Bit Volatile | Update Rate |
Display Format | Version | Decimal Places | 0
Coding | RO, ND, NC, PT

Module firmare version in ww.xx.yy.zz format

Parameter | 4.00.003 Hardware Version
--- | ---
Short description | Hardware Version
Minimum | 0.00 | Maximum | 99.99
Default |  | Units |
Type | 16 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 2
Coding | RO, ND, NC, PT

Contains the module’s hardware version information in the format xx.yy.

Parameter | 4.00.004 Serial Number LS
--- | ---
Short description | Serial Number LS
Minimum | 0 (Display: 00000000) | Maximum | 99999999 (Display: 99999999)
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | Power-up write
Display Format | Lead Zero Pad | Decimal Places | 0
Coding | RO, ND, NC, PT

The module serial number is available as a pair of 32 bit values where Serial Number LS (MM.004) provides the least significant 8 decimal digits and Serial Number MS (MM.005) provides the most significant 8 decimal digits. The reconstructed serial number is ((MM.005* 100000000) + MM.004). For example serial number "0001234567898765" would be stored as MM.005 = 12345, MM.004 = 67898765.

Parameter | 4.00.005 Serial Number MS
--- | ---
Short description | Serial Number MS
Minimum | 0 | Maximum | 99999999
Default |  | Units |
Type | 32 Bit Volatile | Update Rate | Power-up write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Serial Number LS (MM.004).

Parameter | 4.00.006 Status
--- | ---
Short description | Status
Minimum | -2 | Maximum | 3
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Background
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT

Value | Text | Description
‑2 | Bootldr - Update | The bootloader is performing a flash update
‑1 | Bootldr - Idle | The bootloader is idle
0 | Initialising |
1 | OK | Module is initialised with no errors present
2 | Config | A configuration error has been detected
3 | Error | An error has occured preventing the module from running correctly

Parameter | 4.00.007 Reset
--- | ---
Short description | Reset
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | Read every 200ms, Written to 0 on module initialisation
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

When set the module performs a warm reset. When the reset has been performed and the module is performing its initialization routines the parameter will be cleared to zero. Note: The drive, and any other modules fitted to the drive will not be affected by the reset.

Parameter | 4.00.008 Default
--- | ---
Short description | Default
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | Read every 200ms, Written to 0 on module initialisation
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

If set to “ON” when the module is reset, this parameter will cause the option module to return to its "Out of Box configuration" any settings stored on the module will be returned to their default values. This will include any Web page customisations, e-mail settings etc. Following the default the module will set the parameter to "OFF" and the module will reset.

Take care using this parameter as any configuration information will be irretrievably lost!

Note: The password for the ‘root’ account is not reset back to default.

Parameter | 4.00.009 Active Alarm Bits
--- | ---
Short description |
Minimum | 0 (Display: 0000000000000000) | Maximum | 65535 (Display: 1111111111111111)
Default | 0 (Display: 0000000000000000) | Units |
Type | 16 Bit Volatile | Update Rate | Background
Display Format | Binary | Decimal Places | 0
Coding | RO, NC, BU

Bit | Alarm
0 | User Program
1 | eCMP
2 | Modbus
3 | Ethernet/IP
4 | Reserved
5 | Filesystem
6 | Too Hot

Parameter | 4.00.010 Active IP Address
--- | ---
Short description |
Minimum | -2147483648 (Display: 128.0.0.0) | Maximum | 2147483647 (Display: 127.255.255.255)
Default | 0 (Display: 0.0.0.0) | Units |
Type | 32 Bit Volatile | Update Rate | Background
Display Format | IP Address | Decimal Places | 0
Coding | RO, NC, PT

Modules active IP address.

Parameter | 4.00.011 Date Code
--- | ---
Short description |
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | Background
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

Date Code (4.0.011) is a two-digit number in the form yyww where yy is the year and ww the week number.

Parameter | 4.00.054 Drive Date Code
--- | ---
Short description |
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Volatile | Update Rate |
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU