# Menu 24 Single Line Descriptions − Ethernet Setup

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
24.001 | Module ID | 0 to 65535 |  | RO | Num | ND | NC | PT |
24.002 | Software Version | 0 to 99999999 |  | RO | Num | ND | NC | PT |
24.003 | Hardware Version | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
24.004 | Serial Number LS | 00000000 to 99999999 |  | RO | Num | ND | NC | PT |
24.005 | Serial Number MS | 0 to 99999999 |  | RO | Num | ND | NC | PT |
24.006 | Status | Bootldr ‑ Update (‑2), Bootldr ‑ Idle (‑1), Initialising (0), OK (1), Config (2), Error (3) |  | RO | Txt | ND | NC | PT |
24.007 | Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
24.008 | Default | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
24.009 | Active Alarm Bits | 0000000000000000 to 1111111111111111 | 0000000000000000 | RO | Bin |  | NC |  |
24.010 | Active IP Address | 128.0.0.0 to 127.255.255.255 | 0.0.0.0 | RO | IP |  | NC | PT |
24.011 | Date Code | 0 to 65535 |  | RO | Num | ND | NC | PT |
24.054 | Drive Date Code | 0 to 65535 |  | RO | Num | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |