# Slot 4 Menu 10 Single Line Descriptions − Easy Mode Cyclic Data

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
4.10.001 | Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
4.10.002 | Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
4.10.003 | Default | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
4.10.004 | Cyclic Messages Per Second | 0 to 65535 |  | RO | Num | ND | NC | PT |
4.10.005 | Configuration Valid | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
4.10.006 | Operational | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
4.10.007 | Active Configuration | None (0), Easy Mode (1), Offline (2) |  | RO | Txt | ND | NC | PT |
4.10.008 | Timeout Count | 0 to 65535 |  | RO | Num | ND | NC | PT |
4.10.009 | Data Late Count | 0 to 65535 |  | RO | Num | ND | NC | PT |
4.10.010 | Tx1 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.011 | Tx1 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.012 | Tx1 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
4.10.013 | Tx1 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.014 | Tx1 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
4.10.015 | Tx1 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
4.10.016 | Tx1 Message Rate | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
4.10.019 | Tx1 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
4.10.020 | Tx2 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.021 | Tx2 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.022 | Tx2 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
4.10.023 | Tx2 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.024 | Tx2 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
4.10.025 | Tx2 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
4.10.026 | Tx2 Message Rate | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
4.10.029 | Tx2 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
4.10.030 | Tx3 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.031 | Tx3 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.032 | Tx3 Source Parameter | 0 to 499999 | 0 | RW | Num |  |  | PT | US
4.10.033 | Tx3 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.034 | Tx3 Link Transmission Type | Unicast (0), Broadcast (1), Multicast1 (2), Multicast2 (3), Multicast3 (4), Multicast4 (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Unicast (0) | RW | Txt |  |  |  | US
4.10.035 | Tx3 Destination Address | 0.0.0.0 to 255.255.255.255 | 0.0.0.0 | RW | IP |  |  |  | US
4.10.036 | Tx3 Message Rate | 0 to 100 ms | 0 ms | RW | Num |  |  |  | US
4.10.039 | Tx3 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
4.10.040 | Rx1 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.041 | Rx1 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.042 | Rx1 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
4.10.043 | Rx1 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.044 | Rx1 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
4.10.045 | Rx1 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
4.10.046 | Rx1 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
4.10.047 | Rx1 Timeout Event Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.10.048 | Rx1 Timeout Event Type | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US
4.10.049 | Rx1 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
4.10.050 | Rx2 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.051 | Rx2 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.052 | Rx2 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
4.10.053 | Rx2 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.054 | Rx2 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
4.10.055 | Rx2 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
4.10.056 | Rx2 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
4.10.057 | Rx2 Timeout Event Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.10.058 | Rx2 Timeout Event Type | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US
4.10.059 | Rx2 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |
4.10.060 | Rx3 Link Profile | Std (0), Sync (1) | Std (0) | RW | Txt |  |  |  | US
4.10.061 | Rx3 Link Number | 0 to 255 | 0 | RW | Num |  |  |  | US
4.10.062 | Rx3 Destination Parameter | 0 to 499999 | 0 | RW | Num |  |  |  | US
4.10.063 | Rx3 Parameter Count | 0 to 10 | 0 | RW | Num |  |  |  | US
4.10.064 | Rx3 Source Type | Direct (0), Multicast1 (1), Multicast2 (2), Multicast3 (3), Multicast4 (4), Local (5), Multicast5 (6), Multicast6 (7), Multicast7 (8), Multicast8 (9), Multicast9 (10), Multicast10 (11) | Direct (0) | RW | Txt |  |  |  | US
4.10.065 | Rx3 Timeout | 0 to 65535 ms | 100 ms | RW | Num |  |  |  | US
4.10.066 | Rx3 Timeout Action | Trip (0), Clear output (1), Hold last (2) | Trip (0) | RW | Txt |  |  |  | US
4.10.067 | Rx3 Timeout Event Destination | This slot (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) | This slot (0) | RW | Txt |  |  |  | US
4.10.068 | Rx3 Timeout Event Type | No Event (0), Event (1), Event1 (2), Event2 (3), Event3 (4) | No Event (0) | RW | Txt |  |  |  | US
4.10.069 | Rx3 Link Status | VLAN disabled (‑30), Reserved 29 (‑29), Reserved 28 (‑28), Reserved 27 (‑27), Reserved 26 (‑26), Reserved 25 (‑25), Reserved 24 (‑24), Reserved 23 (‑23), Invalid DST IP (‑22), SYNC unsupported (‑21), MEC offset (‑20), Invalid tx rate (‑19), Too many mapping (‑18), Link busy (‑17), Invalid profile (‑16), Invalid mapping (‑15), Read only param (‑14), Msg mismatch (‑13), Msg too long (‑12), Attrib NA (‑11), Attrib RO (‑10), Attrib missing (‑9), Timeout (‑8), In error (‑7), Link num in use (‑6), Not editable (‑5), Invalid link num (‑4), Invalid args (‑3), Too many links (‑2), Out of memory (‑1), OK (0), Not running (1), OK sync (2) |  | RO | Txt | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |