# Slot 4 Menu 2 − Ethernet Configuration

Mode: Regeneration

Note: The maximum Ethernet packet size is 400 bytes.

Parameter | 4.02.003 Network Status
--- | ---
Short description | Shows the module status
Minimum | 0 | Maximum | 5
Default |  | Units |
Type | 8 Bit Volatile | Update Rate | Written every second
Display Format | Standard | Decimal Places | 0
Coding | RO, TE, ND, NC, PT, BU

Value | Text | Description
0 | Initialising | The network interface is being initialised
1 | Links Down | No link connection has been detected on either of the Ethernet ports
2 | DHCP In Progress | The module is apptempting to obtain an IP address, subnet mask, default gateway and DNS server addresses from a DHCP server
3 | No Address | The module does not have an IP address - either the user has not provided one manually or one could not be allocated via DHCP
4 | Ready | The network interface has been successfully configured but no data is being received or transmitted
5 | Active | The network interface is receiving or transmitting data

This parameter indicates the status of the network that the module is connected to.

Parameter | 4.02.004 Network Message Count
--- | ---
Short description | Shows the number of messages per second
Minimum | 0 | Maximum | 65535
Default |  | Units | Messages/s
Type | 16 Bit Volatile | Update Rate | Written every second
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

The number of frames that the module is transmitting / receiving every second.

Parameter | 4.02.005 DHCP Enable
--- | ---
Short description | Set to enable DHCP
Minimum | 0 | Maximum | 1
Default | 1 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

Controls whether or not the module will attempt to use a Dynamic Host Configuration Protocol (DHCP) server to obtain an IP address, subnet mask, default gateway and DNS servers.

When DHCP is enabled, the following parameters will become read-only immediately (no reset required):

IP Address (4.02.006)

Subnet Mask (4.02.007)

Default Gateway (4.02.008)

Primary DNS (4.02.009)
Secondary DNS (4.02.010)

Parameter | 4.02.006 IP Address
--- | ---
Short description | Sets and/or shows the IP address of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default | 3232235876 (Display: 192.168.1.100) | Units |
Type | 32 Bit User Save | Update Rate | DHCP enabled : write on event; DHCP disabled : read on reset
Display Format | IP Address | Decimal Places | 0
Coding | RW, BU

Controls and displays the IP address of the module.

If DHCP is enabled ( DHCP Enable (4.02.005) ) this parameter becomes read-only and, until an IP address is allocated to the module, will display 0.0.0.0.

If DHCP is disabled the module will initialise, on reset or power cycle, with the IP address stored for the parameter.

Parameter | 4.02.007 Subnet Mask
--- | ---
Short description | Sets and/or shows the subnet mask of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default | 4294967040 (Display: 255.255.255.0) | Units |
Type | 32 Bit User Save | Update Rate | DHCP enabled : write on event; DHCP disabled : read on reset
Display Format | IP Address | Decimal Places | 0
Coding | RW, BU

Controls and displays the subnet mask of the module.

If DHCP is enabled ( DHCP Enable (4.02.005) ) this parameter becomes read-only and, until a subnet mask is allocated to the module, will display 0.0.0.0.

If DHCP is disabled the module will initialise, on reset or power cycle, with the subnet mask stored for the parameter.

Parameter | 4.02.008 Default Gateway
--- | ---
Short description | Sets and/or shows the default gateway of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default | 3232236030 (Display: 192.168.1.254) | Units |
Type | 32 Bit User Save | Update Rate | DHCP enabled : write on event; DHCP disabled : read on reset
Display Format | IP Address | Decimal Places | 0
Coding | RW, BU

Controls and displays the default gateway of the module.

If DHCP is enabled ( DHCP Enable (4.02.005) ) this parameter becomes read-only and, until a default gateway is allocated to the module, will display 0.0.0.0.

If DHCP is disabled the module will initialise, on reset or power cycle, with the default gateway stored for the parameter.

Parameter | 4.02.009 Primary DNS
--- | ---
Short description | Sets and/or shows the primary DNS address of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default | 0 (Display: 0.0.0.0) | Units |
Type | 32 Bit User Save | Update Rate | DHCP enabled : write on event; DHCP disabled : read on reset
Display Format | IP Address | Decimal Places | 0
Coding | RW, BU

The module can use this IP address when it wishes to resolve the IP address for a domain name. This parameter performs the same function as the Secondary DNS parameter Secondary DNS (4.02.010) , however the address specified in this parameter will be tried first. Only when this address is unsuccessful will the Secondary DNS address be tried.

If DHCP is enabled ( DHCP Enable (4.02.005) ) this parameter becomes read-only and, until a primary DNS address is allocated to the module, will display 0.0.0.0.

If DHCP is disabled the module will initialise, on reset or power cycle, with the primary DNS address stored for the parameter.

Parameter | 4.02.010 Secondary DNS
--- | ---
Short description | Sets and/or shows the secondary DNS address of the module
Minimum | 0 (Display: 0.0.0.0) | Maximum | 4294967295 (Display: 255.255.255.255)
Default | 0 (Display: 0.0.0.0) | Units |
Type | 32 Bit User Save | Update Rate | DHCP enabled : write on event; DHCP disabled : read on reset
Display Format | IP Address | Decimal Places | 0
Coding | RW, BU

The module can use this IP address when it wishes to resolve the IP address for a domain name. This parameter performs the same function as the Primary DNS parameter Primary DNS (4.02.009) , however the address specified in this parameter will be tried only when the Primary DNS address is unsuccessful.

If DHCP is enabled ( DHCP Enable (4.02.005) ) this parameter becomes read-only and, until a secondary DNS address is allocated to the module, will display 0.0.0.0.

If DHCP is disabled the module will initialise, on reset or power cycle, with the secondary DNS address stored for the parameter.

Parameter | 4.02.011 MAC Address
--- | ---
Short description | Shows the MAC address of the module
Minimum | 0 (Display: 00:00:00:00:00:00) | Maximum | 281474976710655 (Display: FF:FF:FF:FF:FF:FF)
Default |  | Units |
Type | 64 Bit Volatile | Update Rate | Power-up write
Display Format | MAC Address | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

The 48-bit MAC address of the module.

Parameter | 4.02.020 Priority Protocol
--- | ---
Short description | Sets the Priority Protocol
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE, BU

Selection of the fieldbus protocol to have priority over all other protocols.

Value | Text | Description
0 | None | All protocols have equal priority
1 | Modbus TCP | Modbus TCP has highest priority
2 | EtherNet/IP | EtherNet/IP has highest priority

Enables selection of one fieldbus protocol to have priority over others. A tick period of 1 ms will be given to the highest priority fieldbus protocol, 5 ms to all other fieldbus protocols (equal priority).

If no fieldbus protocol has been selected to have priority over others all protocols will have equal priority and a tick rate of 5 ms.

Parameter | 4.02.021 Web Server Enable
--- | ---
Short description | Enables the Web Server
Minimum | 0 | Maximum | 1
Default | 1 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

Controls the running of the webserver on the module.

Parameter | 4.02.022 Web Server Port
--- | ---
Short description | Specifies the web server port
Minimum | 0 | Maximum | 65535
Default | 80 | Units |
Type | 16 Bit User Save | Update Rate | Read on module reset and HTTP_ENABLE
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

The web server port. This may be changed for added security.

Parameter | 4.02.024 Ethernet MTU
--- | ---
Short description | Specifies the MTU for the Ethernet interface
Minimum | 158 | Maximum | 1500
Default | 1500 | Units | Bytes
Type | 16 Bit User Save | Update Rate | Read on module reset
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

This parameter is now deprecated. The maximum Ethernet packet size is now 400 bytes.

Parameter | 4.02.025 Gateway Mode
--- | ---
Short description | Specifies the operation mode of the gateway
Minimum | 0 | Maximum | 2
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Read on module reset
Display Format | Standard | Decimal Places | 0
Coding | RW, TE, BU

Value | Text
0 | Switch
1 | Gateway
2 | Strict Gateway

Specifies the operation mode of the gateway. By default the gateway is disabled and the switch operates in normal switch mode, by enabling the gateway mode all packets are filtered by the module and prioritised before being forwarded on. In strict mode the gateway will drop packets from unsupported protocols.

VLAN must be enabled VLAN Enable (4.02.030) when the gateway is enabled.

Parameter | 4.02.030 VLAN Enable
--- | ---
Short description | Enables VLAN tagging
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Read on module reset
Display Format | Standard | Decimal Places | 0
Coding | RW

Controls whether the module will use VLAN tagging.

When used in conjunction with Drive VLAN ID (4.02.031) network traffic from the interface will be tagged with the chosen VLAN identifier.

When default values for Drive VLAN ID (4.02.031) is set, enabling this parameter will add VLAN prioritisation to all packets helping to ensure real-time packets are not delayed by those of lower priority. If disabled, prioritisation will use the Diffserv field in IP traffic only, meaning non-IP traffic can still affect real-time IP traffic.

Parameter | 4.02.031 Drive VLAN ID
--- | ---
Short description | Specifies a VLAN ID that the drive (Port 0) will be a member of
Minimum | 0 | Maximum | 255
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Read on module reset and VLAN_ENABLE
Display Format | Standard | Decimal Places | 0
Coding | RW, BU

Specifies the VLAN ID that the interface will be a member of. Any packets entering the switch without this VLAN ID will not be handled.

Parameter | 4.02.034 Drive compatibility mode
--- | ---
Short description | Specifies the mimic of the GT8 from a PLC for EthernetIP and Modbus
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Read on module reset
Display Format | Standard | Decimal Places | 0
Coding | RW, TE, BU

Defines the parameter conversion for EthernetIP and Modbus.

Value | Text
0 | Unidrive M
1 | Unidrive SP

Parameter | 4.02.035 Non cyclic enable
--- | ---
Short description | Specify non cyclic enable
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background
Display Format | Standard | Decimal Places | 0
Coding | RW

Enable the Non cyclic data transfer.

Parameter | 4.02.036 Non cyclic base parameter
--- | ---
Short description | Specify the base parameter of the user program non cyclic handling
Minimum | 0 | Maximum | 59999
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | Background
Display Format | Slot Menu Parameter | Decimal Places | 0
Coding | RW, BU

The value in this parameter points to the base address of a group of parameters which used for handling non cyclic data by user programs.

Suppose the base address is S.MM.PPP, the following are the functions of the group of the parameters. Please note that these parameters should be at least 16 bits in size.

Parameter | S.MM.PPP
Description | Command and Status
Identifier |
Mode(s) |
Minimum | 0 | Maximum | 0x0403
Default | 0 | Units |
Type | 16 bit user save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 0 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 1
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 0 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 1

The MSB is used for Status and the LSB is used for Command.

Possible values for the Command are:

Value | Meaning | Description
0 | No Command | No command or Abort during a command process
1 | Check / Abort | Check if the status idle or abort from read or write command.
2 | Read | Read one parameter
3 | Write | Write one parameter

Possible values for the Status are:

Value | Meaning | Description
0 | IDLE | Idle
1 | READY | The parameter channel is ready to take commands
2 | PROCESSING | Processing the command
3 | OK | The command processed successfully
4 | ERROR | Error is detected, detail will be found in the first parameter.

Parameter | S.MM.PPP + 1
Description | Destination IP Address www.xxx
Identifier |
Mode(s) |
Minimum | 0 | Maximum | 0xFFFF
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 0 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 1 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 1

The higher two sections for the destination IP address. 0xFF000000 (127.0.0.1) represents the current drive.

Parameter | S.MM.PPP + 2
Description | Destination IP Address yyy.zzz
Identifier |
Mode(s) |
Minimum | 0 | Maximum | 0xFFFF
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 0 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 1 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 1

The lower two sections for the destination IP address

Parameter | S.MM.PPP + 3
Description | Parameter Address SMM
Identifier |
Mode(s) |
Minimum | 0 | Maximum | 499
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 0 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 0 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 1

Destination parameter address – Slot and Menu sections.

Parameter | S.MM.PPP + 4
Description | Parameter Address PPP
Identifier |
Mode(s) |
Minimum | 0 | Maximum | 999
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 0 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 0 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 1

Destination parameter address - parameter section

Parameter | S.MM.PPP + 5
Description | Parameter Value LSW / Error Code
Identifier |
Mode(s) |
Minimum | -215 | Maximum | 215-1
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 4 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 0 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 0

It stores the least significant word of the value to be write in to the destination parameter if the command is Write (2)

It stores the least significant word of the value read from the destination parameter if the command is read and the status is Done.

It is the error code for the process if the status is Error.

The following table list the possible error codes:

Value | Meaning | Description
-1 | Address Type | The addressing type is not supported
-2 | Timeout | A timeout occurred trying to access the specified item
-3 | Access Denied | The requesting device does not have sufficient access rights
-4 | Does not exist | The specified item does not exist
-5 | Data Type | The data could not be converted from the specified type
-6 | Failed Read | The value could not be read, reason unknown
-7 | Failed Write | The value could not be written, reason unknown
-8 | Not Readable | The data could not be read as the source does not allow read access.
-9 | Not Writeable | The data could not be written as the destination does not allow write access.
-10 | Over Range | The specified value is outside the suitable range for the item.
-11 | Request Invalid | The request contained invalid information.
-12 | Response Too Big | The response will not fit in the maximum response size.
-13 | Decimal Place | The decimal place information is invalid (i.e. out of range of allowed values for a write).
-14 | Invalid Param | Invalid parameter in the parameter channel.
-15 | Invalid CMD | Invalid command
-16 | Invalid IP | Invalid IP address
-17 | Unknown Error | An unknown error happens
-18 to -128 | Reserved |

Parameter | S.MM.PPP + 6
Description | Parameter Value MSW
Identifier |
Mode(s) |
Minimum | -215 | Maximum | 215-1
Default | 0 | Units |
Type | 16 Bit User Save | Update rate |

|  | FL | Floating point parameter | 0 | ND | No default | 0
|  | DF | Display format | 4 | RA | Rating dependent | 0
|  | PR | Pseudo read-only | 0 | NC | Not clonable | 0
|  | FI | Filtered | 0 | NV | Not visible | 0
|  | DE | Destination parameter | 0 | PT | Protected | 0
|  | TE | Text parameter | 0 | NR | Not readable | 0
|  | VM | Variable minimum/maximum | 0 | W | Writable | 1
UNIT | 0 | DP | Decimal places | 0 | BU | Default (1 bit types) / Unipolar (all other types): | 0

It stores the most significant word of the value to be write in to the destination parameter if the command is Write (2)

It stores the most significant word of the value read from the destination parameter if the command is read and the status is Done.