# Menu 1 Single Line Descriptions − Frequency References

Parameter | Range | Default | Type
--- | --- | --- | ---
01.001 | Reference Selected | ±VM_SPEED_FREQ_REF Hz |  | RO | Num | ND | NC | PT |
01.002 | Pre‑skip Filter Reference | ±VM_SPEED_FREQ_REF Hz |  | RO | Num | ND | NC | PT |
01.003 | Pre‑ramp Reference | ±VM_SPEED_FREQ_REF Hz |  | RO | Num | ND | NC | PT |
01.004 | Reference Offset | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.005 | Jog Reference | 0.00 to 300.00 Hz | 1.50 Hz | RW | Num |  |  |  | US
01.006 | Maximum Reference Clamp | ±VM_POSITIVE_REF_CLAMP Hz | 50Hz: 50.00 Hz 60Hz: 60.00 Hz | RW | Num |  |  |  | US
01.007 | Minimum Reference Clamp | ±VM_NEGATIVE_REF_CLAMP1 Hz | 0.00 Hz | RW | Num |  |  |  | US
01.008 | Negative Reference Clamp Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
01.009 | Reference Offset Select | 0 to 2 | 0 | RW | Num |  |  |  | US
01.010 | Bipolar Reference Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
01.011 | Reference On | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
01.012 | Reverse Select | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
01.013 | Jog Select | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
01.014 | Reference Selector | A1.A2 (0), A1.Pr (1), A2.Pr (2), Preset (3), Pad (4), Res (5), Pad.Ref (6) | A1.A2 (0) | RW | Txt |  |  |  | US
01.015 | Preset Selector | 0 to 9 | 0 | RW | Num |  |  |  | US
01.016 | Preset Selector Timer | 0.0 to 400.0 s | 10.0 s | RW | Num |  |  |  | US
01.017 | Keypad Control Mode Reference | ±VM_SPEED_FREQ_USER_REFS Hz | 0.00 Hz | RO | Num |  | NC | PT | PS
01.021 | Preset Reference 1 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.022 | Preset Reference 2 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.023 | Preset Reference 3 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.024 | Preset Reference 4 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.025 | Preset Reference 5 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.026 | Preset Reference 6 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.027 | Preset Reference 7 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.028 | Preset Reference 8 | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RW | Num |  |  |  | US
01.029 | Skip Reference 1 | 0.00 to 550.00 Hz | 0.00 Hz | RW | Num |  |  |  | US
01.030 | Skip Reference Band 1 | 0.00 to 25.00 Hz | 0.50 Hz | RW | Num |  |  |  | US
01.031 | Skip Reference 2 | 0.00 to 550.00 Hz | 0.00 Hz | RW | Num |  |  |  | US
01.032 | Skip Reference Band 2 | 0.00 to 25.00 Hz | 0.50 Hz | RW | Num |  |  |  | US
01.033 | Skip Reference 3 | 0.00 to 550.00 Hz | 0.00 Hz | RW | Num |  |  |  | US
01.034 | Skip Reference Band 3 | 0.00 to 25.00 Hz | 0.50 Hz | RW | Num |  |  |  | US
01.035 | Reference In Rejection Zone | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
01.036 | Analog Reference 1 | ±VM_SPEED_FREQ_USER_REFS Hz | 0.00 Hz | RO | Num |  | NC |  |
01.038 | Percentage Trim | ±100.00 % | 0.00 % | RW | Num |  | NC |  |
01.042 | Reference Select Flag 2 | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.043 | Reference Select Flag 3 | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.045 | Preset Select Flag 1 | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.046 | Preset Select Flag 2 | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.047 | Preset Select Flag 3 | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.048 | Preset Selector Timer Reset | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
01.049 | Reference Selected Indicator | 1 to 6 |  | RO | Num | ND | NC | PT |
01.050 | Preset Selected Indicator | 1 to 8 |  | RO | Num | ND | NC | PT |
01.051 | Power‑up Keypad Control Mode Reference | Reset (0), Last (1), Preset (2) | Reset (0) | RW | Txt |  |  |  | US
01.057 | Force Reference Direction | None (0), For (1), Rev (2) | None (0) | RW | Txt |  |  |  |
01.069 | Reference in rpm | ±VM_SPEED_FREQ_REF rpm |  | RO | Num | ND | NC | PT |
01.070 | Clamped Reference | ±VM_SPEED_FREQ_REF Hz |  | RO | Num | ND | NC | PT |
01.071 | Alternative Reference | ±VM_SPEED_FREQ_REF Hz | 0.00 Hz | RO | Num |  | NC |  |
01.072 | Alternative Reference Enable | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |