# Menu 6 Single Line Descriptions − Sequencer and Clock

Parameter | Range | Default | Type
--- | --- | --- | ---
06.001 | Stop Mode | Coast (0), rp (1), rP.dcI (2), dc I (3), td.dcI (4), Dis (5) | rp (1) | RW | Txt |  |  |  | US
06.002 | Limit Switch Stop Mode | Stop (0), rp (1) | rp (1) | RW | Txt |  |  |  | US
06.003 | Supply Loss Mode | Dis (0), rP.Stop (1), ridE.th (2) | Dis (0) | RW | Txt |  |  |  | US
06.004 | Start/Stop Logic Select | 0 to 6 | 50Hz: 0 60Hz: 4 | RW | Num |  |  |  | US
06.006 | Injection Braking Level | 0.0 to 150.0 % | 100.0 % | RW | Num |  | RA |  | US
06.007 | Injection Braking Time | 0.0 to 100.0 s | 1.0 s | RW | Num |  |  |  | US
06.008 | Hold Zero Frequency | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.009 | Catch A Spinning Motor | Dis (0), Enable (1), Fr.Only (2), Rv.Only (3) | Dis (0) | RW | Txt |  |  |  | US
06.010 | Enable Conditions | 000000000000 to 111111110111 |  | RO | Bin | ND | NC | PT |
06.011 | Sequencer State Machine Inputs | 0000000 to 1111111 |  | RO | Bin | ND | NC | PT |
06.012 | Enable Stop Key | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.014 | Disable Auto Reset On Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.015 | Drive Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
06.016 | Date | 00-00-00 to 31-12-99 |  | RW | Date | ND | NC | PT |
06.017 | Time | 00:00:00 to 23:59:59 |  | RW | Time | ND | NC | PT |
06.018 | Day Of Week | Sun (0), Non (1), Tue (2), Ued (3), Thu (4), Fri (5), Sat (6) |  | RO | Txt | ND | NC | PT |
06.019 | Date/Time Selector | Set (0), Po.up (1), Run (2), Acc.Po (3) | Po.up (1) | RW | Txt |  |  |  | US
06.020 | Date Format | Std (0), US (1) | Std (0) | RW | Txt |  |  |  | US
06.021 | Time Between Filter Changes | 0 to 30000 Hours | 0 Hours | RW | Num |  |  |  | US
06.022 | Filter Change Required / Change Done | Off (0) or On (1) |  | RW | Bit | ND | NC |  |
06.023 | Time Before Filter Change Due | 0 to 30000 Hours |  | RO | Num | ND | NC | PT | PS
06.024 | Reset Energy Meter | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
06.025 | Energy Meter: MWh | ±999.9 MWh |  | RO | Num | ND | NC | PT | PS
06.026 | Energy Meter: kWh | ±99.99 kWh |  | RO | Num | ND | NC | PT | PS
06.027 | Energy Cost Per kWh | 0.0 to 600.0 | 0.0 | RW | Num |  |  |  | US
06.028 | Running Cost | ±32000 |  | RO | Num | ND | NC | PT |
06.029 | Hardware Enable | Off (0) or On (1) | On (1) | RO | Bit |  | NC |  |
06.030 | Run Forward | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.031 | Jog Forward | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.032 | Run Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.033 | Forward/Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.034 | Run | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.035 | Forward Limit Switch | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.036 | Reverse Limit Switch | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.037 | Jog Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.038 | User Enable | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.039 | Not Stop | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.040 | Enable Sequencer Latching | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.041 | Drive Event Flags | 00 to 11 | 00 | RW | Bin |  | NC |  |
06.045 | Cooling Fan control | 0 to 5 | 2 | RW | Num |  |  |  | US
06.046 | Supply Loss Hold Disable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.047 | Input Phase Loss Detection Mode | Full (0), RIPPLE (1), Dis (2) | Full (0) | RW | Txt |  |  |  | US
06.048 | Supply Loss Detection Level | 0 to VM_SUPPLY_LOSS_LEVEL V | 110V drive: 205 V 200V drive: 205 V 400V drive: 410 V 575V drive: 540 V 690V drive: 540 V | RW | Num |  | RA |  | US
06.051 | Hold Supply Loss Active | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.052 | Motor Pre‑heat Current Magnitude | 0 to 100 % | 0 % | RW | Num |  |  |  | US
06.058 | Output Phase Loss Detection Time | 0.5 (0), 1.0 (1), 2.0 (2), 4.0 (3) | 0.5 (0) | RW | Txt |  |  |  | US
06.059 | Output Phase Loss Detection Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.060 | Standby Mode Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.061 | Standby Mode Mask | 00 to 11 | 00 | RW | Bin |  |  |  | US
06.071 | Slow Rectifier Charge Rate Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.073 | Braking IGBT Lower Threshold | ±VM_DC_VOLTAGE_SET V | 110V drive: 390 V 200V drive: 390 V 400V drive: 780 V 575V drive: 930 V 690V drive: 1120 V | RW | Num |  | RA |  | US
06.074 | Braking IGBT Upper Threshold | ±VM_DC_VOLTAGE_SET V | 110V drive: 390 V 200V drive: 390 V 400V drive: 780 V 575V drive: 930 V 690V drive: 1120 V | RW | Num |  | RA |  | US
06.075 | Low Voltage Braking IGBT Threshold | ±VM_DC_VOLTAGE_SET V | 0 V | RW | Num |  | RA |  | US
06.076 | Low Voltage Braking IGBT Threshold Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
06.077 | Low DC Link Operation | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.084 | UTC Offset | ±24.00 Hours | 0.00 Hours | RW | Num |  |  |  | US
06.089 | DC Injection Active | Off (0) or On (1) | Off (0) | RO | Bit |  | NC | PT | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |