# Menu 7 − Analog I/O

Mode: RFC‑S

Analog Outputs
The update rate for analog outputs is 250μs; although the output will only change at the update rate defined by the source parameter for the input. The following exceptions apply:

1. Speed Feedback (03.002) has an update rate of 4ms and includes a 16ms window filter. If this parameter is selected as a source for output 2 the update rate of the source changes to 250us and the only filter applied is the window filter associated with the position feedback interface (i.e. P1 Feedback Filter (03.042) for the P1 interface). It should be noted that this feature is only provided when the position feedback is from a drive interface and not from an option module.
2. If either analogue output is set up for current mode then the update rate for both analogue outputs is 4ms.

Analog Inputs
The normal sample rate for the analog inputs is 4ms, however this is increased to 250us for analogue inputs 1 and 2 under the following conditions:

1. The maximum and the minimum for the input are at their default values of 100.00% and -100.00% respectively.
2. The input is set to voltage mode.
3. One of the destinations given in the table below must be selected.
4. If the destination is Analog Reference 1 (01.036) or Analog Reference 2 (01.037) the reference system must not be in uinpolar mode, i.e. Bipolar Reference Enable (01.010) must be one.

Note that Analogue Input 1 Fast Update Active (07.026) and Analogue Input 2 Fast Update Active (07.027) indicate if fast updating is active for each input.

Parameter | Drive modes | Comment
Analog Reference 1 (01.036) | RFC-A, RFC-S | The data from Analog Reference 1 (01.036) is processed in the 250us task so that the reference to the speed controller is updated every 250us.
Analog Reference 2 (01.037) | RFC-A, RFC-S | The data from Analog Reference 2 (01.037) is processed in the 250us task so that the reference to the speed controller is updated every 250us.
Hard Speed Reference (03.022) | RFC-A, RFC-S |
Torque Reference (04.008) | RFC-A, RFC-S |
Power Input 1 (03.010) Power Input 2 (03.013) Power Input 3 (03.014) | Regen |

Parameter | 07.001 Analog Input 1
--- | ---
Short description | Displays the value of analog input 1
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 2
Coding | RO, FI, ND, NC, PT

Each analogue input has a resolution of 11 bits plus sign. The inputs can operate in different modes (defined by Analog Input 1 Mode (07.007) for analogue input 1). These modes include voltage, current and thermistor modes. The available modes depend on the hardware configuration and are given in the table below.

Internal I/O Identifier (11.068) | Analogue Input 1 | Analogue Input 2 | Analogue Input 3
0: Standard Analogue and Digital I/O | Bipolar Voltage, Current | Bipolar Voltage, Current | Bipolar Voltage, Thermistor, Disabled
1: Digital I/O | Not present | Not present | Thermistor, Disabled
2: HVAC Analogue and Digital I/O | UnipolarVoltage, Current, Thermistor | Unipolar Voltage, Current, Thermistor | Not present

The "Input Level" is defined for the different modes in the table below.

Mode | Input Level
Voltage | (Input Voltage / 10V) x 100.00%
0-20mA | (Input Current / 20mA) x 100.00%
20-0mA | ((20mA - Input Current) / 20mA) x 100.00%
4-20mA | ((Input Current - 4mA) / 16mA) x 100.00%
20-4mA | ((20mA - Input Current) / 16mA) x 100.00%
Thermistor | (Input resistance / 10K Ohm) x 100%

Analog Input 1 (07.001) is derived as follows:

Limits
A1 is the value after the minimum and maximum limits are applied.

If Analog Input 1 Minimum (07.040) ≥ Analog Input 1 Maximum (07.043) then:
A1 = 0.00% whatever the input level.

If Analog Input 1 Minimum (07.040) < 0.00% and Analog Input 1 Maximum (07.043) > 0.00% then:
A1 = Input Level x (100.00% / Analog Input 1 Maximum (07.043))
A1 is then limited between -100% and +100%.

Otherwise:
Input Level is limited between Analog Input 1 Minimum (07.040) and Analog Input 1 Maximum (07.043)
A1 = [Input Level - Analog Input 1 Minimum (07.040)] x 100.00% / (Analog Input 1 Maximum (07.043) - Analog Input 1 Minimum (07.040))

For thermistor modes it should be noted that Analog Input 1 Minimum (07.040) and Analog Input 1 Minimum (07.040) have no effect and that the input resistance is limited between 0 and 5K Ohms.

Parameter | 07.002 Analog Input 2
--- | ---
Short description | Displays the value of analog input 2
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 2
Coding | RO, FI, ND, NC, PT

See Analog Input 1 (07.001).

Parameter | 07.003 Analog Input 3
--- | ---
Short description | Displays the value of analog input 3
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 4ms write
Display Format | Standard | Decimal Places | 2
Coding | RO, FI, ND, NC, PT

See Analog Input 1 (07.001).

Parameter | 07.004 Monitored Temperature 1
--- | ---
Short description | Displays the temperature set up by Temperature Monitor Select 1
Mode | RFC‑S
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Thermal monitoring is provided within the drive to protect the power stage and the control system from over temperature.

Monitored Temperature 1 (07.004), Monitored Temperature 2 (07.005) and Monitored Temperature 3 (07.006) give an indication of the temperature of three selected monitoring points within the drive power system or control system. The required monitoring points can be selected using Temperature Monitor Select 1 (07.038), Temperature Monitor Select 2 (07.039) and Temperature Monitor Select 3 (07.052) respectively. The default values give two monitoring points in the power system in Monitored Temperature 1 (07.004) and Monitored Temperature 2 (07.005), and control board temperature 1 in Monitored Temperature 3 (07.006).

Parameter | 07.005 Monitored Temperature 2
--- | ---
Short description | Displays the temperature set up by Temperature Monitor Select 2
Mode | RFC‑S
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Monitored Temperature 1 (07.004) for details.

Parameter | 07.006 Monitored Temperature 3
--- | ---
Short description | Displays the temperature set up by Temperature Monitor Select 3
Mode | RFC‑S
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Monitored Temperature 1 (07.004) for details.

Parameter | 07.007 Analog Input 1 Mode
--- | ---
Short description | Defines the mode of analog input 1
Mode | RFC‑S
Minimum | -4 | Maximum | 6
Default | 6 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text | Description
‑4 | 4-20mA Low | 4-20mA low value on current loss
‑3 | 20-4mA Low | 20-4mA low value on current loss
‑2 | 4-20mA Hold | 4-20mA hold at level before loss on current loss
‑1 | 20-4mA Hold | 20-4mA hold at level before loss on current loss
0 | 0-20mA | 0-20mA
1 | 20-0mA | 20-0mA
2 | 4-20mA Trip | 4-20mA trip on current loss
3 | 20-4mA Trip | 20-4mA trip on current loss
4 | 4-20mA | 4-20mA no action on loss
5 | 20-4mA | 20-4mA no action on loss
6 | Volt | Voltage
7 | Therm Short Cct | Temperature measurement input with short circuit detection
8 | Thermistor | Temperature measurement without short circuit detection
9 | Therm No Trip | Temperature measurement input with no trips

The table below gives all the possible input modes for analog inputs 1 and 2.

Mode | Function
4-20mA Low | 4-20mA low value on current loss (1)
20-4mA Low | 20-4mA low value on current loss (1)
4-20mA Hold | 4-20mA hold at level before loss on current loss (2)
20-4mA Hold | 20-4mA hold at level before loss on current loss (2)
0-20mA | 0-20mA
20-0mA | 20-0mA
4-20mA Trip | 4-20mA trip on current loss (1), (3)
20-4mA Trip | 20-4mA trip on current loss (1), (3)
4-20mA | 4-20mA no action on loss (1)
20-4mA | 20-4mA no action on loss (1)
Voltage | Voltage
Therm Short Cct | Temperature measurement input with short circuit detection
Thermistor | Temperature measurement without short circuit detection
Therm No Trip | Temperature measurement input with no trips
Disabled | Input always zero (4)

(1) Analogue input level is 0.00% if the current is below 3mA.

(2) Analogue input level remains at the value it had in the previous sample before the current fell below 3mA.

(3) A An Input 1 Loss is initiated if the current falls below 3mA.

(4) When the Digital I/O only is present this mode is used disable the current source as the input is on a shared connection with Digital Output 2.

Parameter | 07.008 Analog Input 1 Scaling
--- | ---
Short description | Defines the scaling factor of analog input 1
Mode | RFC‑S
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

Analog Input 1 (07.001) is modified by Analog Input 1 Scaling (07.008), Analog Input 1 Offset (07.030) and Analog Input 1 Invert (07.009) before it is routed to its destination as follows:

A1O = Analog Input 1 (07.001) + Analog Input 1 Offset (07.030)

A1O is the value after the offset has been applied and is limited between -100.00% and 100.00%

A1S = A1O x Analog Input 1 Scaling (07.008)

A1S is the value after the scaling and the offset have been applied and is limited between -100.00% and 100.00%

If Analog Input 1 Invert (07.009) = 0 then A1I = A1S otherwise A1I = -A1S

A1I is the value after the invert, scaling and offset have been applied and is the final value that is routed to the destination defined by Analog Input 1 Destination (07.010).

Parameter | 07.009 Analog Input 1 Invert
--- | ---
Short description | Inverts the signal for analog input 1
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Analog Input 1 Scaling (07.008).

Parameter | 07.010 Analog Input 1 Destination
--- | ---
Short description | Defines the output parameter for analog input 1
Mode | RFC‑S
Minimum | 0.000 | Maximum | 59.999
Default | 1.036 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

See Analog Input 1 Scaling (07.008).

Parameter | 07.011 Analog Input 2 Mode
--- | ---
Short description | Defines the mode for analog input 2
Mode | RFC‑S
Minimum | -4 | Maximum | 6
Default | 6 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text | Description
‑4 | 4-20mA Low | 4-20mA low value on current loss
‑3 | 20-4mA Low | 20-4mA low value on current loss
‑2 | 4-20mA Hold | 4-20mA hold at level before loss on current loss
‑1 | 20-4mA Hold | 20-4mA hold at level before loss on current loss
0 | 0-20mA | 0-20mA
1 | 20-0mA | 20-0mA
2 | 4-20mA Trip | 4-20mA trip on current loss
3 | 20-4mA Trip | 20-4mA trip on current loss
4 | 4-20mA | 4-20mA no action on loss
5 | 20-4mA | 20-4mA no action on loss
6 | Volt | Voltage
7 | Therm Short Cct | Temperature measurement input with short circuit detection
8 | Thermistor | Temperature measurement without short circuit detection
9 | Therm No Trip | Temperature measurement input with no trips

See Analog Input 1 Mode (07.007).

Parameter | 07.012 Analog Input 2 Scaling
--- | ---
Short description | Defines the scaling factor for analog input 2
Mode | RFC‑S
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

The scaling, offset and invert functions for analog input 2 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.013 Analog Input 2 Invert
--- | ---
Short description | Inverts the signal for analog input 2
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

The scaling, offset and invert functions for analog input 2 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.014 Analog Input 2 Destination
--- | ---
Short description | Defines the output parameter for analog input 2
Mode | RFC‑S
Minimum | 0.000 | Maximum | 59.999
Default | 1.037 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

The scaling, offset and invert functions for analog input 2 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.015 Analog Input 3 Mode
--- | ---
Short description | Defines the mode of analog input 3
Mode | RFC‑S
Minimum | 6 | Maximum | 9
Default | 6 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text | Description
6 | Volt | Voltage
7 | Therm Short Cct | Temperature measurement input with short circuit detection
8 | Thermistor | Temperature measurement without short circuit detection
9 | Therm No Trip | Temperature measurement input with no trips
10 | Disabled | Input always zero

The table below gives all the possible input modes for analog input 3.

Mode | Function
Voltage | Voltage
Therm Short Cct | Temperature measurement input with short circuit detection
Thermistor | Temperature measurement without short circuit detection
Therm No Trip | Temperature measurement input with no trips
Disabled | Input always zero (1)

(1) When the Digital I/O only is present this mode is used disable the current source as the input is on a shared connection with Digital Output 2.

Parameter | 07.016 Analog Input 3 Scaling
--- | ---
Short description | Defines the scaling factor for analog input 3
Mode | RFC‑S
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

The scaling, offset and invert functions for analog input 3 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.017 Analog Input 3 Invert
--- | ---
Short description | Inverts the signal of analog input 3
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

The scaling, offset and invert functions for analog input 3 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.018 Analog Input 3 Destination
--- | ---
Short description | Defines the ouptut paramter for analog input 3
Mode | RFC‑S
Minimum | 0.000 | Maximum | 59.999
Default | 0.000 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, DE, PT, BU

The scaling, offset and invert functions for analog input 3 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.019 Analog Output 1 Source
--- | ---
Short description | Defines the input parameter for analog output 1
Mode | RFC‑S
Minimum | 0.000 | Maximum | 59.999
Default | 3.002 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT, BU

Analog Output 1 Source (07.019) defines the source parameter for analog output 1. The value of the source parameter is scaled with Analog Output 1 Scaling (07.020) and if the scaling is greater than 1.000 the value is clamped between -100% and +100% or between 0% and 100% depending on whether the output is biploar or uniploar. The resulting value is then used to control the output. It should be noted that the normal rules for parameter routing do not apply, but the scaling always makes -100% to +100% correspond to the range from minus source parameter maximum to plus source parameter maximum, and 0% corresponds to the source parameter value of zero. This means for example that a parameter with a minimum of 1 and a maximum of 10 will produce an output that changes from 10% to 100% as the parameter is change from minimum to maximum.

The outputs provided with different hardware are given in the table below.

Internal I/O Identifier (11.068) | Analogue Output 1 | Analogue Output 2
0: Standard Analogue and Digital I/O | Bipolar Voltage | Bipolar Voltage
1: Basic I/O | No output | No output
2: HVAC Analogue and Digital I/O | Unipolar Voltage or Current | Unipolar Voltage or Current

The output mode is defined by Analogue Output 1 Mode (07.021) as shown in the table below.

Analogue Output 1 Mode (07.021) | Standard Analogue and Digital I/O | HVAC Analogue and Digital I/O
Volt | -10V to + 10V | 0V to +10V
0-20mA | Not possible | 0mA to 20mA
20-0mA | Not possible | 20mA to 0mA
4-20mA | Not possible | 4mA to 20mA
20-4mA | Not possible | 20mA to 4mA

Parameter | 07.020 Analog Output 1 Scaling
--- | ---
Short description | Defines the scaling factor for analog output 1
Mode | RFC‑S
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See Analog Output 1 Source (07.019).

Parameter | 07.022 Analog Output 2 Source
--- | ---
Short description | Defines the input source for analog output 2
Mode | RFC‑S
Minimum | 0.000 | Maximum | 59.999
Default | 4.002 | Units |
Type | 16 Bit User Save | Update Rate | Drive reset read
Display Format | Standard | Decimal Places | 3
Coding | RW, PT, BU

Analog Output 2 Source (07.022) defines the source parameter for analog output 1. The value of the source parameter is scaled with Analog Output 2 Scaling (07.023) and if the scaling is greater than 1.000 the value is clamped between -100% and +100% or between 0% and 100% depending on whether the output is biploar or uniploar. The resulting value is then used to control the output. The outputs provided with different hardware are given in the table below.

Internal I/O Identifier (11.068) | Analogue Output 1 | Analogue Output 2
0: Standard Analogue and Digital I/O | Bipolar Voltage | Bipolar Voltage
1: Basic I/O | No output | No output
2: HVAC Analogue and Digital I/O | Unipolar Voltage or Current | Unipolar Voltage or Current

The output mode is defined by Analogue Output 2 Mode (07.024) as shown in the table below.

Analogue Output 2 Mode (07.024) | Standard Analogue and Digital I/O | HVAC Analogue and Digital I/O
Volt | -10V to + 10V | 0V to +10V
0-20mA | Not possible | 0mA to 20mA
20-0mA | Not possible | 20mA to 0mA
4-20mA | Not possible | 4mA to 20mA
20-4mA | Not possible | 20mA to 4mA

Parameter | 07.023 Analog Output 2 Scaling
--- | ---
Short description | Defines the scaling factor for analog output 2
Mode | RFC‑S
Minimum | 0.000 | Maximum | 10.000
Default | 1.000 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 3
Coding | RW

See Analog Output 2 Source (07.022).

Parameter | 07.025 Calibrate Analog Input 1 Full Scale
--- | ---
Short description | Caibrates the input level for analog input 1
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit Volatile | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, NC

For analog input 1, and in voltage mode only, the full scale value used to determine the input level can be changed from 10V by calibrating the input. The calibration process is triggered by setting Calibrate Analog Input 1 Full Scale (07.025) to one. Calibrate Analog Input 1 Full Scale (07.025) is cleared automatically when the calibration process is complete. After calibration the actions are as follows:

Input voltage during calibration | Result
V < 1.5V | The calibration result is ignored and the full scale is set to 10V. Analog Input 1 Full Scale (07.051) is set to zero.
1.5V < V < 2.5V | The calibration result is ignored and the full scale or Analog Input 1 Full Scale (07.051) are not affected.
V > 2.5V | The calibration result is used to set full scale and the value is also stored in Analog Input 1 Full Scale (07.051).

It should be noted that Analog Input 1 Full Scale (07.051) is a power-down save parameter, and so the result is automatically retained after power-down.

Parameter | 07.026 Analogue Input 1 Fast Update Active
--- | ---
Short description | Analogue Input 1 Fast Update Active
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Analogue Input 1 Fast Update Active (07.026) is one if the destination for analogue input 1 is being updated at the fast rate of 250us.

Parameter | 07.027 Analogue Input 2 Fast Update Active
--- | ---
Short description | Analogue Input 2 Fast Update Active
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Analogue Input 2 Fast Update Active (07.027) is one if the destination for analogue input 1 is being updated at the fast rate of 250us.

Parameter | 07.028 Analog Input 1 Current Loop Loss
--- | ---
Short description | Displays when analog input 1 falls below 3mA
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

If Analog Input 1 Mode (07.007) is set to any of the 4-20mA or 20-4mA modes and the current falls below 3mA then Analog Input 1 Current Loop Loss (07.028) is set to one. If the current is more than 3mA or any other mode is selected then Analog Input 1 Current Loop Loss (07.028) is set to zero.

Parameter | 07.029 Analog Input 2 Current Loop Loss
--- | ---
Short description | Displays when analog input 2 falls below 3mA
Mode | RFC‑S
Minimum | 0 | Maximum | 1
Default |  | Units |
Type | 1 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

See Analog Input 1 Current Loop Loss (07.028).

Parameter | 07.030 Analog Input 1 Offset
--- | ---
Short description | Defines the offset of analog input 1
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 Scaling (07.008).

Parameter | 07.031 Analog Input 2 Offset
--- | ---
Short description | Defines the offset of analog input 2
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

The scaling, offset and invert functions for analog input 2 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.032 Analog Input 3 Offset
--- | ---
Short description | Defines the offset of analog input 3
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 0.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

The scaling, offset and invert functions for analog input 3 are defined in the same way as for analog input 1. See Analog Input 1 Scaling (07.008).

Parameter | 07.033 Power Output
--- | ---
Short description | Instant output power
Mode | RFC‑S
Minimum | -100.0 | Maximum | 100.0
Default |  | Units | %
Type | 16 Bit Volatile | Update Rate | 250µs write
Display Format | Standard | Decimal Places | 1
Coding | RO, ND, NC, PT

This is an instantaneous power output with fast update rate that is primarily intended to be used as a power feed-forward for applications with a Regen system front end. The full scale (100.0%) value is equal to a power of 3 x (VM_DC_VOLTAGE[MAX] / 2√2) x Full Scale Current Kc (11.061). This is compatible with the power output provided in Unidrive SP and is directly comptible with Power Input 1 (03.010) (and the other power feed-forward parameters) in Regen mode. The scaling is intended to cover the maximum range of likely power in the drive. For example with a 400V 7.5kW drive the full scale d.c. link voltage is 831V and Kc=38.222A, and so the full scale value of this parameter is 3 x (831 / 2√2) x 38.222 = 33.689kW. For Open-loop, RFC-A and RFC-S modes a positive value of power indicates power flowing from the drive to motor. For Regen mode a positive value of power indicates power flowing from the supply to the regen drive.

Parameter | 07.034 Inverter Temperature
--- | ---
Short description | Displays the estimated junction temperature of the hottest power device within the drive inverter
Mode | RFC‑S
Minimum | -250 | Maximum | 250
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Inverter Temperature (07.034) shows the estimated junction temperature of the hottest power device within the drive inverter. If this temperature exceeds the switch down threshold defined for the power stage the switching frequency is reduced provided this feature has not been disabled (see Auto-switching Frequency Change (05.035)).

Parameter | 07.035 Percentage Of d.c. Link Thermal Trip Level
--- | ---
Short description | Displays the percentage of the maximum allowed temperature as estimated by the thermal model of the d.c. link components
Mode | RFC‑S
Minimum | 0 | Maximum | 100
Default |  | Units | %
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Percentage Of d.c. Link Thermal Trip Level (07.035) gives the percentage of the maximum allowed temperature as estimated by the thermal model of the d.c. link components.

Parameter | 07.036 Percentage Of Drive Thermal Trip Level
--- | ---
Short description | Displays the percentage of the thermal trip level of the temperature monitoring point or thermal model in the drive that is highest
Mode | RFC‑S
Minimum | 0 | Maximum | 100
Default |  | Units | %
Type | 8 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Percentage Of Drive Thermal Trip Level (07.036) gives the percentage of the thermal trip level of the temperature monitoring point or thermal model in the drive that is highest. This includes all thermal monitoring points (not just those selected by Monitored Temperature 1 (07.004), Monitored Temperature 2 (07.005) and Monitored Temperature 3 (07.006)), Inverter Temperature (07.034) and Percentage Of d.c. Link Thermal Trip Level (07.035).

Percentage Of d.c. Link Thermal Trip Level (07.035) is used directly to give Percentage Of Drive Thermal Trip Level (07.036), but for all other monitored values which are temperatures this is given by Percentage of thermal trip level = (Temperature - 40oC) / (Trip temperature - 40oC) x 100%

The location of the measurement or the thermal model that is related to this temperature is given in Temperature Nearest To Trip Level (07.037). If Percentage Of Drive Thermal Trip Level (07.036) exceeds 90% Drive Over-temperature Alarm (10.018) is set to one. If Percentage Of Drive Thermal Trip Level (07.036) reaches 100% one of the trips given in the table below is initiated. The trip can be reset when the percentage of thermal trip level fall below 95%.

Temperature | Trip
Inverter Temperature (07.034) | OHt Inverter
Power system temperature | OHt Power
Percentage Of d.c. Link Thermal Trip Level (07.035) | OHt dc Link
Control system temperature | OHt Control

Parameter | 07.037 Temperature Nearest To Trip Level
--- | ---
Short description | Displays the thermistor location or the model that corresponds to the value shown in Percentage Of Drive Thermal Trip Level
Mode | RFC‑S
Minimum | 0 | Maximum | 20999
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Temperature Nearest To Trip Level (07.037) shows the thermistor location or the model that corresponds to the value shown in Percentage Of Drive Thermal Trip Level (07.036) in the form xxyzz as shown in the table below.

Source | xx | y | zz
Control system | 00 | 0 | 01: Control board thermistor 1
Control system | 00 | 0 | 02: Control board thermistor 2
Control system | 00 | 0 | 03: I/O board thermistor
Control system | 00 | 1 | 00: Inverter thermal model
Control system | 00 | 2 | 00: D.c. link thermal model
Control system | 00 | 3 | 00: Braking IGBT thermal model
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power system
Power system | 01 | Rectifier number | zz: Thermistor location defined by zz in the rectifier

Parameter | 07.038 Temperature Monitor Select 1
--- | ---
Short description | Defines the temperature to be monitored in Monitored Temperature 1
Mode | RFC‑S
Minimum | 0 | Maximum | 1999
Default | 1001 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

Temperature Monitor Select 1 (07.038) selects the temperature to be monitored in Monitored Temperature 1 (07.004) using the format given for Temperature Nearest To Trip Level (07.037). If the monitoring point selected does not exist then the monitored temperature is always zero. The table below shows the monitoring points that can be selected.

Source | xx | y | zz
Control system | 00 | 0 | 01: Control board thermistor 1
Control system | 00 | 0 | 02: Control board thermistor 2
Control system | 00 | 0 | 03: I/O board thermistor
Control system | 00 | 1 | 00: Inverter thermal model
Control system | 00 | 3 | 00: Braking IGBT thermal model
Power system | 01 | 0 | zz: Thermistor location defined by zz in the power system
Power system | 01 | Rectifier number | zz: Thermistor location defined by zz in the rectifier

For a multi-module power system the power system measurement that can be selected is shown in the table below. It should be noted that the specific power module cannot be selected and that the highest temperature from each of the power modules is given.

Source | xx | y | zz
Power system | 01 | 0 | 01: U phase power device thermistor
Power system | 01 | 0 | 02: V phase power device thermistor
Power system | 01 | 0 | 03: W phase power device thermistor
Power system | 01 | 0 | 04: General rectifier thermistors
Power system | 01 | 0 | 05: General power system thermistor

Parameter | 07.039 Temperature Monitor Select 2
--- | ---
Short description | Defines the temperature to be monitored in Monitored Temperature 2
Mode | RFC‑S
Minimum | 0 | Maximum | 1999
Default | 1002 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Temperature Monitor Select 1 (07.038).

Parameter | 07.040 Analog Input 1 Minimum
--- | ---
Short description | Defines the minimum value for analog input 1
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | -100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.041 Analog Input 2 Minimum
--- | ---
Short description | Defines the minimum value for analog input 2
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | -100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.042 Analog Input 3 Minimum
--- | ---
Short description | Defines the minimum value for analog input 3
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | -100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.043 Analog Input 1 Maximum
--- | ---
Short description | Defines the maximum value for analog input 1
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.044 Analog Input 2 Maximum
--- | ---
Short description | Defines the maximum value for analog input 2
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.045 Analog Input 3 Maximum
--- | ---
Short description | Defines the maximum value for analog input 3
Mode | RFC‑S
Minimum | -100.00 | Maximum | 100.00
Default | 100.00 | Units | %
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 2
Coding | RW

See Analog Input 1 (07.001).

Parameter | 07.046 Analog Input 3 Thermistor Type
--- | ---
Short description | Defines the thermistor type for analog input 3
Mode | RFC‑S
Minimum | 0 | Maximum | 9
Default | 0 | Units |
Type | 8 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW, TE

Value | Text
0 | DIN44082
1 | KTY84
2 | PT100 (4W)
3 | PT1000 (4W)
4 | PT2000 (4W)
5 | 2.0mA (4W)
6 | PT100 (2W)
7 | PT1000 (2W)
8 | PT2000 (2W)
9 | 2.0mA (2W)

Analog Input 3 Thermistor Type (07.046) defines the operation of the temperature feedback interface for analog input 3 when Analog Input 3 Mode (07.015) is set up for a temperature feedback mode. When a temperature feedback mode is selected a 2mA current source is connected to analog input 3 to supply the temperature feedback device that is connected to the input.

Analog Input 3 Thermistor Type (07.046) | Compatible devices
0: DIN44082 | Three thermistors in series as specified in DIN44082 standard
1: KTY84 | KTY84 PTC thermistor
2: PT100 (4W) | PT100 PTC thermistor with 4 wire connection
3: PT1000 (4W) | PT1000 PTC thermistor with 4 wire connection
4:PT2000 (4W) | PT2000 PTC thermistor with 4 wire connection
5: 2.0mA (4W) | Any device. Full scale equivalent to a resistance of 5k Ohms with 4 wire connection
6: PT100 (2W) | PT100 PTC thermistor with 2 wire connection
7: PT1000 (2W) | PT1000 PTC thermistor with 2 wire connection
8: PT2000 (2W) | PT2000 PTC thermistor with 2 wire connection
9: 2.0mA (2W) | Any device. Full scale equivalent to a resistance of 5k Ohms with 2 wire connection

DIN44082 and KTY84 devices should always be connected directly to analog input 3. The other devices can be connected directly to analog input 3 if the 2 wire connection option is selected. Alternatively these devices can be used with a 4 wire connection to remove the effect of voltage drops due to the 2mA supply current as shown below. If a 4 wire connection is selected analog input 1 is disabled and Analog Input 1 (07.001) always reads as 0.0%.

Parameter | 07.047 Analog Input 3 Thermistor Feedback
--- | ---
Short description | Displays the measured resistance of analog input 3
Mode | RFC‑S
Minimum | 0 | Maximum | 5000
Default |  | Units | Ω
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

Analog Input 3 Thermistor Feedback (07.047) shows the measured resistance.

Parameter | 07.048 Analog Input 3 Thermistor Trip Threshold
--- | ---
Short description | Defines the thermistor trip threshold for analog input 3
Mode | RFC‑S
Minimum | 0 | Maximum | 5000
Default | 3300 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

Over-temperature detection becomes active for input 3 if Analog Input 3 Thermistor Feedback (07.047) > Analog Input 3 Thermistor Trip Threshold (07.048). Over-temperature becomes inactive for input 3 if Analog Input 3 Thermistor Feedback (07.047) < Analog Input 3 Thermistor Reset Threshold (07.049). If Analog Input 3 Mode (07.015) is 7 or 8 (i.e. tripping is enabled) an Thermistor.003 trip is initiated. The default values for Analog Input 3 Thermistor Trip Threshold (07.048) and Analog Input 3 Thermistor Reset Threshold (07.049) are the levels specified in the DIN 44082 standard.

Parameter | 07.049 Analog Input 3 Thermistor Reset Threshold
--- | ---
Short description | Defines the thermistor reset threshold for analog input 3
Mode | RFC‑S
Minimum | 0 | Maximum | 5000
Default | 1800 | Units | Ω
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Analog Input 3 Thermistor Trip Threshold (07.048).

Parameter | 07.050 Analog Input 3 Thermistor Temperature
--- | ---
Short description | Displays the temperature of the device based on the resistance to temperature characteristic for the specified device
Mode | RFC‑S
Minimum | -50 | Maximum | 300
Default |  | Units | °C
Type | 16 Bit Volatile | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT

If a KTY84, PT100, PT1000 or PT2000 type device is selected for temperature feedback then Analog Input 3 Thermistor Temperature (07.050) shows the temperature of the device based on the resistance to temperature characteristic specified for this device. Otherwise Analog Input 3 Thermistor Temperature (07.050) = 0.0.

Parameter | 07.051 Analog Input 1 Full Scale
--- | ---
Short description | Displays the full scale value of analog input 1
Mode | RFC‑S
Minimum | 0 | Maximum | 65535
Default |  | Units |
Type | 16 Bit Power Down Save | Update Rate | Background write
Display Format | Standard | Decimal Places | 0
Coding | RO, ND, NC, PT, BU

See Calibrate Analog Input 1 Full Scale (07.025).

Parameter | 07.052 Temperature Monitor Select 3
--- | ---
Short description | Defines the temperature to be monitored in Monitored Temperature 3
Mode | RFC‑S
Minimum | 0 | Maximum | 1999
Default | 1 | Units |
Type | 16 Bit User Save | Update Rate | Background read
Display Format | Standard | Decimal Places | 0
Coding | RW

See Temperature Monitor Select 1 (07.038).