# Menu 11 Single Line Descriptions − Miscellaneous

Mode: Regeneration

Parameter | Range | Default | Type
--- | --- | --- | ---
11.001 | Option Synchronisation Select | Not Active (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4), Automatic (5) | Slot 4 (4) | RW | Txt |  |  |  | US
11.002 | Option synchronisation Active | Not Active (0), Slot 1 (1), Slot 2 (2), Slot 3 (3), Slot 4 (4) |  | RO | Txt | ND | NC | PT |
11.018 | Status Mode Parameter 1 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
11.019 | Status Mode Parameter 2 | 0.000 to 59.999 | 0.000 | RW | Num |  |  | PT | US
11.020 | Reset Serial Communications | Off (0) or On (1) |  | RW | Bit | ND | NC |  |
11.021 | Parameter 00.030 Scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
11.022 | Parameter Displayed At Power‑up | 0.000 to 0.080 | 0.011 | RW | Num |  |  | PT | US
11.023 | Serial Address | 1 to 247 | 1 | RW | Num |  |  |  | US
11.024 | Serial Mode | 8 2 NP (0), 8 1 NP (1), 8 1 EP (2), 8 1 OP (3), 8 2 NP M (4), 8 1 NP M (5), 8 1 EP M (6), 8 1 OP M (7), 7 2 NP (8), 7 1 NP (9), 7 1 EP (10), 7 1 OP (11), 7 2 NP M (12), 7 1 NP M (13), 7 1 EP M (14), 7 1 OP M (15) | 8 2 NP (0) | RW | Txt |  |  |  | US
11.025 | Serial Baud Rate | 300 (0), 600 (1), 1200 (2), 2400 (3), 4800 (4), 9600 (5), 19200 (6), 38400 (7), 57600 (8), 76800 (9), 115200 (10) | 19200 (6) | RW | Txt |  |  |  | US
11.026 | Minimum Comms Transmit Delay | 0 to 250 ms | 2 ms | RW | Num |  |  |  | US
11.027 | Silent Period | 0 to 250 ms | 0 ms | RW | Num |  |  |  | US
11.028 | Drive Derivative | 0 to 255 |  | RO | Num | ND | NC | PT |
11.029 | Software Version | 0 to 99999999 |  | RO | Num | ND | NC | PT |
11.030 | User Security Code | 0 to 2147483647 |  | RW | Num | ND | NC | PT | US
11.031 | User Drive Mode | Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4) |  | RW | Txt | ND | NC | PT |
11.032 | Maximum Heavy Duty Rating | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.033 | Drive Rated Voltage | 200V (0), 400V (1), 575V (2), 690V (3) |  | RO | Txt | ND | NC | PT |
11.034 | Software Sub‑version | 0 to 99 |  | RO | Num | ND | NC | PT |
11.035 | Number Of Power Modules Test | -1 to 20 | -1 | RW | Num |  |  |  | US
11.036 | NV Media Card File Previously Loaded | 0 to 999 | 0 | RO | Num |  | NC | PT |
11.037 | NV Media Card File Number | 0 to 999 | 0 | RW | Num |  |  |  |
11.038 | NV Media Card File Type | None (0), Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4), User Prog (5), Option App (6) |  | RO | Txt | ND | NC | PT |
11.039 | NV Media Card File Version | 0 to 9999 |  | RO | Num | ND | NC | PT |
11.040 | NV Media Card File Checksum | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.042 | Parameter Cloning | None (0), Read (1), Program (2), Auto (3), Boot (4) | None (0) | RW | Txt |  | NC |  | US
11.043 | Load Defaults | None (0), Standard (1), US (2) | None (0) | RW | Txt |  | NC |  |
11.044 | User Security Status | Menu 0 (0), All Menus (1), Read‑only Menu 0 (2), Read‑only (3), Status Only (4), No Access (5) |  | RW | Txt | ND |  | PT |
11.045 | Select Motor 2 Parameters | Motor 1 (0), Motor 2 (1) | Motor 1 (0) | RW | Txt |  |  |  | US
11.046 | Defaults Previously Loaded | 0 to 2000 |  | RO | Num | ND | NC | PT | US
11.047 | Onboard User Program: Enable | Stop (0), Run (1) | Run (1) | RW | Txt |  |  |  | US
11.048 | Onboard User Program: Status | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.049 | Onboard User Program: Programming Events | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.050 | Onboard User Program: FreewheelingTasks Per Second | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.051 | Onboard User Program: Clock Task Time Used | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
11.052 | Serial Number LS | 000000000 to 999999999 |  | RO | Num | ND | NC | PT |
11.053 | Serial Number MS | 0 to 999999999 |  | RO | Num | ND | NC | PT |
11.054 | Drive Date Code | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.055 | Onboard User Program: Clock Task Scheduled Interval | 0 to 262140 ms |  | RO | Num | ND | NC | PT |
11.056 | Option Slot Identifiers | 1234 (0), 1243 (1), 1324 (2), 1342 (3), 1423 (4), 1432 (5), 4123 (6), 3124 (7), 4132 (8), 2134 (9), 3142 (10), 2143 (11), 3412 (12), 4312 (13), 2413 (14), 4213 (15), 2314 (16), 3214 (17), 2341 (18), 2431 (19), 3241 (20), 3421 (21), 4231 (22), 4321 (23) | 1234 (0) | RW | Txt |  |  | PT |
11.060 | Maximum Rated Current | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.061 | Full Scale Current Kc | 0.000 to 99999.999 A |  | RO | Num | ND | NC | PT |
11.062 | Power Board Software Version Number | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
11.063 | Product Type | 0 to 255 |  | RO | Num | ND | NC | PT |
11.064 | Product Identifier Characters | 1295396912 to 2147483647 |  | RO | Num | ND | NC | PT |
11.065 | Drive Rating And Configuration | 00000000 to 99999999 |  | RO | Num | ND | NC | PT |
11.066 | Power Stage Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.067 | Control Board Identifier | 0.000 to 65.535 |  | RO | Num | ND | NC | PT |
11.068 | Internal I/O Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.069 | Position Feedback Interface Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.070 | Core Parameter Database Version | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
11.071 | Number Of Power Modules Detected | 0 to 20 |  | RO | Num | ND | NC | PT | US
11.072 | NV Media Card Create Special File | 0 to 1 | 0 | RW | Num |  | NC |  |
11.073 | NV Media Card Type | None (0), SMART Card (1), SD Card (2) |  | RO | Txt | ND | NC | PT |
11.075 | NV Media Card Read‑only Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.076 | NV Media Card Warning Suppression Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.077 | NV Media Card File Required Version | 0 to 9999 |  | RW | Num | ND | NC | PT |
11.079 | Drive Name Characters 1‑4 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.080 | Drive Name Characters 5‑8 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.081 | Drive Name Characters 9‑12 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.082 | Drive Name Characters 13‑16 | -2147483648 to 2147483647 | 0 | RW | Num |  |  | PT | US
11.084 | Drive Mode | Open‑loop (1), RFC‑A (2), RFC‑S (3), Regen (4) |  | RO | Txt | ND | NC | PT | US
11.085 | Security Status | None (0), Read‑only (1), Status‑only (2), No Access (3) |  | RO | Txt | ND | NC | PT | PS
11.086 | Menu Access Status | Menu 0 (0), All Menus (1) |  | RO | Txt | ND | NC | PT | PS
11.090 | Keypad Port Serial Address | 1 to 16 | 1 | RW | Num |  |  |  | US
11.091 | Additional Identifier Characters 1 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.092 | Additional Identifier Characters 2 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.093 | Additional Identifier Characters 3 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.095 | Number Of Rectifiers Detected | 0 to 9 |  | RO | Num | ND | NC | PT |
11.096 | Number Of Rectifiers Expected | 0 to 9 | 0 | RW | Num |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |