# Menu 6 Single Line Descriptions − Sequencer and Clock

Mode: RFC‑A

Parameter | Range | Default | Type
--- | --- | --- | ---
06.001 | Stop Mode | Coast (0), Ramp (1), No Ramp (2) | Ramp (1) | RW | Txt |  |  |  | US
06.002 | Limit Switch Stop Mode | Stop (0), Ramp (1) | Stop (0) | RW | Txt |  |  |  | US
06.003 | Supply Loss Mode | Disable (0), Ramp Stop (1), Ride Thru (2), Limit Stop (3) | Disable (0) | RW | Txt |  |  |  | US
06.008 | Hold Zero Speed | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.009 | Catch A Spinning Motor | Disable (0), Enable (1), Fwd Only (2), Rev Only (3) | Disable (0) | RW | Txt |  |  |  | US
06.010 | Enable Conditions | 000000000000 to 111111111111 |  | RO | Bin | ND | NC | PT |
06.011 | Sequencer State Machine Inputs | 000000 to 111111 |  | RO | Bin | ND | NC | PT |
06.012 | Enable Stop Key | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.013 | Enable Auxiliary Key | Disabled (0), Forward/Reverse (1), Run Reverse (2) | Disabled (0) | RW | Txt |  |  |  | US
06.015 | Drive Enable | Off (0) or On (1) | On (1) | RW | Bit |  |  |  | US
06.016 | Date | 00-00-00 to 31-12-99 |  | RW | Date | ND | NC | PT |
06.017 | Time | 00:00:00 to 23:59:59 |  | RW | Time | ND | NC | PT |
06.018 | Day Of Week | Sunday (0), Monday (1), Tuesday (2), Wednesday (3), Thursday (4), Friday (5), Saturday (6) |  | RO | Txt | ND | NC | PT |
06.019 | Date/Time Selector | Set (0), Powered (1), Running (2), Acc Powered (3), Local Keypad (4), Remote Keypad (5), Slot 1 (6), Slot 2 (7), Slot 3 (8), Slot 4 (9) | Powered (1) | RW | Txt |  |  |  | US
06.020 | Date Format | Std (0), US (1) | Std (0) | RW | Txt |  |  |  | US
06.021 | Time Between Filter Changes | 0 to 30000 Hours | 0 Hours | RW | Num |  |  |  | US
06.022 | Filter Change Required / Change Done | Off (0) or On (1) |  | RW | Bit | ND | NC |  |
06.023 | Time Before Filter Change Due | 0 to 30000 Hours |  | RO | Num | ND | NC | PT | PS
06.024 | Reset Energy Meter | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
06.025 | Energy Meter: MWh | ±999.9 MWh |  | RO | Num | ND | NC | PT | PS
06.026 | Energy Meter: kWh | ±99.99 kWh |  | RO | Num | ND | NC | PT | PS
06.027 | Energy Cost Per kWh | 0.0 to 600.0 | 0.0 | RW | Num |  |  |  | US
06.028 | Running Cost | ±32000 |  | RO | Num | ND | NC | PT |
06.029 | Hardware Enable | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
06.030 | Run Forward | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.031 | Jog | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.032 | Run Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.033 | Forward/Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.034 | Run | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.035 | Forward Limit Switch | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.036 | Reverse Limit Switch | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.037 | Jog Reverse | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.039 | Not Stop | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.040 | Enable Sequencer Latching | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.041 | Drive Event Flags | 00 to 11 | 00 | RW | Bin |  | NC |  |
06.042 | Control Word | 000000000000000 to 111111111111111 | 000000000000000 | RW | Bin |  | NC |  |
06.043 | Control Word Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.044 | Active Supply | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
06.045 | Cooling Fan control | 0 to 11 | 10 | RW | Num |  |  |  | US
06.047 | Input Phase Loss Detection Mode | Full (0), Ripple Only (1), Disabled (2) | Full (0) | RW | Txt |  |  |  | US
06.048 | Supply Loss Detection Level | ±VM_SUPPLY_LOSS_LEVEL V | 200V drive: 205 V 400V drive: 410 V 575V drive: 540 V 690V drive: 540 V | RW | Num |  | RA |  | US
06.051 | Hold Supply Loss Active | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
06.052 | Motor Pre‑heat Current Magnitude | 0 to 100 % | 0 % | RW | Num |  |  |  | US
06.058 | Output Phase Loss Detection Time | 0.5s (0), 1.0s (1), 2.0s (2), 4.0s (3) | 0.5s (0) | RW | Txt |  |  |  | US
06.059 | Output Phase Loss Detection Enable | Disabled (0), Enabled (1) | Disabled (0) | RW | Txt |  |  |  | US
06.060 | Standby Mode Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.061 | Standby Mode Mask | 0000000 to 1111111 | 0000000 | RW | Bin |  |  |  | US
06.065 | Standard Under Voltage Threshold | ±VM_STD_UNDER_VOLTS V | 200V drive: 175 V 400V drive: 330 V 575V drive: 435 V 690V drive: 435 V | RW | Num |  | RA |  | US
06.066 | Low Under Voltage Threshold | ±VM_LOW_UNDER_VOLTS V | 200V drive: 175 V 400V drive: 330 V 575V drive: 435 V 690V drive: 435 V | RW | Num |  | RA |  | US
06.067 | Low Under Voltage Threshold Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.068 | Backup Supply Mode Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.069 | Under‑voltage System Contactor Close | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
06.070 | Under‑voltage System Contactor Closed | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
06.071 | Slow Rectifier Charge Rate Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.072 | User Supply Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
06.073 | Braking IGBT Lower Threshold | ±VM_DC_VOLTAGE_SET V | 200V drive: 390 V 400V drive: 780 V 575V drive: 930 V 690V drive: 1120 V | RW | Num |  | RA |  | US
06.074 | Braking IGBT Upper Threshold | ±VM_DC_VOLTAGE_SET V | 200V drive: 390 V 400V drive: 780 V 575V drive: 930 V 690V drive: 1120 V | RW | Num |  | RA |  | US
06.075 | Low Voltage Braking IGBT Threshold | ±VM_DC_VOLTAGE_SET V | 0 V | RW | Num |  | RA |  | US
06.076 | Low Voltage Braking IGBT Threshold Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  |
06.084 | Date And Time Offset | ±24.00 Hours | 0.00 Hours | RW | Num |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |